For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter-to-Exhaust Manifold Nuts | 50 N·m | 37 lb ft
Connecting Pipe-to-Catalytic Converter Nuts | 40 N·m | 30 lb ft
Exhaust Manifold Cover Bolts | 15 N·m | 11 lb ft
Front Exhaust Pipe Mounting Bracket Bolt | 40 N·m | 30 lb ft
Front Muffler-to-Connecting Pipe Nuts | 30 N·m | 22 lb ft
Front Muffler-to-Rear Muffler Nuts | 30 N·m | 22 lb ft
Post-Converter Heated Oxygen Sensor | 41 N·m | 30 lb ft