For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug Locknut | 70 N·m | 52 lb ft
Ball Joint Hex Nut | 45 N·m | 33 lb ft
Crossmember-to-Underbody Bolts | 150 N·m | 111 lb ft
Outer Tie Rod Hex Nuts | 45 N·m | 33 lb ft
Outer Tie Rod Lock Nuts | 54 N·m | 40 lb ft
Pinion Preload | 0.9-1.7 N·m | 8-15 lb in
Stabilizer Shaft-to-Knuckle Bolts | 45 N·m | 33 lb ft
Steering Gear Retaining Bracket Nuts | 50 N·m | 37 lb ft