For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery

- Manual

• | 1.2L SOHC

• | 1.5L SOHC

410 Cold Cranking Amps

- Automatic

• | 1.4L SOHC/DOHC

• | 1.5L SOHC

550 Cold Cranking Amps

Alternator

• | 1.4L SOHC/DOHC

• | 1.5L SOHC, A/T

85 A

Alternator

• | 1.2L SOHC

• | 1.5L SOHC, M/T

75 A

Starter-Manual (No-Load Test Current Draw)

• | 1.2L SOHC

• | 1.5L SOHC

0.8 kW

Maximum 53 A (Drive Pinion Speed at Minimum 5,000 RPM, 11.5 V

Starter-Automatic (No-Load Test Current Draw)

• | 1.4L SOHC/DOHC

• | 1.5L SOHC

1.2 kW

Maximum 90 A (Drive Pinion Speed at Minimum 2,600 RPM, 11.5 V