For 1990-2009 cars

The front and the rear door lock strikers each consist of a striker with 2 screws threaded into a floating cage plate in the B-pillars and C-pillars. The door is secured in the closed position when the door lock fork snaps over and engages the striker.

### Childproof Rear Door Lock

The childproof rear door locks help prevent passengers, especially children, from opening the rear doors of the vehicle from the inside.

To activate the door locks, move the levers of both rear doors to the lock position and close both doors. Now the rear passengers will be unable to open the doors from inside of the vehicle.

To deactivate the door locks, unlock the doors from the inside of the vehicle and open the doors from the outside. Move the lever to the unlock position. The rear doors will now work normally.