For 1990-2009 cars

Connector 1: | A/C Compressor Clutch (LMU)
Connector 2: | A/C Compressor Clutch (without LMU)
Connector 3: | A/C Engine Coolant Temperature (ECT) Sensor (C68)
Connector 4: | A/C Refrigerant Pressure Sensor
Connector 5: | Accelerator Pedal Position (APP) Sensor (LDT/LXV)
Connector 6: | Air Temperature Actuator (C68)
Connector 7: | Air Temperature Sensor - Inside (C68)
Connector 8: | Ambient Air Temperature Sensor (U68)
Connector 9: | Ashtray Lamp
Connector 10: | Automatic Transmission
Connector 11: | Automatic Transmission Input Shaft Speed (ISS) Sensor
Connector 12: | Automatic Transmission Shift Lever
Connector 13: | Automatic Transmission Shift Lever Position Indicator
Connector 14: | Automatic Transmission Shift Program Switch
Connector 15: | Auxiliary Power Outlet
Connector 16: | Backup Lamp (Hatchback with WHB)
Connector 17: | Backup Lamp Switch (M/T without LMU)
Connector 18: | Backup Lamp Switch (LMU with M/T)
Connector 19: | Blower Motor
Connector 20: | Blower Motor Control Module (C68)
Connector 21: | Blower Motor Resistor
Connector 22: | Blower Motor Switch (without C68)
Connector 23: | Brake Fluid Level Switch
Connector 24: | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust (LDT/LXV)
Connector 25: | Camshaft Position (CMP) Actuator Solenoid Valve - Intake (LDT/LXV)
Connector 26: | Camshaft Position (CMP) Sensor - Exhaust (LDT/LXV)
Connector 27: | Camshaft Position (CMP) Sensor - Intake (LDT/LXV)
Connector 28: | Camshaft Position (CMP) Sensor (LMU)
Connector 29: | Camshaft Position (CMP) Sensor (L95/LXT)
Connector 30: | Camshaft Position (CMP) Sensor (LV8)
Connector 31: | Cellular Telephone Microphone (UE1)
Connector 32: | Cellular Telephone Microphone (UV8)
Connector 33: | Center High Mounted Stop Lamp (CHMSL) (TS6)
Connector 34: | Center High Mounted Stop Lamp (CHMSL) (Notchback with T43)
Connector 35: | Cigar Lighter
Connector 36: | Clock
Connector 37: | Clutch Pedal Position (CPP) Switch (WHB with MLM)
Connector 38: | Cooling Fan
Connector 39: | Courtesy/Reading Lamp (without Sunroof)
Connector 40: | Crankshaft Position (CKP) Sensor (LDT/LXV)
Connector 41: | Crankshaft Position (CKP) Sensor (without LDT/LXV)
Connector 42: | Data Link Connector (DLC)
Connector 43: | Data Link Connector (DLC) 2 (JM4)
Connector 44: | Door Handle Switch - Driver (LHD with AU3)
Connector 45: | Door Handle Switch - Driver (RHD) (AU3)
Connector 46: | Door Handle Switch - Passenger (LHD with AU3)
Connector 47: | Door Handle Switch - Passenger (RHD with AU3)
Connector 48: | Door Lock Actuator - Driver (AU3)
Connector 49: | Door Lock Actuator - Left Rear (AU3)
Connector 50: | Door Lock Actuator - Liftgate (AU3)
Connector 51: | Door Lock Actuator - Passenger (AU3)
Connector 52: | Door Lock Actuator - Right Rear (AU3)
Connector 53: | Electronic Brake Control Module (EBCM) (JM4)
Connector 54: | Engine Control Module (ECM) - Sirius D42 (1.2L) (LMU)
Connector 55: | Engine Control Module (ECM) X1 (1.5L) (LV8)
Connector 56: | Engine Control Module (ECM) X2 (1.5L) (LV8)
Connector 57: | Engine Control Module (ECM) X1 (1.4L, 1.6L) (L95, LXT)
Connector 58: | Engine Control Module (ECM) X2 (1.4L, 1.6L) (L95, LXT)
Connector 59: | Engine Control Module (ECM) X1 (1.4L) (LDT)
Connector 60: | Engine Control Module (ECM) X2 (1.4L) (LDT)
Connector 61: | Engine Control Module (ECM) X1 (1.6L) (LXV)
Connector 62: | Engine Control Module (ECM) X2 (1.6L) (LXV)
Connector 63: | Engine Coolant Temperature (ECT) Sensor
Connector 64: | Engine Coolant Temperature (ECT) Sensor (LDT/LXV)
Connector 65: | Engine Coolant Temperature (ECT) Sensor 2 (LDT/LXV)
Connector 66: | Engine Coolant Thermostat (LDT/LXV)
Connector 67: | Engine Oil Level (EOL) Sensor (NT4)
Connector 68: | Engine Oil Pressure (EOP) Switch (L95/LV8/LXT)
Connector 69: | Engine Oil Pressure (EOP) Switch (LDT/LXV)
Connector 70: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LMU)
Connector 71: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LDT)
Connector 72: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LXV)
Connector 73: | Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (L95/LV8/LXT)
Connector 74: | Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LXV)
Connector 75: | Evaporator Temperature Sensor (without LDT/WHB)
Connector 76: | Exhaust Gas Recirculation (EGR) Valve (LMU)
Connector 77: | Exhaust Gas Recirculation (EGR) Valve (L95/LXT)
Connector 78: | Fog Lamp - Left Front (T96)
Connector 79: | Fog Lamp - Right Front (T96)
Connector 80: | Folding Mirror Unit (Notchback with Folding Mirrors)
Connector 81: | Fuel Injector 1 (LDT/LXV)
Connector 82: | Fuel Injector 2 (LDT/LXV)
Connector 83: | Fuel Injector 3 (LDT/LXV)
Connector 84: | Fuel Injector 4 (LDT/LXV)
Connector 85: | Fuel Injector 1 (LMU/LV8)
Connector 86: | Fuel Injector 2 (LMU/LV8)
Connector 87: | Fuel Injector 3 (LMU/LV8)
Connector 88: | Fuel Injector 4 (LMU/LV8)
Connector 89: | Fuel Injector 1 (L95/LXT with NN1)
Connector 90: | Fuel Injector 2 (L95/LXT with NN1)
Connector 91: | Fuel Injector 3 (L95/LXT with NN1)
Connector 92: | Fuel Injector 4 (L95/LXT with NN1)
Connector 93: | Fuel Injector 1 (L95/LXT without NN1)
Connector 94: | Fuel Injector 2 (L95/LXT without NN1)
Connector 95: | Fuel Injector 3 (L95/LXT without NN1)
Connector 96: | Fuel Injector 4 (L95/LXT without NN1)
Connector 97: | Fuel Pump and Sender Assembly
Connector 98: | Fuel Tank Pressure (FTP) Sensor (NQU)
Connector 99: | Fuel Tank Pressure (FTP) Sensor (WHB)
Connector 100: | Generator (L95/LV8/LXT)
Connector 101: | Generator (LDT/LXV)
Connector 102: | Generator (LMU)
Connector 103: | Hazard Warning Switch
Connector 104: | Headlamp - Left
Connector 105: | Headlamp - Right
Connector 106: | Headlamp Leveling Actuator - Left (T84)
Connector 107: | Headlamp Leveling Actuator - Right (T84)
Connector 108: | Headlamp Leveling Switch (Except North America)
Connector 109: | Headlamp Switch
Connector 110: | Heated Oxygen Sensor (HO2S) 1 (LTD/LXV)
Connector 111: | Heated Oxygen Sensor (HO2S) 1 (L95/LXT without NN1)
Connector 112: | Heated Oxygen Sensor (HO2S) 1 (L95/LXT with NN1)
Connector 113: | Heated Oxygen Sensor (HO2S) 1 (LMU)
Connector 114: | Heated Oxygen Sensor (HO2S) 2 (L95/LXT/LDT/LXV with NOU/NT4/NU2)
Connector 115: | Heated Oxygen Sensor (HO2S) 2 (L95/LV8/LXT with NT3)
Connector 116: | Heated Seat Element - Driver Cushion (C37)
Connector 117: | Hood Ajar Switch
Connector 118: | Horn - Left
Connector 119: | Horn - Right (Hatchback)
Connector 120: | HVAC Control Module X1 (C68)
Connector 121: | HVAC Control Module X2 (C68)
Connector 122: | HVAC Control Module (C60)
Connector 123: | I/P Compartment Lamp Switch (C99)
Connector 124: | I/P Dimmer Switch
Connector 125: | Ignition Control Module (ICM) (LDT/LXV)
Connector 126: | Ignition Control Module (ICM) (without LDT/LXV)
Connector 127: | Ignition Key Alarm Switch (without WHB)
Connector 128: | Ignition Key Illumination Lamp (without WHB)
Connector 129: | Ignition Lock Cylinder Control Actuator (WHB with MLQ)
Connector 130: | Ignition Relay (with WHB)
Connector 131: | Ignition Switch (with WHB)
Connector 132: | Ignition Switch (without WHB)
Connector 133: | Inflatable Restraint Front End Sensor - Left (WHB)
Connector 134: | Inflatable Restraint Front End Sensor - Right (WHB)
Connector 135: | Inflatable Restraint Front Passanger Presence System (PPS) Sensor (C98)
Connector 136: | Inflatable Restraint I/P Module (WHB with C98)
Connector 137: | Inflatable Restraint I/P Module (AK5)
Connector 138: | Inflatable Restraint I/P Module Disable Switch (C99)
Connector 139: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (with WHB)
Connector 140: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (without WHB)
Connector 141: | Inflatable Restraint Side Impact Module - Left (AJ7)
Connector 142: | Inflatable Restraint Side Impact Module - Right (AJ7)
Connector 143: | Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 with C98)
Connector 144: | Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 without C98)
Connector 145: | Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 with C98)
Connector 146: | Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 without C98)
Connector 147: | Inflatable Restraint Steering Wheel Module (WHB with C98)
Connector 148: | Inflatable Restraint Steering Wheel Module (AJ3 without C98)
Connector 149: | Inflatable Restraint Steering Wheel Module Coil (AJ3 with UV8/WHB)
Connector 150: | Instrument Panel Cluster (IPC) X1 (with WHB)
Connector 151: | Instrument Panel Cluster (IPC) X2 (with WHB)
Connector 152: | Instrument Panel Cluster (IPC) X1 (without WHB)
Connector 153: | Instrument Panel Cluster (IPC) X2 (without WHB)
Connector 154: | Intake Air Temperature (IAT) Sensor (without WHB)
Connector 155: | Intake Air Temperature (IAT) Sensor - HVAC (C68)
Connector 156: | Knock Sensor (KS) (LDT/LXV)
Connector 157: | Knock Sensor (KS) (LMU)
Connector 158: | Knock Sensor (KS) (L95/LV8/LXT)
Connector 159: | Lamp Driver Module
Connector 160: | License Lamp
Connector 161: | Manifold Absolute Pressure (MAP) Sensor (LDT/LXV)
Connector 162: | Manifold Absolute Pressure (MAP) Sensor (LMU)
Connector 163: | Manifold Absolute Pressure (MAP) Sensor (LV8)
Connector 164: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LXV)
Connector 165: | Mode Actuator (C68)
Connector 166: | Octane Selection Switch (LDT/LXV)
Connector 167: | Octane Selection Switch (L95/LXT)
Connector 168: | Octane Selection Switch (LMU/LV8)
Connector 169: | OnStar X1 (UE1)
Connector 170: | OnStar X2 (UE1)
Connector 171: | OnStar Backup Battery (UE1)
Connector 172: | OnStar Button Assembly (UE1)
Connector 173: | Outside Rearview Mirror - Driver (Hatchback with DM7)
Connector 174: | Outside Rearview Mirror - Driver (Notchback with DM7)
Connector 175: | Outside Rearview Mirror - Passenger (Hatchback with DM7)
Connector 176: | Outside Rearview Mirror - Passenger (Notchback with DM7)
Connector 177: | Outside Rearview Mirror Switch
Connector 178: | Overhead Console Courtesy/Reading Lamps
Connector 179: | Park Lamp - Left Front (Hatchback with NA)
Connector 180: | Park Lamp - Right Front (Hatchback with NA)
Connector 181: | Park/Neutral Position (PNP) Switch (LMU)
Connector 182: | Park/Neutral Position (PNP) Switch (without LMU)
Connector 183: | Passenger Airbag Disable Switch
Connector 184: | Passenger Presence System (PPS) Sensor
Connector 185: | Radio (UY4)
Connector 186: | Radio X1 (without UY4)
Connector 187: | Radio X2 (without UY4)
Connector 188: | Radio Antenna X1 (UE1)
Connector 189: | Radio Antenna X2 (UE1)
Connector 190: | Radio Antenna X1 (XMR)
Connector 191: | Radio Antenna X2 (XMR)
Connector 192: | Rear Compartment Lamp
Connector 193: | Rear Compartment Lid Ajar Switch
Connector 194: | Rear Compartment Lid Latch Release Actuator (Notchback)
Connector 195: | Rear Compartment Lid Latch Switch (Hatchback)
Connector 196: | Rear Window Defogger Grid X1 (Hatchback)
Connector 197: | Rear Window Defogger Grid X2 (Hatchback)
Connector 198: | Rear Window Defogger Grid (Notchback with UE1)
Connector 199: | Rear Window Defogger Grid ( Notchback without UE1)
Connector 200: | Rear Window Washer Fluid Pump (Hatchback)
Connector 201: | Rear Window Wiper Motor (Hatchback with C25)
Connector 202: | Rear Window Wiper Motor (Hatchback with C16)
Connector 203: | Recirculation Actuator (C60)
Connector 204: | Recirculation Actuator (C68)
Connector 205: | Remote Control Door Lock Receiver (RCDLR) (UA5)
Connector 206: | Rough Road Sensor (without JM4)
Connector 207: | Seat Belt Pretensioner - Driver (A70)
Connector 208: | Seat Belt Pretensioner - Passenger (A70)
Connector 209: | Seat Belt Switch
Connector 210: | Speaker - Left Front
Connector 211: | Speaker - Left Rear
Connector 212: | Speaker - Left Tweeter
Connector 213: | Speaker - Right Front
Connector 214: | Speaker - Right Rear
Connector 215: | Speaker - Right Tweeter
Connector 216: | Starter Relay (MLQ without WHB)
Connector 217: | Stop Lamp Switch
Connector 218: | Sunload Sensor (C68)
Connector 219: | Sunroof Control Module (CF5)
Connector 220: | Tail Lamp - Left (Hatchback with T9E)
Connector 221: | Tail Lamp - Left (Notchback)
Connector 222: | Tail Lamp - Right (Hatchback with T9E)
Connector 223: | Tail Lamp - Right (Notchback)
Connector 224: | Theft Deterrent Alarm
Connector 225: | Theft Detterent Module (TDM) (BAH with WHB)
Connector 226: | Theft Detterent Module (TDM) (BAH without WHB)
Connector 227: | Throttle Body (LMU)
Connector 228: | Throttle Body (LDT/LXV)
Connector 229: | Tire Pressure Module (UJ9)
Connector 230: | Transmission Control Module (TCM) X1
Connector 231: | Transmission Control Module (TCM) X2
Connector 232: | Turn Signal Lamp - Left Front (T84)
Connector 233: | Turn Signal Lamp - Left Front (FL2)
Connector 234: | Turn Signal Lamp - Right Front (T84)
Connector 235: | Turn Signal Lamp - Right Front (FL2)
Connector 236: | Turn Signal/Hazard Flasher Module
Connector 237: | Turn Signal/Multifunction Switch
Connector 238: | Turn Signal Repeater Lamp - Left (Hatchback without NA)
Connector 239: | Turn Signal Repeater Lamp - Left (Hatchback with NA)
Connector 240: | Turn Signal Repeater Lamp - Right (Hatchback without NA)
Connector 241: | Turn Signal Repeater Lamp - Right (Hatchback with NA)
Connector 242: | Vehicle Speed Sensor (VSS) (LDT/LXV with MLM)
Connector 243: | Vehicle Speed Sensor (VSS) (L95/LXT with M/T)
Connector 244: | Vehicle Speed Sensor (VSS) (LMU/LV8 with M/T)
Connector 245: | Vehicle Speed Sensor (VSS) (XG2)
Connector 246: | Vehicle Speed Sensor (VSS) (without XG2)
Connector 247: | Wheel Speed Sensor (WSS) - Left Front (JM4)
Connector 248: | Wheel Speed Sensor (WSS) - Left Rear (JM4)
Connector 249: | Wheel Speed Sensor (WSS) - Right Front (JM4)
Connector 250: | Wheel Speed Sensor (WSS) - Right Rear (JM4)
Connector 251: | Window Motor - Driver (A31/A32)
Connector 252: | Window Motor - Driver (LHD with ABZ)
Connector 253: | Window Motor - Driver (RHD with ABZ)
Connector 254: | Window Motor - Left Rear (A31)
Connector 255: | Window Motor - Passenger (A31)
Connector 256: | Window Motor - Right Rear (A31)
Connector 257: | Window Switch - Driver (ABZ)
Connector 258: | Window Switch - Driver (A31)
Connector 259: | Window Switch - Driver (A32)
Connector 260: | Window Switch - Left Rear (A31)
Connector 261: | Window Switch - Passenger (A31)
Connector 262: | Window Switch - Right Rear (A31)
Connector 263: | Windshield Washer Fluid Pump
Connector 264: | Windshield Wiper Motor
Connector 265: | Windshield Wiper/Washer Switch X1
Connector 266: | Windshield Wiper/Washer Switch X2

### A/C Compressor Clutch (LMU)

#### Connector Part Information

- OEM: MG 610041
- Service: N/A
- Description: 1-Way F 250 Series, KET

#### A/C Compressor Clutch (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | 812 | A/C Compressor Clutch Supply Voltage

### A/C Compressor Clutch (without LMU)

#### Connector Part Information

- OEM: 12162017
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series, Sealed (GY)

#### A/C Compressor Clutch (without LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG/BK | 812 | A/C Compressor Clutch Supply Voltage
B | BK | 51 | Ground (LDT/LXV)
BK | 250 | Ground (L95/LV8/LXT)

### A/C Engine Coolant Temperature (ECT) Sensor (C68)

#### Connector Part Information

- OEM: MG 620490
- Service: N/A
- Description: 2-Way F

#### A/C Engine Coolant Temperature (ECT) Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/RD | -- | Coolant Temperature Sensor Signal
2 | D-BU/WH | -- | Low Reference

### A/C Refrigerant Pressure Sensor

#### Connector Part Information

- OEM: 12078090
- Service: 88988301
- Description: 3-Way F Metri-Pack 150 Series (BK)

#### A/C Refrigerant Pressure Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 432 | 5-Volt Reference (LMU)
OG/BK | 1031 | 5-Volt Reference (L95/LV8/LXT)
L-BU | 1031 | 5-Volt Reference (LDT/LXV)
2 | L-BU | 733 | Low Reference (LMU)
L-BU | 1937 | Low Reference (L95/LV8/LXT)
BN | 1937 | Low Reference (LDT/LXV)
3 | OG/BK | 203 | A/C Refrigerant Pressure Sensor Signal (LMU)
L-BU | 203 | A/C Refrigerant Pressure Sensor Signal (L95/LV8/LXT)
PU | 203 | A/C Refrigerant Pressure Sensor Signal (LDT/LXV)

### Accelerator Pedal Position (APP) Sensor (LDT/LXV)

#### Connector Part Information

- OEM: 174923-2
- Service: N/A
- Description: 6-Way F 070 SRS Series, AMP (BK)

#### Accelerator Pedal Position (APP) Sensor (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/RD | 1161 | APP Sensor 2 Signal
2 | D-GN | 718 | Low Reference
3 | YE | 1162 | APP Sensor 1 Signal
4 | RD | 645 | Low Reference
5 | D-BU | 474 | 5-Volt Reference
6 | GY | 596 | 5-Volt Reference

### Air Temperature Actuator (C68)

#### Connector Part Information

- OEM: MG 651444
- Service: N/A
- Description: 3-Way F 030 Series, KET (WH)

#### Air Temperature Actuator (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/D-BU | -- | 5-Volt Reference
2 | BK | -- | Ground
3 | D-BU | -- | Signal

### Air Temperature Sensor - Inside (C68)

#### Connector Part Information

- OEM: MG 620630
- Service: N/A
- Description: 2-Way M

#### Air Temperature Sensor - Inside (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/BK | -- | Inside Air Temperature Sensor Signal
2 | D-BU/WH | -- | Low Reference

### Ambient Air Temperature Sensor (U68)

#### Connector Part Information

- OEM: PB 295-02020
- Service: N/A
- Description: 2-Way F NMWP 04F-B Assembly

#### Ambient Air Temperature Sensor (U68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 61 | Outside Ambient Air Temperature Sensor Signal
2 | L-GN/BK | 735 | Low Reference

### Ashtray Lamp

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Ashtray Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Illumination Supply Voltage
2 | BK | -- | Ground

### Automatic Transmission

#### Connector Part Information

- OEM: 7283-1407-40
- Service: N/A
- Description: 10-Way, Yazaki (GY)

#### Automatic Transmission

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 898 | Transmission Fluid Temperature Sensor Signal
2 | PK | 1224 | Timing Valve Control
3 | OG | 1226 | Pressure Control Solenoid Control
4 | D-BU | 1225 | Torque Converter Clutch Solenoid Control
5 | L-GN | 1222 | Shift Solenoid 1 Valve Control
6 | OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference
7 | -- | -- | Not Used
8 | YE/BK | 1227 | Low Reference
9 | -- | -- | Not Used
10 | YE/BK | 1223 | Shift Solenoid 2 Valve Control

### Automatic Transmission Input Shaft Speed (ISS) Sensor

#### Connector Part Information

- OEM: 7283-8125-90
- Service: N/A
- Description: 2-Way F, Yazaki (BU)

#### Automatic Transmission Input Shaft Speed (ISS) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 6253 | Input Shaft Speed (ISS) Sensor Low Signal
2 | WH | 6254 | Input Shaft Speed (ISS) Sensor High Signal

### Automatic Transmission Shift Lever

#### Connector Part Information

- OEM: MG 610396
- Service: N/A
- Description: 4-Way F Series Sealed, KET (WH)

#### Automatic Transmission Shift Lever

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | 434 | Automatic Transmission Shift Lock Control (-WHB)
BN | 1075 | Park Position Switch Signal (WHB)
2 | BK | 650 | Ground
3 | OG/BK | 434 | Automatic Transmission Shift Lock Control (-WHB)
BK | 650 | Ground (WHB)
4 | PU | 878 | Stop Lamp Switch Signal (-WHB)
OG/BK | 434 | Automatic Transmission Shift Lock Control (WHB)

### Automatic Transmission Shift Lever Position Indicator

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Automatic Transmission Shift Lever Position Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Right Park Lamp Supply Voltage
2 | D-GN | 230 | Instrument Panel Lamps Dimming Control

### Automatic Transmission Shift Program Switch

#### Connector Part Information

- OEM: MG 610366
- Service: N/A
- Description: 4-Way F PCB 040 Series, KET (WH)

#### Automatic Transmission Shift Program Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
2 | BK | 650 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | D-GN | 230 | Instrument Panel Lamps Dimming Control

### Auxiliary Power Outlet

#### Connector Part Information

- OEM: 174197-1
- Service: N/A
- Description: 2-Way F HSG Series, (Tyco) (BK)

#### Auxiliary Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 450 | Ground
2 | YE | 143 | Accessory Voltage
YE | 143 | Accessory Voltage (UQN)

### Backup Lamp (Hatchback with WHB)

#### Connector Part Information

- OEM: 35843
- Service: N/A
- Description: 2-Way Lamp Socket, Sealed Molex (WH)

#### Backup Lamp (Hatchback with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
-- | WH | 841 | Ignition 2 Voltage
-- | BK | 24 | Backup Lamp Supply Voltage

### Backup Lamp Switch (M/T without LMU)

#### Connector Part Information

- OEM: AK 7207
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series, (BK)

#### Backup Lamp Switch (M/T without LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 841 | Ignition 2 Voltage (-WHB)
BK | 51 | Ground (WHB)
2 | L-GN | 24 | Backup Lamp Supply Voltage

### Backup Lamp Switch (LMU with M/T)

#### Connector Part Information

- OEM: MG 610320
- Service: N/A
- Description: 2-Way F SWP Series, KET (BK)

#### Backup Lamp Switch (LMU with M/T)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 841 | Ignition 2 Voltage
2 | L-GN | 24 | Backup Lamp Supply Voltage

### Blower Motor

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (NA)

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 650 | Ground (C60)
D-BU/RD | -- | Blower Motor Low Control (C68)
2 | OG | 52 | Blower Motor High Control (C60)
RD/WH | -- | Blower Motor High Control (C68)

### Blower Motor Control Module (C68)

#### Connector Part Information

- OEM: MG 610267
- Service: N/A
- Description: 4-Way F

#### Blower Motor Control Module (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/YE | -- | Blower Motor Speed Control
2 | D-BU/RD | -- | Blower Motor Control
3 | -- | -- | Not Used
4 | BK | -- | Ground

### Blower Motor Resistor

#### Connector Part Information

- OEM: MG 610267
- Service: N/A
- Description: 4-Way F 250 D/L Series, KET (NA)

#### Blower Motor Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 60 | Blower Motor Low Control
2 | OG | 52 | Blower Motor High Control
3 | BN | 63 | Blower Motor Medium 1 Control
4 | L-BU | 72 | Medium 2 Blower Motor Control

### Blower Motor Switch (without C68)

#### Connector Part Information

- OEM: MG 610049-5
- Service: N/A
- Description: 6-Way F 250 Series, KET (BK)

#### Blower Motor Switch (without C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 362 | Upper Mode Valve Solenoid Control
2 | OG | 300 | Ignition 3 Voltage
3 | L-BU | 72 | Medium 2 Blower Motor Control
4 | YE | 60 | Low Blower Motor Control
5 | BN | 63 | Blower Motor Medium 1 Control
6 | OG | 52 | Blower Motor High Control

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: MG 610320-5
- Service: N/A
- Description: 2-Way

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 33 | Brake Warning Indicator Control
2 | BK | 50 | Ground (LHD)
BK | 250 | Ground (RHD)

### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust (LDT/LXV)

#### Connector Part Information

- OEM: 284556
- Service: N/A
- Description: 2-Way F 1.5 Series Sealed, Tyco (GY)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 5282 | Camshaft Phaser Exhaust Solenoid (1)
2 | OG/BK | 1732 | Low Reference (-WHB)
PK | 1729 | Low Reference (WHB)

### Camshaft Position (CMP) Actuator Solenoid Valve - Intake (LDT/LXV)

#### Connector Part Information

- OEM: 284556
- Service: N/A
- Description: 2-Way F 1.5 Series Sealed, Tyco (GY)

#### Camshaft Position (CMP) Actuator Solenoid Valve - Intake (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 5272 | Camshaft Phaser Intake Solenoid (2)
2 | OG/BK | 1732 | Low Reference (-WHB)
PK | 1730 | Low Reference (WHB)

### Camshaft Position (CMP) Sensor - Exhaust (LDT/LXV)

#### Connector Part Information

- OEM: 805-121-522
- Service: N/A
- Description: 3-Way F 1.2 Series, Sealed (BK)

#### Camshaft Position (CMP) Sensor - Exhaust (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 1666 | 5-Volt Reference
2 | BK | 5276 | Low Reference
3 | YE | 630 | CMP Sensor Signal

### Camshaft Position (CMP) Sensor - Intake (LDT/LXV)

#### Connector Part Information

- OEM: 805-121-522
- Service: N/A
- Description: 3-Way F 1.2 Series, Sealed (BK)

#### Camshaft Position (CMP) Sensor - Intake (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 1667 | 5-Volt Reference
2 | BK | 5276 | Low Reference
3 | YE | 633 | CMP Sensor Signal

### Camshaft Position (CMP) Sensor (LMU)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer Series (BK)

#### Camshaft Position (CMP) Sensor (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | 630 | Camshaft Position (CMP) Sensor Signal
2 | YE | 1748 | Low Reference
3 | OG | 1732 | Ignition 1 Voltage

### Camshaft Position (CMP) Sensor (L95/LXT)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer Series (BK)

#### Camshaft Position (CMP) Sensor (L95/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | BK | 50 | Low Reference
3 | L-BU/BK | 1748 | Camshaft Position (CMP) Sensor Signal

### Camshaft Position (CMP) Sensor (LV8)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer Series (BK)

#### Camshaft Position (CMP) Sensor (LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | 1748 | Camshaft Position (CMP) Sensor Signal
2 | OG | 52 | Low Reference
3 | PK | 539 | Ignition 1 Voltage

### Cellular Telephone Microphone (UE1)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way F Metri-Pack 150 Series

#### Cellular Telephone Microphone (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 655 | Cellular Microphone Signal
2 | D-GN | 654 | Cellular Telephone Microphone Low Reference

### Cellular Telephone Microphone (UV8)

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Cellular Telephone Microphone (UV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU/BK | 659 | Cellular Telephone Voice Low Reference
2 | D-BU | 658 | Cellular Telephone Voice Signal

### Center High Mounted Stop Lamp (CHMSL) (TS6)

#### Connector Part Information

- OEM: MG 610392
- Service: N/A
- Description: 2-Way F SDL Series, KET (WH)

#### Center High Mounted Stop Lamp (CHMSL) (TS6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 850 | Ground
2 | L-BU | 20 | Stop Lamp Supply Voltage

### Center High Mounted Stop Lamp (CHMSL) (Notchback with T43)

#### Connector Part Information

- OEM: MG 630679
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Center High Mounted Stop Lamp (CHMSL) (Notchback with T43)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 20 | Stop Lamp Supply Voltage
2 | BK | 450 | Ground

### Cigar Lighter

#### Connector Part Information

- OEM: MG 630685-5
- Service: N/A
- Description: 2-Way F 250 Series, KET (BK)

#### Cigar Lighter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 450 | Ground
2 | YE | 143 | Accessory Voltage

### Clock

#### Connector Part Information

- OEM: 5557-10R
- Service: N/A
- Description: 10-Way F Mini-Fit Jr Series, MLX (NA)

#### Clock

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 1358 | DIC Switch Signal (AJ3-WHB)
2 | -- | -- | Not Used
3 | YE | 749 | Security Indicator Control
4 | GY/BK | 1357 | Passenger Air Bag ON Indicator Control (AJ3)
5 | D-GN/WH | 1358 | Passenger Air Bag OFF Indicator Control (AJ3)
6 | PK | 139 | Ignition 1 Voltage
7 | BN/WH | 309 | Right Park Lamp Supply Voltage
8 | YE | 43 | Accessory Voltage
9 | BK | 650 | Ground
10 | RD/WH | 540 | Battery Positive Voltage

### Clutch Pedal Position (CPP) Switch (WHB with MLM)

#### Connector Part Information

- OEM: MG 612034
- Service: N/A
- Description: 3-Way F ASC Series, KET (WH)

#### Clutch Pedal Position (CPP) Switch (WHB with MLM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 6338 | Manual Transmission Clutch Position Sensor Signal Position
2 | OG | 7360 | Manual Transmission Clutch Position Sensor Return
3 | BN | 7361 | Manual Transmission Clutch Position Sensor Supply

### Cooling Fan

#### Connector Part Information

- OEM: 176146-2
- Service: N/A
- Description: 2-Way F 187 Series, Sealed Tyco (BK)

#### Cooling Fan

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | GY | 532 | Cooling Fan Motor Supply Voltage

### Courtesy/Reading Lamp (without Sunroof)

#### Connector Part Information

- OEM: MG 610489
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (NA)

#### Courtesy/Reading Lamp (without Sunroof)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 157 | Courtesy Lamp Control
2 | RD/WH | 1340 | Battery Positive Voltage

### Crankshaft Position (CKP) Sensor (LDT/LXV)

#### Connector Part Information

- OEM: 1928403870
- Service: 88953312
- Description: 3-Way F Junior Power Timer Series, Sealed Bosch (BK)

#### Crankshaft Position (CKP) Sensor (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 1867 | Crankshaft Position (CKP) Sensor Signal
2 | BK | 1869 | Low Reference
3 | PU | 1868 | 5-Volt Reference

### Crankshaft Position (CKP) Sensor (without LDT/LXV)

#### Connector Part Information

- OEM: 85205-1
- Service: N/A
- Description: 3-Way F JR Power Timer Series, Tyco (BK)

#### Crankshaft Position (CKP) Sensor (without LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | 1868 | Low Reference
3 | BK | 50 | Ground

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: MG 610761
- Service: N/A
- Description: 16-Way F SP Series, KET (BK)

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 5060 | Low Speed GMLAN Serial Data (WHB)
2-3 | -- | -- | Not Used
4 | BK | 450 | Ground
5 | BK | 450 | Ground
6 | D-GN | 1807 | Class 2 Serial Data (Primary) (WHB)
PU | 1807 | Class 2 Serial Data (Primary) (-WHB)
7 | BK/WH | 2051 | Serial Data Signal
8 | BK/WH | 2051 | Serial Data Signal (UA5)
9-13 | -- | -- | Not Used
14 | YE | 710 | Class 2 Serial Data (-WHB)
YE/BK | 710 | Class 2 Serial Data (WHB)
15 | -- | -- | Not Used
16 | RD/WH | 240 | Battery Positive Voltage

### Data Link Connector (DLC) 2 (JM4)

#### Connector Part Information

- OEM: MG 640329-5
- Service: N/A
- Description: 3-Way M SWP Series, KET (BK)

#### Data Link Connector (DLC) 2 (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | BK/WH | 2051 | Serial Data Signal
3 | PK | 539 | Ignition + Voltage

### Door Handle Switch - Driver (LHD with AU3)

#### Connector Part Information

- OEM: AK 32421
- Service: N/A
- Description: 4-Way M Metri-Pack 150 Series, Packard (GY)

#### Door Handle Switch - Driver (LHD with AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 195 | Door Lock Control
B | BK | 650 | Ground
C | WH | 194 | Door Unlock Control
D | L-GN/RD | 262 | Driver Door Key Switch Signal

### Door Handle Switch - Driver (RHD) (AU3)

#### Connector Part Information

- OEM: AK 32421
- Service: N/A
- Description: 4-Way M Metri-Pack 150 Series, Packard (GY)

#### Door Handle Switch - Driver (RHD) (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN/RD | 262 | Driver Door Key Switch Signal
B | WH | 194 | Door Unlock Control
C | BK | 650 | Ground
D | L-BU | 195 | Door Lock Control

### Door Handle Switch - Passenger (LHD with AU3)

#### Connector Part Information

- OEM: AK 32421
- Service: N/A
- Description: 4-Way M Metri-Pack 150 Series, Packard (GY)

#### Door Handle Switch - Passenger (LHD with AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN/RD | 265 | Passenger Door Key Switch Signal
B | -- | -- | Not Used
C | BK | 650 | Ground
D | -- | -- | Not Used

### Door Handle Switch - Passenger (RHD with AU3)

#### Connector Part Information

- OEM: AK 32421
- Service: N/A
- Description: 4-Way M Metri-Pack 150 Series, Packard (GY)

#### Door Handle Switch - Passenger (RHD with AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BK | 650 | Ground
C | -- | -- | Not Used
D | L-GN/RD | 265 | Passenger Door Key Switch Signal

### Door Lock Actuator - Driver (AU3)

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed Packard (BK)

#### Door Lock Actuator - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control
2 | BN | 294 | Door Lock Actuator Unlock Control

### Door Lock Actuator - Left Rear (AU3)

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed Packard (BK)

#### Door Lock Actuator - Left Rear (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control
2 | BN | 294 | Door Lock Actuator Unlock Control

### Door Lock Actuator - Liftgate (AU3)

#### Connector Part Information

- OEM: MG 620490
- Service: N/A
- Description: 2-Way M 090 Series, KET (WH)

#### Door Lock Actuator - Liftgate (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 294 | Door Lock Actuator Unlock Control
2 | GY | 295 | Door Lock Actuator Lock Control

### Door Lock Actuator - Passenger (AU3)

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed Packard (BK)

`

#### Door Lock Actuator - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control
2 | BN | 294 | Door Lock Actuator Unlock Control

### Door Lock Actuator - Right Rear (AU3)

#### Connector Part Information

- OEM: AK 6023
- Service: N/A
- Description: 2-Way F Metri-Pack 280 Series, Sealed Packard (BK)

#### Door Lock Actuator - Right Rear (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 295 | Door Lock Actuator Lock Control
2 | BN | 294 | Door Lock Actuator Unlock Control

### Electronic Brake Control Module (EBCM) (JM4)

#### Connector Part Information

- OEM:: 1612683-2
- Service: N/A
- Description: 26-Way F 060/187 Series, Tyco (BK)

#### Electronic Brake Control Module (EBCM) (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 40 | Battery Positive Voltage
2 | BN | 884 | Left Rear Wheel Speed Sensor Signal
3 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference
4 | -- | -- | Not Used
5 | BN | 833 | Right Front Wheel Speed Sensor Low Reference
6 | D-GN | 872 | Right Front Wheel Speed Sensor Signal
7 | -- | -- | Not Used
8 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
9 | YE | 873 | Left Front Wheel Speed Sensor Low Reference
10 | L-GN/BK | 867 | ABS Indicator Failure Control
11 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference
12 | BN | 882 | Right Rear Wheel Speed Sensor Signal
13 | BK | 50 | Ground
14 | RD | 40 | Battery Positive Voltage
15 | -- | -- | Not Used
16 | L-BU | 20 | Stop Lamp Supply Voltage
17 | -- | -- | Not Used
18 | BK/WH | 2051 | Serial Data Signal
19 | PK | 539 | Ignition 1 Voltage
20-25 | -- | -- | Not Used
26 | BK | 50 | Ground

### Engine Control Module (ECM) - Sirius D42 (1.2L) (LMU)

#### Connector Part Information

- OEM: FC1
- Service: N/A
- Description: 90-Way Connector (BK)

#### Engine Control Module (ECM) - Sirius D42 (1.2L) (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | BK | 50 | Ground
4 | -- | -- | Not Used
5 | BN | 697 | Exhaust Gas Recirculation (EGR) Valve Control
6 | L-GN | 497 | Fuel Pump Relay Control
7 | BN | 1741 | Main Relay Control
8 | D-GN | 135 | Engine Coolant Temperature (ECT) Gage Signal
9 | D-BU | 473 | High Speed Cooling Fan Relay Control
10 | D-GN | 335 | Low Speed Cooling Fan Relay Control
11 | BK/WH | 51 | Ground
12 | WH | 1876 | Low Reference
13 | BN | 469 | Low Reference
14 | PU | 1666 | Heated Oxygen Sensor (HO2S) 2 Low Reference
15 | -- | -- | Not Used
16 | L-BU | 733 | Low Reference
17 | YE | 748 | Low Reference
18 | -- | -- | Not Used
19 | BN | 808 | Low Reference
20 | OG/BK | 203 | A/C Pressure Sensor Signal
21 | PK | 427 | Fuel Level Sensor Signal
22 | L-GN/WH | 630 | Camshaft Position (CMP) Sensor Signal
23 | WH/BK | -- | Serial Data
24 | BK | 50 | Ground
25 | BK/WH | 51 | Ground
26 | -- | -- | Not Used
27 | BN | 892 | Octane Selector Switch
28 | BK | 50 | Ground
29 | PK | 1739 | Ignition 1 Voltage
30 | RD/WH | 440 | Battery Positive Voltage
31 | WH | 423 | Ignition Coil and 2 and 3 Control
32 | OG | 406 | Ignition Coil and 1 and 4 Control
33 | BK | 50 | Ground
34 | -- | -- | Not Used
35 | PK/BK | 3113 | Heated Oxygen Sensor (HO2S) 1 Signal
36-38 | -- | -- | Not Used
39 | BN/WH | 419 | Malfunction Indicator Lamp (MIL) Control
40 | PU | 30 | Fuel Gage Control
41 | PU/WH | 67 | A/C Clutch Relay Control (C60)
42 | OG | 496 | Knock Sensor (KS) Signal
43 | D-GN | 534 | Idle Motor Position Signal
44 | D-GN/WH | 1665 | Heated Oxygen Sensor (HO2S) 1 Low Reference
45 | GY | 5763 | Exhaust Gas Recirculation (EGR) Valve Control
46 | L-BU | 1936 | Fuel Level Sensor Signal
47-48 | -- | -- | Not Used
49 | D-BU | 732 | Evaporator Temperature Sensor Signal
50 | L-GN | 432 | 5-Volt Reference
51 | D-GN/WH | 817 | Vehicle Speed Signal
52 | D-GN/WH | 762 | A/C Request Signal
53 | L-BU | 830 | Rough Road Signal
54 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
55 | PK | 427 | Idle Switch Position Signal
56 | BK/WH | 2051 | Serial Data Signal
57 | YE | 710 | CAN Serial Data Low
58 | -- | -- | Not Used
59 | L-BU/WH | 1747 | Fuel Injector 1 Control
60 | L-GN/BK | 1745 | Fuel Injector 3 Control
61 | L-BU | 425 | Idle Speed Motor Feed
62 | D-BU | 426 | Idle Speed Motor Return
63 | -- | -- | Not Used
64 | BN | 3122 | Heated Oxygen Sensor (HO2S) 2 Signal
65 | BN | 428 | EVAP Canister Purge Valve Solenoid Control
66 | OG/BK | 1733 | Ignition 3 Voltage
67 | BK | 50 | Ground
68 | WH | 121 | Engine Speed Signal
69-73 | -- | -- | Not Used
74 | D-BU | 417 | Throttle Position (TP) Sensor Signal
75 | GY/BK | 433 | Manifold Absolute Pressure (MAP) Sensor Signal
76 | YE | 410 | Engine Coolant Temperature (ECT) Sensor Signal
77 | -- | -- | Not Used
78 | RD | 468 | Intake Air Temperature (IAT) Sensor Signal
79 | GY | 416 | 5-Volt Reference
80 | -- | -- | Not Used
81 | D-GN | 890 | Octane Selection Switch
82 | -- | -- | Not Used
83 | GY | 1056 | Power Steering Pressure Switch Signal
84 | YE | 873 | Rough Road Sensor Return
85 | YE/BK | 1868 | Low Reference
86-87 | -- | -- | Not Used
88 | PU | 1807 | CAN Serial Data High
89 | BN | 1744 | Fuel Injector 4 Control
90 | PK/BK | 1746 | Fuel Injector 2 Control

### Engine Control Module (ECM) X1 (1.5L) (LV8)

#### Connector Part Information

- OEM: 12129231
- Service: N/A
- Description: 32-Way Retainer Lock (BK)

#### Engine Control Module (ECM) X1 (1.5L) (LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | BK | 50 | Ground
3 | D-BU | 496 | Knock Sensor (KS) Signal
4-5 | -- | -- | Not Used
6 | YE/BK | -- | Low Reference
7 | L-BU | 425 | Throttle Position (TP) Sensor Signal
8 | L-GN/BK | 1745 | Fuel Injector 3 Control
9 | L-BU/WH | 1747 | Fuel Injector 1 Control
10 | OG | 52 | Low Reference
11 | YE | 410 | Engine Coolant (ECT) Temperature Sensor Signal
12 | D-GN/WH | 412 | Oxygen Sensor (O2) Signal
13 | D-BU | 417 | Idle Air Control (IAC) B High Control
14 | -- | -- | Not Used
15 | PK | 427 | 5-Volt Reference
16 | D-BU | 732 | Low Reference
17 | BK | 50 | Ground
18 | WH | 423 | Ignition Coil 2 and 3 Control
19 | OG | 406 | Ignition Coil 1 and 4 Control
20 | D-GN/WH | 428 | EVAP Canister Purge Valve Solenoid Control
21 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
22 | PK/BK | 1746 | Fuel Injector 2 Control
23 | BN | 6118 | Intake Air Temperature (IAT) Sensor Signal
24 | D-GN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
25 | L-BU/BK | 1748 | Camshaft Position (CMP) Sensor Signal
26 | BN | 1744 | Fuel Injector 4 Control
27 | BN | 1665 | Oxygen Sensor (O2) Low Reference
28 | D-GN | 534 | Idle Air Control (IAC) A High Control
29 | PK/BK | 415 | Idle Air Control (IAC) B Low Control
30 | L-GN/BK | 444 | Idle Air Control (IAC) A Low Control
31 | PU | 719 | 5-Volt Reference
32 | BN | 808 | Low Reference

### Engine Control Module (ECM) X2 (1.5L) (LV8)

#### Connector Part Information

- OEM: PED 12129232
- Service: N/A
- Description: 32-Way Retainer Lock (CL)

#### Engine Control Module (ECM) X2 (1.5L) (LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 1937 | Low Reference
2 | RD/WH | 440 | Battery Positive Voltage
3 | PK | 1739 | Ignition 1 Voltage
4-6 | -- | -- | Not Used
7 | L-BU | 203 | A/C Pressure Sensor Signal
8 | D-GN | 892 | Octane Selection Signal 2
9 | WH | 121 | Engine Speed Signal
10 | D-GN/WH | 732 | A/C Request Signal
11 | -- | -- | Not Used
12 | D-BU | 473 | High Speed Cooling Fan Control
13 | -- | -- | Not Used
14 | PU | 1807 | CAN Serial Data High
15 | BK/WH | 2051 | Serial Data Signal
16 | -- | -- | Not Used
17 | OG/BK | 1031 | 5-Volt Reference
18 | RD/WH | 440 | Battery Positive Voltage
19 | D-BU | 1936 | Fuel Level Sensor Signal
20-21 | -- | -- | Not Used
22 | D-GN | 890 | Octane Selection Signal 1
23 | D-GN/WH | 817 | Vehicle Speed Sensor (VSS) Signal (Manual Transmission)
24 | D-GN | 135 | Engine Coolant Temperature (ECT) Gage Control
25 | -- | -- | Not Used
26 | L-GN | 497 | Fuel Pump Relay Control
27 | GY/D-GN | 355 | Low Speed Cooling Fan Relay Control
28 | PU/WH | 67 | A/C Clutch Relay Control
29 | -- | -- | Not Used
30 | YE | 710 | Can Serial Data Low
31 | PU | 30 | Fuel Gage Control
32 | BN/WH | 419 | MIL Control

### Engine Control Module (ECM) X1 (1.4L, 1.6L) (L95, LXT)

#### Connector Part Information

- OEM: 1-368434-1
- Service: N/A
- Description: 64-Way F ECU 64P Series, Tyco (BN)

#### Engine Control Module (ECM) X1 (1.4L, 1.6L) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 440 | Battery Positive Voltage
2-4 | -- | -- | Not Used
5 | D-GN | 892 | Octane Selector Switch Signal
6 | D-GN/WH | 817 | Vehicle Speed Signal (M/T)
7 | BN | 834 | Rough Road Signal with ABS (JM4)
8-11 | -- | -- | Not Used
12 | D-BU | 473 | High Speed Cooling Fan Relay Control
13 | YE | 492 | Intake Manifold Tuning Valve Control
14 | PU | 1807 | CAN Serial Data High
15 | YE | 710 | CAN Serial Data Low
16 | BK | 50 | Ground
17 | RD/WH | 440 | Battery Positive Voltage
18 | PK | 1739 | Ignition 1 Voltage
19-20 | -- | -- | Not Used
21 | D-GN | 602 | Rough Road Signal (-ABS)
22 | L-BU | 203 | Air Conditioning Refrigerant Pressure Switch Signal
23 | -- | -- | Not Used
24 | D-GN | 135 | Engine Coolant Temperature Gage Control
25 | WH | 121 | Engine Speed Signal
26-27 | -- | -- | Not Used
28 | GY/D-GN | 355 | Low Speed Cooling Fan Relay Control
29 | PU/WH | 67 | Air Conditioning Compressor Clutch Relay Control
30 | PU | 30 | Fuel Gage Control
31 | -- | -- | Not Used
32 | BK/WH | 2051 | Serial Data Signal
33 | -- | -- | Not Used
34 | L-BU | 1937 | Low Reference
35 | D-GN/WH | 762 | Air Conditioning Request Signal
36 | BN | 413 | Heated Oxygen Sensor 2 Signal
37-49 | -- | -- | Not Used
50 | OG/BK | 1031 | 5-Volt Reference
51 | D-BU | 1936 | Fuel Level Sensor Signal
52 | -- | -- | Not Used
53 | PU | 1670 | Heated Oxygen Sensor 2 Low Reference
54 | L-GN | 497 | Fuel Pump Relay Control
55-63 | -- | -- | Not Used
64 | BN/WH | 419 | Malfunction Indicator Lamp Control

### Engine Control Module (ECM) X2 (1.4L, 1.6L) (L95, LXT)

#### Connector Part Information

- OEM: 0-368434-1
- Service: N/A
- Description: 64-Way F ECU 64P Series, Tyco (BK)

#### Engine Control Module (ECM) X2 (1.4L, 1.6L) (L95, LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 423 | Ignition Coil 2 and 3 Control
2 | BN | 1671 | Heated Oxygen Sensor 2 Heater Control
3 | PK | 539 | Ignition 1 Voltage
4 | BN | 452 | EVAP Canister Purge Solenoid Control
5 | YE/BK | 1868 | Low Reference
6 | L-BU | 425 | Throttle Position Sensor Signal
7 | BN | 6118 | Intake Air Temperature (IAT) Sensor Signal
8 | L-GN | 432 | Exhaust Gas Recirculation (EGR) Valve Signal
9 | GY | 5763 | Exhaust Gas Recirculation (EGR) Valve Position Sensor Signal
10 | -- | -- | Not Used
11 | BN | 1744 | Fuel Injector #4 Control
12 | GN/WH | 428 | Heated Oxygen Sensor 1 Low Reference
13 | D-GN | 534 | High Idle Switch Output
14 | PK/BK | 415 | Idle Air Control (IAC) Valve Coil B Low Control
15 | L-GN/BK | 444 | Idle Air Control (IAC) Valve Coil A Low Control
16 | PU | 719 | 5-Volt Reference
17 | -- | -- | Not Used
18 | D-BU | 496 | Knock Sensor Signal
19 | WH | 257 | Exhaust Gas Recirculation Valve Control
20 | -- | -- | Not Used
21 | D-BU/WH | 1869 | Crankshaft Position Sensor Signal
22 | PK/BK | 1746 | Fuel Injector 2 Control
23 | -- | -- | Not Used
24 | L-GN/BK | 1745 | Fuel Injector 3 Control
25 | L-BU/WH | 1747 | Fuel Injector 1 Control
26 | L-BU/BK | 1748 | Camshaft Position Sensor Signal
27 | -- | -- | Not Used
28 | YE | 410 | Engine Coolant Temperature Sensor Signal
29 | BN | 1665 | Heated Oxygen Sensor 1 Signal
30 | D-BU | 417 | Idle Air Control (IAC) Valve Coil B High Control
31 | -- | -- | Not Used
32 | PK | 427 | 5-Volt Reference
33 | WH | 423 | Ignition Coil 2 and 3 Control
34 | -- | -- | Not Used
35 | OG | 406 | Ignition Coil 1 and 4 Control
36 | -- | -- | Not Used
37 | BK | 50 | Ground
38 | BK | 50 | Ground
39 | BK | 50 | Ground
40 | BK | 50 | Ground
41 | BK | 50 | Ground
42-47 | -- | -- | Not Used
48 | BN/WH | 469 | Low Reference
49-50 | -- | -- | Not Used
51 | OG | 406 | Ignition Coil 1 and 4 Control
52 | WH | 257 | Exhaust Gas Recirculation Valve Control
53-63 | -- | -- | Not Used
64 | BN | 808 | Low Reference

### Engine Control Module (ECM) X1 (1.4L) (LDT)

#### Connector Part Information

- OEM:15452126
- Service: N/A
- Description: 73-Way F Micro Pack 064 Series, Sealed (BK)

#### Engine Control Module (ECM) X1 (1.4L) (LDT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 440 | Battery Positive Voltage
2 | -- | -- | Not Used
3 | PK | 539 | Ignition 1 Voltage
4-9 | -- | -- | Not Used
10 | L-BU | 830 | Rough Road Sensor Signal
11 | YE | 873 | Rough Road Sensor Return
12 | WH | 1162 | APP Sensor 2 Signal
13 | GY | 121 | Engine Speed Signal
14-15 | -- | -- | Not Used
16 | YE | 710 | CAN Bus High Serial Data
17 | -- | -- | Not Used
18 | BN | 20 | Brake Switch Signal
19-21 | -- | -- | Not Used
22 | OG | 1733 | Ignition 1 Voltage
23-24 | -- | -- | Not Used
25 | PU | 203 | A/C High Side Pressure Sensor Signal
26 | -- | -- | Not Used
27 | D-BU | 1161 | APP Sensor 1 Signal
28 | BN/BK | 1030 | Fuel Tank Pressure (FTP) Sensor Signal
29 | -- | -- | Not Used
30 | BN | 413 | Heated Oxygen Sensor (HO2S) 1 Hi Signal
31 | -- | -- | Not Used
32 | PU | 1807 | CAN Bus Low Serial Data
33-34 | -- | -- | Not Used
35 | GY | 596 | 5-Volt Reference
36 | GY | 474 | 5-Volt Reference
37 | BN | 1937 | Low Reference
38 | -- | -- | Not Used
39 | YE | 645 | Low Reference
40 | BN | 415 | Engine Coolant Temperature Sensor 2 Signal
41 | L-BU | 817 | Vehicle Speed Signal
42-44 | -- | -- | Not Used
45 | L-BU | 834 | Low Reference
46 | BN | 1671 | Oxygen Sensor 2 Heater Low Control
47 | -- | -- | Not Used
48 | BN | 419 | Malfunction Indicator Lamp Control
49 | GY | 1936 | Fuel Level Sensor Signal
50 | -- | -- | Not Used
51 | PU/WH | 67 | A/C Compressor Relay Control
52 | WH | 30 | Fuel Gage Control
53 | -- | -- | Not Used
54 | D-GN/WH | 718 | Low Reference
55 | WH | 1977 | Low Reference
56-57 | -- | -- | Not Used
58 | L-BU | 1031 | 5-Volt Reference
59 | BN | 1937 | Low Reference
60 | YE | 1578 | EVAP Canister Purge Solenoid Control
61 | -- | -- | Not Used
62 | BN | 441 | MAIN Relay Control
63-64 | -- | -- | Not Used
65 | D-GN/WH | 762 | A/C Request Signal
66 | D-BU | 473 | Ignition Coil B Control
67 | GY/D-GN | 355 | Oxygen Sensor 1 Heater Low Control
68 | WH | 135 | Ground
69-70 | -- | -- | Not Used
71 | L-GN | 497 | Fuel Pump Relay Control
72 | BK/WH | 2051 | Serial Data Signal
73 | BK | 50 | Ground

### Engine Control Module (ECM) X2 (1.4L) (LDT)

#### Connector Part Information

- OEM: PE155848
- Service: N/A
- Description: 73-Way F Micro Pack 064 Series, Sealed (GY)

#### Engine Control Module (ECM) X2 (1.4L) (LDT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 423 | Ignition Coil A Control
2 | WH | 428 | Low Reference
3 | PU | 427 | Low Reference
4 | L-BU | 426 | 5-Volt Reference
5 | PU | 1868 | Crankshaft Position (CKP) Sensor Signal
6 | WH | 433 | 5-Volt Reference
7 | PU | 1666 | Camshaft Position (CMP) Sensor - Exhaust Signal
8 | -- | -- | Not Used
9 | WH | 6118 | 5-Volt Reference
10 | BN | 1665 | Heated Oxygen Sensor (HO2S) 1 Hi Signal
11 | -- | -- | Not Used
12 | OG | 496 | Knock Sensor Signal
13 | -- | -- | Not Used
14 | GY | 53 | Oxygen Sensor 1 Heater Low Control
15-16 | -- | -- | Not Used
17 | BK | 405 | Ignition Coil B Control
18 | BK | 5276 | Camshaft Position (CMP) Sensor - Intake Signal
19-20 | -- | -- | Not Used
21 | YE | 1867 | Low Reference
22 | -- | -- | Not Used
23 | PU | 1667 | 5-Volt Reference
24 | BN | 808 | Low Reference
25 | -- | -- | Not Used
26 | WH | 425 | Throttle Position Sensor 1 Signal
27 | L-BU | 469 | Manifold Absolute Pressure (MAP) Sensor Signal
28 | WH | 1876 | Low Reference
29 | BN | 410 | 5-Volt Reference
30-32 | -- | -- | Not Used
33 | D-BU | 424 | Ignition Coil C Control
34 | BK | 5276 | 5-Volt Reference
35 | BK | 1869 | 5-Volt Reference
36-38 | -- | -- | Not Used
39 | BN/BK | 486 | Throttle Position Sensor 2 Signal
40-44 | -- | -- | Not Used
45 | BN | 892 | Octane Selector Switch Signal
46 | D-GN | 890 | Octane Selector Switch Signal
47-52 | -- | -- | Not Used
53 | PU | 406 | Ignition Coil D Control
54 | BN | 5272 | Camshaft Position (CMP) Actuator Solenoid Valve - Intake Control Signal
55 | YE | 630 | Low Reference
56 | YE | 633 | Low Reference
57 | WH | 452 | EVAP Canister Purge Solenoid Control
58 | BN | 465 | Camshaft Position (CMP) Actuator Solenoid Valve - Exhaust Control Signal
59 | BN | 5282 | 5-Volt Reference
60 | -- | -- | Not Used
61 | L-BU | 581 | ETC Motor Close
62 | -- | -- | Not Used
63 | WH | 1746 | Fuel Injector 2 Control
64 | L-GN/BK | 1745 | Fuel Injector 3 Control
65 | L-BU/WH | 1747 | Fuel Injector 1 Control
66 | BN | 1744 | Fuel Injector 4 Control
67 | D-BU | 528 | ETC Motor Open
68-73 | -- | -- | Not Used

### Engine Control Module (ECM) X1 (1.6L) (LXV)

#### Connector Part Information

- OEM: 54395602
- Service: N/A
- Description: 56-Way F Connector Assembly (BK)

#### Engine Control Module (ECM) X1 (1.6L) (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 419 | Malfunction Indicator Lamp Control
2 | L-GN | 497 | Fuel Pump Relay Control
3 | OG | 1733 | Ignition 1 Voltage
4 | PU/WH | 67 | A/C Compressor Relay Control
5 | GY | 474 | Low Reference
6 | YE | 1578 | EVAP Canister Vent Solenoid Control
7 | L-GN/BK | 822 | Low Reference (MLM)
8-9 | -- | -- | Not Used
10 | PU | 1807 | CAN Bus High Serial Data - Terminated
11 | YE | 710 | CAN Bus Low Serial Data - Terminated
12 | RD/WH | 440 | Battery Positive Voltage
13 | -- | -- | Not Used
14 | PK | 539 | Ignition 1 Voltage
15 | D-BU | 473 | FAN HI Relay Control
16 | BN | 441 | MAIN Relay Control
17-18 | -- | -- | Not Used
19 | GY | 596 | 5-Volt Reference
20 | YE | 645 | Low Reference
21 | D-GN/WH | 718 | Low Reference
22 | -- | -- | Not Used
23 | OG | 7360 | Low Reference (MLM)
24 | BN | 456 | Low Reference
25 | BN | 20 | Brake Switch Signal
26 | BN | 323 | Neutral Start Signal
27 | L-BU | 817 | Vehicle Speed Sensor (VSS) Signal (MLM)
28 | L-BU | 24 | Backup Lamp Supply Voltage (MLM)
29 | L-GN | 323 | Starter Relay Control
30-31 | -- | -- | Not Used
32 | BN | 7361 | 5-Volt Reference (MLM)
33 | L-BU | 1031 | 5-Volt Reference
34 | L-BU | 1031 | 5-Volt Reference
35 | -- | -- | Not Used
36 | BN | 7007 | Vehicle Wake Up Signal
37 | -- | -- | Not Used
38 | BN | 1973 | Low Reference
39 | -- | -- | Not Used
40 | WH | 1162 | APP Sensor 2 Signal
41 | PU | 203 | A/C High Side Pressure Sensor Signal
42 | D-BU | 1161 | APP Sensor 1 Signal
43 | BN | 465 | Cold Start Fuel Injector Control
44 | D-GN | 355 | FAN LOW Relay Control
45 | BN | 1937 | Low Reference
46 | WH | 1977 | Low Reference
47 | D-GN | 605 | 5-Volt Reference (MLM)
48-50 | -- | -- | Not Used
51 | L-BU | 469 | MAF Sensor Signal
52 | GY | 1936 | Fuel Level Sensor Signal
53 | BN | 415 | Engine Coolant Temperature (ECT) Sensor 2 Signal
54 | WH | 455 | Intake Air Temperature (IAT) Sensor Signal
55 | L-BU | 1030 | Fuel Tank Pressure (FTP) Sensor Signal
56 | D-BU | 6338 | Clutch Pedal Position (CPP) Sensor Signal (MLM)

### Engine Control Module (ECM) X2 (1.6L) (LXV)

#### Connector Part Information

- OEM: 54397302
- Service: N/A
- Description: 73-Way F Connector Assembly (BK)

#### Engine Control Module (ECM) X2 (1.6L) (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 225 | Generator L Terminal
2 | -- | -- | Not Used
3 | BN | 413 | Heated Oxygen Sensor (HO2S) 2 Hi Signal
4 | BN | 1665 | Heated Oxygen Sensor (HO2S) 1 Hi Signal
5 | BN/BK | 486 | Throttle Position Sensor 1 Signal
6-7 | -- | -- | Not Used
8 | L-BU | 469 | Manifold Absolute Pressure (MAP) Sensor Signal
9 | WH | 425 | Throttle Position Sensor 2 Signal
10 | PU | 1670 | Low Reference
11 | YE | 630 | Camshaft Position (CMP) Sensor - Exhaust Signal
12 | BN | 1744 | Fuel Injector 4
13 | PK | 1729 | Low Reference
14 | BN | 5282 | Camshaft Position (CMP) Actuator Solenoid Valve-Exhaust Control Signal
15 | PK | 1730 | Low Reference
16 | WH | 1746 | Fuel Injector 2
17 | -- | -- | Not Used
18 | PU | 1868 | 5-Volt Reference
19 | -- | -- | Not Used
20 | WH | 428 | Low Reference
21 | OG | 23 | Generator F Terminal
22-23 | -- | -- | Not Used
24 | D-GN | 31 | Engine Oil Pressure Switch
25 | BN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
26 | YE | 1867 | Crankshaft Position (CKP) Sensor Signal
27 | YE | 633 | Camshaft Position (CMP) Sensor - Intake Signal
28-31 | -- | -- | Not Used
32 | BN | 5272 | Camshaft Position (CMP) Actuator Solenoid Valve - Intake Control Signal
33 | PU | 1666 | 5-Volt Reference
34 | -- | -- | Not Used
35 | OG | 496 | Knock Sensor Signal
36 | WH | 433 | 5-Volt Reference
37-38 | -- | -- | Not Used
39 | BK | 5276 | Low Reference
40 | BK | 5276 | Low Reference
41-44 | -- | -- | Not Used
45 | BK | 1869 | Low Reference
46 | D-BU | 424 | Ignition Coil C Control
47 | PU | 406 | Ignition Coil D Control
48 | -- | -- | Not Used
49 | YE | 131 | Low Reference
50 | L-BU/WH | 1747 | Fuel Injector 1
51 | L-GN/BK | 1745 | Fuel Injector 3
52 | BN | 1671 | Oxygen Sensor 2 Heater Low Control
53 | -- | -- | Not Used
54 | PU | 1667 | 5-Volt Reference
55 | WH | 1876 | Knock Sensor Signal
56 | PU | 427 | 5-Volt Reference
57-59 | -- | -- | Not Used
60 | L-BU | 426 | Low Reference
61 | -- | -- | Not Used
62 | BN | 808 | Low Reference
63 | -- | -- | Not Used
64 | WH | 808 | Low Reference
65 | -- | -- | Not Used
66 | WH | 452 | EVAP Canister Purge Solenoid Control
67 | -- | -- | Not Used
68 | L-BU | 581 | ETC Motor Close
69 | D-BU | 528 | ETC Motor Open
70 | RD | 423 | Ignition Coil A Control
71 | BK | 405 | Ignition Coil B Control
72 | GY | 53 | Oxygen Sensor 1 Heater Low Control
73 | BK | 50 | Ground

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: PED 12040753
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | -- | Engine Coolant Temperature (ECT) Sensor Signal
B | BN | -- | Low Reference

### Engine Coolant Temperature (ECT) Sensor (LDT/LXV)

#### Connector Part Information

- OEM: 967644-1
- Service: N/A
- Description: 2-Way F 0.64 MQS Series, Sealed (AMP) (BK)

#### Engine Coolant Temperature (ECT) Sensor (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 808 | Low Reference (WHB)
BN | 808 | Low Reference (-WHB)
2 | BN | 410 | Engine Coolant Temperature (ECT) Sensor Signal

### Engine Coolant Temperature (ECT) Sensor 2 (LDT/LXV)

#### Connector Part Information

- OEM: 0-936059-1
- Service: N/A
- Description: 2-Way F 0.64 MQS Series , Sealed Tyco (BK)

#### Engine Coolant Temperature (ECT) Sensor 2 (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 415 | Engine Coolant Temperature (ECT) Sensor Signal
2 | WH | 1977 | Low Reference

### Engine Coolant Thermostat (LDT/LXV)

#### Connector Part Information

- OEM: 1928403920
- Service: N/A
- Description: 2-Way F, Sealed Bosch (BK)

#### Engine Coolant Thermostat (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 465 | Engine Coolant Thermostat Signal
2 | OG/BK | 1732 | Ignition Voltage Reference

### Engine Oil Level (EOL) Sensor (NT4)

#### Connector Part Information

- OEM: 936059
- Service: N/A
- Description: 2-Way F SLD (2.8 mm) Series, Sealed AMP (BK)

#### Engine Oil Level (EOL) Sensor (NT4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 550 | Ground
2 | OG | 551 | Oil Level Sensor Signal

### Engine Oil Pressure (EOP) Switch (L95/LV8/LXT)

#### Connector Part Information

- OEM: ZPF 1-2
- Service: N/A
- Description: 1-Way F Sealed, Tyco (BK)

#### Engine Oil Pressure (EOP) Switch (L95/LV8/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 31 | Oil Pressure Indicator Control

### Engine Oil Pressure (EOP) Switch (LDT/LXV)

#### Connector Part Information

- OEM: MG 610278
- Service: N/A
- Description: 1-Way F SWP Series Sealed, KET (BK)

#### Engine Oil Pressure (EOP) Switch (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 31 | Oil Pressure Indicator Control

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LMU)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F Junior Power Timer Series, Sealed (AMP) (BK)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 428 | Low Reference
2 | OG | 1732 | 5-Volt Reference

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LDT)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F Junior Power Timer Series, Sealed (AMP) (BK)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LDT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 452 | Low Reference
2 | OG/BK | 1732 | Battery Positive Voltage

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LXV)

#### Connector Part Information

- OEM: 12124037
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 452 | Low Reference
B | OG/BK | 1732 | 5-Volt Reference

### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (L95/LV8/LXT)

#### Connector Part Information

- OEM: 12052643
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series, Sealed (RD)

#### Evaporative Emissions (EVAP) Canister Purge Solenoid Valve (L95/LV8/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 428 | EVAP Canister Purge Valve Solenoid Control
B | PK | 539 | Ignition 1 Voltage

### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LXV)

#### Connector Part Information

- OEM: 32229
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Evaporative Emissions (EVAP) Canister Vent Solenoid Valve (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | 1578 | Fuel Temperature Signal
B | RD/WH | 1340 | Battery Positive Voltage

### Evaporator Temperature Sensor (without LDT/WHB)

#### Connector Part Information

- OEM: MG 610392
- Service: N/A
- Description: 2-Way F Series, Sealed KET (WH)

#### Evaporator Temperature Sensor (without LDT/WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 732 | Evaporator Temperature Sensor Signal
2 | L-BU | 733 | Low Reference

### Exhaust Gas Recirculation (EGR) Valve (LMU)

#### Connector Part Information

- OEM: 12186139
- Service: 15306027
- Description: 5-Way F Metri-Pack 150 Series, Sealed (GY)

#### Exhaust Gas Recirculation (EGR) Valve (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 697 | EGR Valve Supply Voltage
B | BN | 808 | Low Reference
C | GY | 5763 | Exhaust Gas Recirculation Valve Sensor Signal
D | GY | 416 | 5-Volt Reference
E | OG | 1732 | 5-Volt Reference

### Exhaust Gas Recirculation (EGR) Valve (L95/LXT)

#### Connector Part Information

- OEM: 12186139
- Service: 15306027
- Description: 5-Way F Metri-Pack 150 Series, Sealed (GY)

#### Exhaust Gas Recirculation (EGR) Valve (L95/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 257 | EGR Solenoid High Control
B | BN/WH | 469 | Low Reference
C | GY | 5763 | Exhaust Gas Recirculation Valve Sensor Signal
D | PU | 719 | Low Reference
E | PK | 539 | Ignition 1 Voltage

### Fog Lamp - Left Front (T96)

#### Connector Part Information

- OEM: PB 625-02027
- Service: N/A
- Description: 2-Way F NMWP02F-B Series, Sealed KUM (BK)

#### Fog Lamp - Left Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 1769 | Fog Lamp Supply Voltage
2 | BK | 50 | Ground

### Fog Lamp - Right Front (T96)

#### Connector Part Information

- OEM: PB 625-02027
- Service: N/A
- Description: 2-Way F NMWP02F-B Series, Sealed KUM (BK)

#### Fog Lamp - Right Front (T96)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 1769 | Fog Lamp Supply Voltage
2 | BK | 250 | Ground

### Folding Mirror Unit (Notchback with Folding Mirrors)

#### Connector Part Information

- OEM: 173850
- Service: N/A
- Description: 8-Way (WH)

#### Folding Mirror Unit (Notchback with Folding Mirrors)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/BK | -- | Fold Signal
2 | -- | -- | Not Used
3 | RD/WH | -- | Battery Positive Voltage
4 | BN | -- | Ignition 2 Voltage
5 | BK | -- | Ground
6 | -- | -- | Not Used
7 | BN | -- | Folding Mirror Motor Feed
8 | OG | -- | Folding Mirror Motor Feed

### Fuel Injector 1 (LDT/LXV)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series, Sealed (GY)

#### Fuel Injector 1 (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1733 | Ignition 1 Voltage
B | L-BU/WH | 1747 | Fuel Injector 1 Control

### Fuel Injector 2 (LDT/LXV)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series, Sealed (GY)

#### Fuel Injector 2 (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1733 | Ignition 1 Voltage
B | WH | 1746 | Fuel Injector 2 Control

### Fuel Injector 3 (LDT/LXV)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series, Sealed (GY)

#### Fuel Injector 3 (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1733 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 3 Control

### Fuel Injector 4 (LDT/LXV)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series, Sealed (GY)

#### Fuel Injector 4 (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | OG | 1733 | Ignition 1 Voltage
B | BN | 1744 | Fuel Injector 4 Control

### Fuel Injector 1 (LMU/LV8)

#### Connector Part Information

- OEM: AMP 368468-1
- Service: N/A
- Description: 2-Way F Injector Plug Assembly, Tyco (BK)

#### Fuel Injector 1 (LMU/LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | L-BU/WH | 1747 | Fuel Injector 1 Control

### Fuel Injector 2 (LMU/LV8)

#### Connector Part Information

- OEM: AMP 368468-1
- Service: N/A
- Description: 2-Way F Injector Plug Assembly, Tyco (BK)

#### Fuel Injector 2 (LMU/LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | PK/BK | 1746 | Fuel Injector 2 Control

### Fuel Injector 3 (LMU/LV8)

#### Connector Part Information

- OEM: AMP 368468-1
- Service: N/A
- Description: 2-Way F Injector Plug Assembly, Tyco (BK)

#### Fuel Injector 3 (LMU/LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | L-GN/BK | 1745 | Fuel Injector 3 Control

### Fuel Injector 4 (LMU/LV8)

#### Connector Part Information

- OEM: AMP 368468-1
- Service: N/A
- Description: 2-Way F Injector Plug Assembly, Tyco (BK)

#### Fuel Injector 4 (LMU/LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 539 | Ignition 1 Voltage
2 | BN | 1744 | Fuel Injector 4 Control

### Fuel Injector 1 (L95/LXT with NN1)

#### Connector Part Information

- OEM: 15326181
- Service: 88988814
- Description: 2-Way F Micro-Pack 064 Series Sealed, (BK)

#### Fuel Injector 1 (L95/LXT with NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | L-BU/WH | 1747 | Fuel Injector 1 Control

### Fuel Injector 2 (L95/LXT with NN1)

#### Connector Part Information

- OEM: 15326181
- Service: 88988814
- Description: 2-Way F Micro-Pack 064 Series Sealed, (BK)

#### Fuel Injector 2 (L95/LXT with NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | PK/BK | 1746 | Fuel Injector 2 Control

### Fuel Injector 3 (L95/LXT with NN1)

#### Connector Part Information

- OEM: 15326181
- Service: 88988814
- Description: 2-Way F Micro-Pack 064 Series Sealed, (BK)

#### Fuel Injector 3 (L95/LXT with NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 3 Control

### Fuel Injector 4 (L95/LXT with NN1)

#### Connector Part Information

- OEM: 15326181
- Service: 88988814
- Description: 2-Way F Micro-Pack 064 Series Sealed, (BK)

#### Fuel Injector 4 (L95/LXT with NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | BN | 1744 | Fuel Injector 4 Control

### Fuel Injector 1 (L95/LXT without NN1)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed, (GY)

#### Fuel Injector 1 (L95/LXT without NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | L-BU/WH | 1747 | Fuel Injector 1 Control

### Fuel Injector 2 (L95/LXT without NN1)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed, (GY)

#### Fuel Injector 2 (L95/LXT without NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | PK/BK | 1746 | Fuel Injector 2 Control

### Fuel Injector 3 (L95/LXT without NN1)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed, (GY)

#### Fuel Injector 3 (L95/LXT without NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | L-GN/BK | 1745 | Fuel Injector 3 Control

### Fuel Injector 4 (L95/LXT without NN1)

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed, (GY)

#### Fuel Injector 4 (L95/LXT without NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage
B | BN | 1744 | Fuel Injector 4 Control

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 936159-1
- Service: N/A
- Description: 6-Way F Junior Power Timer Series, Sealed Tyco (WH)

#### Fuel Pump and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1936 | Fuel Level Sensor Signal
2 | BK | 850 | Ground
3 | BN | 1723 | Fuel Pump Supply Voltage
4 | PK | 539 | Ignition Voltage
5 | YE | 172 | Low Fuel Indicator Control
6 | L-BU | 1937 | Low Reference

### Fuel Tank Pressure (FTP) Sensor (NQU)

#### Connector Part Information

- OEM: 174357-2
- Service: N/A
- Description: 3-Way F J MK-II Series (AMP), Sealed (BK)

#### Fuel Tank Pressure (FTP) Sensor (NQU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 1937 | Low Reference
2 | BN/BK | 1030 | Fuel Tank Pressure Sensor Signal (TNK)
3 | RD/WH | 1031 | 5-Volt Reference (TNK)

### Fuel Tank Pressure (FTP) Sensor (WHB)

#### Connector Part Information

- OEM: 12059595
- Service: 12059595
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Fuel Tank Pressure (FTP) Sensor (WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 1937 | Low Reference
B | BN/BK | 1030 | Fuel Tank Pressure Sensor Signal
C | RD/WH | 1031 | 5-Volt Reference

### Generator (L95/LV8/LXT)

#### Connector Part Information

- OEM: 12186568
- Service: N/A
- Description: 4-Way F Metri-Pack 150 Series, Sealed (BK)

#### Generator (L95/LV8/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | BN | 25 | Charge Indicator Signal
C | PK | 1739 | Ignition 1 Voltage
D | -- | -- | Not Used

### Generator (LDT/LXV)

#### Connector Part Information

- OEM: 12040753
- Service:12040753
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Generator (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-BU | 25 | Charge Indicator Signal (-WHB)
D-GN | 225 | Generator Turn On Signa (WHB)
B | PK | 539 | Ignition 1 Voltage (-WHB)
OG | 23 | Generator Field Duty Cycle Signal (WHB)

### Generator (LMU)

#### Connector Part Information

- OEM: 12040753
- Service:12040753
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### Generator (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 25 | Charge Indicator Signal
B | PK | 1739 | Ignition 1 Voltage

### Hazard Warning Switch

#### Connector Part Information

- OEM: MG 612234-5
- Service: N/A
- Description: 10-Way F ASC Series, KET (BK)

#### Hazard Warning Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | D-GN | 230 | Instrument Panel Lamps Dimming Control
3 | BN/WH | 309 | Illumination Supply Voltage
4 | -- | -- | Not Used
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
7 | L-BU | 1508 | Turn Signal Switch Signal
8 | RD/WH | 1440 | Battery Positive Voltage
9 | PU | 16 | Turn Signal Flasher Signal
PU | 16 | Turn Signal Flasher Signal
10 | PK | 339 | Ignition 1 Voltage

### Headlamp - Left

#### Connector Part Information

- OEM: OPES-PH2
- Service: N/A
- Description: 3-Way Connector F (WH)

#### Headlamp - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 312 | Left Headlamp Low Beam Supply Voltage
2 | L-GN/BK | 311 | Left Headlamp High Beam Supply Voltage
3 | BK | 50 | Ground

### Headlamp - Right

#### Connector Part Information

- OEM: OPES-PH2
- Service: N/A
- Description: 3-Way Connector F (WH)

#### Headlamp - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 712 | Right Headlamp Low Beam Supply Voltage
2 | D-GN/WH | 711 | Right Headlamp High Beam Supply Voltage
3 | BK | 250 | Ground

### Headlamp Leveling Actuator - Left (T84)

#### Connector Part Information

- OEM: MG 641234-5
- Service: N/A
- Description: 3-Way F SSD Series, Sealed KET (BK)

#### Headlamp Leveling Actuator - Left (T84)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | D-GN | 189 | Headlamp Leveling Motor Feed
3 | PU | 709 | Park Lamp Feed - Left

### Headlamp Leveling Actuator - Right (T84)

#### Connector Part Information

- OEM: MG 641234-5
- Service: N/A
- Description: 3-Way F SSD Series, Sealed KET (BK)

#### Headlamp Leveling Actuator - Right (T84)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | D-GN | 189 | Headlamp Leveling Motor Feed
3 | BN/WH | 309 | Park Lamp Feed - Right

### Headlamp Leveling Switch (Except North America)

#### Connector Part Information

- OEM: 5557-06R
- Service: N/A
- Description: 6-Way Mini Fit Conn. Rec. Housing (WH)

#### Headlamp Leveling Switch (Except North America)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | -- | Right Park Lamp Supply Voltage
2 | L-GN/BK | -- | Headlamp Low Beam Supply Voltage
3 | D-GN | -- | Headlamp Leveling Motor Supply Voltage
4 | BN/WH | -- | Ground
5 | -- | -- | Not Used
6 | BK | -- | Ground

### Headlamp Switch

#### Connector Part Information

- OEM: 5559-06P
- Service: N/A
- Description: 6-Way Mini-Fit Series, MLX (NA)

#### Headlamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 450 | Ground
2 | BK/WH | 1352 | Headlamp Control
3 | BK/WH | 450 | Ground
4 | -- | -- | Not Used
5 | D-GN/WH | 1317 | Fog Lamp Relay Control
6 | L-BU | 74 | Park Lamp Switch Signal

### Heated Oxygen Sensor (HO2S) 1 (LTD/LXV)

#### Connector Part Information

- OEM: 174257-2
- Service: N/A
- Description: 4-Way F 070 J MK-2 Series, Sealed Tyco (BK)

#### Heated Oxygen Sensor (HO2S) 1 (LTD/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1665 | Heated Oxygen Sensor (HO2S) 1 Signal
2 | OG/BK | 1732 | 5-Volt Reference - Ignition
3 | WH | 428 | Heated Oxygen Sensor (HO2S) 1 Signal Return
4 | GY | 53 | Low Reference

### Heated Oxygen Sensor (HO2S) 1 (L95/LXT without NN1)

#### Connector Part Information

- OEM: 174257-2
- Service: N/A
- Description: 4-Way F 070 J MK-2 Series, Sealed Tyco (BK)

#### Heated Oxygen Sensor (HO2S) 1 (L95/LXT without NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 1665 | Heated Oxygen Sensor (HO2S) 1 Signal
2 | BK | 50 | Ground
3 | D-GN/WH | 428 | Heated Oxygen Sensor (HO2S) 1 Signal Return
4 | PK | 539 | Ignition 1 Voltage

### Heated Oxygen Sensor (HO2S) 1 (L95/LXT with NN1)

#### Connector Part Information

- OEM: 12162144
- Service: 12102741
- Description: 4-Way F Metri-Pack 150 Series, Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 1 (L95/LXT with NN1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-GN/WH | 428 | Heated Oxygen Sensor (HO2S) 1 Signal Return
B | BN | 1665 | Heated Oxygen Sensor (HO2S) 1 Signal
C | BK | 50 | Ground
D | PK | 539 | Ignition 1 Voltage

### Heated Oxygen Sensor (HO2S) 1 (LMU)

#### Connector Part Information

- OEM: 625-04027
- Service: N/A
- Description: 4-Way F NMWP04F-B Series, Sealed Mitsubishi (BK)

#### Heated Oxygen Sensor (HO2S) 1 (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-CN/WH | 1665 | Heated Oxygen Sensor (HO2S) 1 Signal
2 | PK/BK | 3113 | Low Reference
3 | BN | 469 | Low Reference
4 | OG | 1732 | 5-Volt Reference

### Heated Oxygen Sensor (HO2S) 2 (L95/LXT/LDT/LXV with NOU/NT4/NU2)

#### Connector Part Information

- OEM: 625-04027
- Service: N/A
- Description: 4-Way F NMWP04F-B Series (Mitsubishi), Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 2 (L95/LXT/LDT/LXV with NOU/NT4/NU2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 413 | Heated Oxygen Sensor (HO2S) 2 Signal
2 | PK/BK | 1739 | Ignition 1 Voltage
3 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
4 | BN | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control

### Heated Oxygen Sensor (HO2S) 2 (L95/LV8/LXT with NT3)

#### Connector Part Information

- OEM: 12162144
- Service: 12102741
- Description: 4-Way F Metri-Pack 150 Series, Sealed (BK)

#### Heated Oxygen Sensor (HO2S) 2 (L95/LV8/LXT with NT3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
B | BN | 413 | Heated Oxygen Sensor (HO2S) 2 Signal
C | BN | 1671 | Heated Oxygen Sensor (HO2S) 2 Heater Control
D | PK/BK | 1739 | Ignition 1 Voltage

### Heated Seat Element - Driver Cushion (C37)

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (NA)

#### Heated Seat Element - Driver Cushion (C37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | 1501 | Driver Heated Seat High/Low Signal
2 | BK | 450 | Ground

### Hood Ajar Switch

#### Connector Part Information

- OEM: 1743695-2
- Service: N/A
- Description: 2-Way F Mark-II Series, Sealed Tyco (BK)

#### Hood Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK/BK | 109 | Hood Ajar Switch Signal
2 | RD/WH | 440 | Battery Positive Voltage

### Horn - Left

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way GT 150 Series, Sealed (GY)

#### Horn - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 28 | Horn Relay Control
B | BK | 250 | Ground

### Horn - Right (Hatchback)

#### Connector Part Information

- OEM: 15419715
- Service: See Catalog
- Description: 2-Way GT 150 Series, Sealed (GY)

#### Horn - Right (Hatchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 250 | Ground
B | BN | 28 | Horn Relay Control

### HVAC Control Module X1 (C68)

#### Connector Part Information

- OEM: 179057-6
- Service: N/A
- Description: 20-Way F 040II/070II MK-II Series, Tyco (GY)

#### HVAC Control Module X1 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | L-GN | 817 | Vehicle Speed Signal
3 | YE/BK | 92 | Windshield Wiper Motor High Speed
4-5 | -- | -- | Not Used
6 | RD/YE | -- | PTC On
7 | -- | -- | Not Used
8 | WH/BK | -- | Inside Air Temperature Sensor Signal
9 | D-GN/YE | -- | Ambient Air Temperature Sensor Signal
10 | BK/YE | -- | Intake Sensor Signal
11 | YE/D-GN | 762 | A/C Request Signal
12-14 | -- | -- | Not Used
15 | D-BU | -- | Water Sensor Signal
16 | D-GN/RD | -- | Coolant Temperature Sensor Signal
17-18 | -- | -- | Not Used
19 | YE/RD | -- | Sunload Sensor Signal
20 | D-BU/WH | 735 | Low Reference

### HVAC Control Module X2 (C68)

#### Connector Part Information

- OEM: 179054-6
- Service: N/A
- Description: 16-Way F 040 MK-II Series, Tyco (GY)

#### HVAC Control Module X2 (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YE/WH | 239 | Ignition 1 Voltage
3 | WH/RD | 540 | Battery Positive Voltage
4 | D-GN/BK | 230 | Instrument Panel Lamps Dimming Control
5 | D-GN/WH | 309 | Right Park Lamp Supply Voltage
6 | BN/RD | 193 | Rear Defog Relay Control
7 | -- | -- | Not Used
8 | RD/D-BU | -- | VACTR (+)
9 | -- | -- | Not Used
10 | D-BU/YE | -- | Blower Motor Speed Control
11 | D-BU/RD | -- | Blower Feedback
12 | RD/WH | -- | Ignition Voltage
13 | BK | -- | Ground
14-15 | -- | -- | Not Used
16 | D-GN | -- | Fan Switch ON

### HVAC Control Module (C60)

#### Connector Part Information

- OEM: MG 610404
- Service: N/A
- Description: 10-Way F 090 II Series (WH)

#### HVAC Control Module (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 239 | Ignition 1 Voltage
2 | BK | 650 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | D-GN | 230 | Instrument Panel Lamps Dimming Control
5 | OG | 362 | Upper Mode Valve Solenoid Control
6 | D-GN/WH | 762 | A/C Request Signal
7 | PK/WH | 1648 | Recirculation Door Control A (C60)
8 | L-GN/BK | 1647 | Recirculation Door Control B (C60)
9 | L-BU | 292 | Rear Defog Switch Signal (DWT)
WH | 193 | Rear Defog Relay Control (-DWT)
10 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage (DWT)
RD/WH | 540 | Battery Positive Voltage (-DWT)

### I/P Compartment Lamp Switch (C99)

#### Connector Part Information

- OEM: AK5306
- Service: N/A
- Description: 2-Way F Connector

#### I/P Compartment Lamp Switch (C99)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 1340 | Ignition 1 Voltage
2 | PU | 175 | Glove Box Lamp Control

### I/P Dimmer Switch

#### Connector Part Information

- OEM: MG610045
- Service: N/A
- Description: 3-Way F 250 Series (NA)

#### I/P Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 230 | Instrument Panel Lamps Dimming Control
2 | BK | 450 | Ground
3 | BN/WH | 309 | Right Park Lamp Supply Voltage

### Ignition Control Module (ICM) (LDT/LXV)

#### Connector Part Information

- OEM: 15317367
- Service: 15306317
- Description: 7-Way F GT 150 Series, Sealed (BK)

#### Ignition Control Module (ICM) (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | PK | 539 | Ignition 1 Voltage (WHB)
OG | 1733 | Ignition 1 Voltage (-WHB)
B | BK | 51 | Ground
C | YE | 131 | Low Reference (WHB)
D | RD | 423 | IC Timing Control
E | PU | 406 | IC Timing Control [B]
F | BK | 405 | Lower Air Temperature Sensor Signal
G | D-BU | 424 | IC Timing Signal

### Ignition Control Module (ICM) (without LDT/LXV)

#### Connector Part Information

- OEM: 12059595
- Service: 88986451
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Ignition Control Module (ICM) (without LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | WH | 423 | Ignition Coil (IC) Timing Control 2 and 3
B | PK | 539 | Ignition 1 Voltage (L95/LV8/LXT)
PK | 739 | Ignition 1 Voltage (LMU)
C | OG | 406 | Ignition Coil (IC) Timing Control 1 and 4

### Ignition Key Alarm Switch (without WHB)

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Ignition Key Alarm Switch (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 540 | Battery Positive Voltage
2 | L-GN | 80 | Key In Ignition Switch Signal

### Ignition Key Illumination Lamp (without WHB)

#### Connector Part Information

- OEM: MG 610207
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series (WH)

#### Ignition Key Illumination Lamp (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 540 | Battery Positive Voltage
2 | D-GN/WH | 900 | Key Illumination Control

### Ignition Lock Cylinder Control Actuator (WHB with MLQ)

#### Connector Part Information

- OEM: 15332129
- Service: 15306425
- Description: 2-Way F GT 150 Series, (BK)

#### Ignition Lock Cylinder Control Actuator (WHB with MLQ)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN | 1076 | Ignition Key Cylinder Solenoid Lock Inhibit
B | BK | 450 | Ground

### Ignition Relay (with WHB)

#### Connector Part Information

- OEM: AK 36907
- Service: N/A
- Description: 9-Way Metri-Pack 150 Series (BN)

#### Ignition Relay (with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not used
2 | BK | 450 | Ground
3 | -- | -- | Not used
4 | RD/BK | 142 | Battery Positive Voltage
5 | -- | -- | Not used
6 | L-BU | 7003 | Ignition Relay Output
7 | -- | -- | Not used
8 | PK | 3 | Ignition 1 Voltage
9 | -- | -- | Not used

### Ignition Switch (with WHB)

#### Connector Part Information

- OEM: IL-AG5-6S S3C1
- Service: N/A
- Description: 6-Way F (GN)

#### Ignition Switch (with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 7009 | Ignition 0 Voltage - Acc/Run
2 | RD/WH | 240 | Battery Positive Voltage
3 | OG | 7004 | Ignition 1 Voltage - Run/Crank
4 | RD/BK | 7008 | Ignition 3 Voltage - Run
5 | BN | 7007 | Vehicle Wake Up Signal
6 | -- | -- | Not Used

### Ignition Switch (without WHB)

#### Connector Part Information

- OEM: MG 650887
- Service: N/A
- Description: 6-Way F 250 III Series, KET (BK)

#### Ignition Switch (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 300 | Ignition 3 Voltage
2 | RD/BK | 42 | Battery Positive Voltage
3 | YE | 5 | Crank Voltage
4 | PK | 3 | Ignition 1 Voltage
5 | RD/BK | 142 | Battery Positive Voltage
6 | BN | 4 | Accessory Voltage

### Inflatable Restraint Front End Sensor - Left (WHB)

#### Connector Part Information

- OEM: 54390240
- Service: N/A
- Description: 2-Way F 64 Series, FCI (GY)

#### Inflatable Restraint Front End Sensor - Left (WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE/BK | 6169 | Front Discriminating Sensor - Left - Low
2 | YE | 6168 | Front Discriminating Sensor - Left - High

### Inflatable Restraint Front End Sensor - Right (WHB)

#### Connector Part Information

- OEM: 54390240
- Service: N/A
- Description: 2-Way F 64 Series, FCI (GY)

#### Inflatable Restraint Front End Sensor - Right (WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 6777 | Front Discriminating Sensor - Left - Low
2 | BN/WH | 6776 | Front Discriminating Sensor - Left - High

### Inflatable Restraint Front Passanger Presence System (PPS) Sensor (C98)

#### Connector Part Information

- OEM: 174357-2
- Service: N/A
- Description: 3-Way 070 Econoseal Series, Sealed Tyco (BK)

#### Inflatable Restraint Front Passanger Presence System (PPS) Sensor (C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 1739 | Ignition 1 Voltage
2 | BN/WH | 5060 | Low Speed GMLAN Serial Data
3 | BK | 250 | Ground

### Inflatable Restraint I/P Module (WHB with C98)

#### Connector Part Information

- OEM: 54550400
- Service: N/A
- Description: 4-Way F 2.8 Series, FCI (YE)

#### Inflatable Restraint I/P Module (WHB with C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 3026 | I/P Module - Stage 2 - Low Control
2 | GY | 3027 | I/P Module - Stage 2 - High Control
3 | WH/BK | 1403 | I/P Module - High Control
4 | D-GN/WH | 1404 | I/P Module - Low Control

### Inflatable Restraint I/P Module (AK5)

#### Connector Part Information

- OEM: 60201724
- Service: N/A
- Description: 2-Way 2.8 Series, FCI (YE)

#### Inflatable Restraint I/P Module (AK5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH/D-GN | 1403 | I/P Module - High Control
2 | D-GN/WH | 1404 | I/P Module - Low Control

### Inflatable Restraint I/P Module Disable Switch (C99)

#### Connector Part Information

- OEM: 54550400
- Service: N/A
- Description: 8-Way F 64 MQS Series, Tyco (YE)

#### Inflatable Restraint I/P Module Disable Switch (C99)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 1358 | DIC Switch Signal
2 | BK | 250 | Ground
3 | D-GN | 2308 | Passenger Air Bag Off Indicator Control
4 | PU | 175 | Glove Box Lamp Control
5 | BK | 250 | Ground
6-8 | -- | -- | Not used

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (with WHB)

#### Connector Part Information

- OEM: 8-0638595-5
- Service: N/A
- Description: 60-Way 64 GET Series, Sealed Tyco (YE)

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | BK/WH | 5060 | Low Speed GMLAN Serial Data
3 | -- | -- | Not Used
4 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control (C98)
OG/WH | 2119 | Seat Belt Pretensioner - Left - Low Control (-C98)
5 | WH | 3023 | Steering Wheel Module - Stage2 - High Control (C98)
BN/WH | 2118 | Seat Belt Pretensioner - Left - High Control (-C98)
6 | GY | 3027 | I/P Module - Stage 2 - High Control (C98)
L-GN | 2116 | Seat Belt Pretensioner - Right - High Control (-C98)
7 | PU | 3026 | I/P Module - Stage 2 - Low Control (C98)
OG | 2117 | Seat Belt Pretensioner - Right - Low Control (-C98)
8 | D-GN | 348 | Steering Wheel Module - Low Control
9 | WH | 347 | Steering Wheel Module - High Control
10 | WH/BK | 1403 | I/P Module - High Control
11 | D-GN/WH | 1404 | I/P Module - Low Control
12 | BN | 2106 | Side Impact Module - Left - Low Control
13 | D-GN | 2105 | Side Impact Module - Left - High Control
14 | GY | 2103 | Side Impact Module - Right - High Control
15 | D-BU | 2104 | Side Impact Module - Right - Low Control
16 | OG/WH | 2119 | Seat Belt Pretensioner - Left - Low Control (C98)
17 | BN/WH | 2118 | Seat Belt Pretensioner - Left - High Control (C98)
18 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control (C98)
19 | OG | 2117 | Seat Belt Pretensioner - Right - Low Control (C98)
20-30 | -- | -- | Not Used
31 | RD/WH | 240 | Battery Positive Voltage
32 | PK | 139 | Ignition 1 Voltage
33-35 | -- | -- | Not Used
36 | PU | 6168 | Middle Front Impact Sensing Module Supply Voltage
37 | BK | 6776 | Middle Front Impact Sensing Module (2) Supply Voltage
38 | RD | 6169 | Middle Front Impact Sensing Module Signal
39 | D-GN | 6777 | Middle Front Impact Sensing Module (2) Signal
40 | GY/BK | 6621 | Left Middle Side Impact Sensing Module Low Reference
41 | L-GN/WH | 6625 | Right Middle Side Impact Sensing Module Low Reference
42 | D-GN/WH | 6620 | Left Middle Side Impact Sensing Module Signal
43 | L-BU/BK | 6624 | Right Middle Side Impact Sensing Module Signal
44-58 | -- | -- | Not Used
59 | BN/WH | 238 | Seat Belt Switch - Left
60 | -- | -- | Not Used

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (without WHB)

#### Connector Part Information

- OEM: 1417642
- Service: N/A
- Description: 75-Way, Tyco

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-25 | -- | -- | Not Used
26 | PK | 139 | Ignition Voltage
27 | BN | 358 | SIR Indicator Lamp Control
28 | BK | 250 | Ground
29 | D-GN | 348 | Steering Wheel Module - Low Control
30 | WH | 347 | Steering Wheel Module - High Control
31 | WH/BK | 1403 | I/P Module - High Control
32 | GN/WH | 1404 | I/P Module - Low Control
33 | OG/WH | 2119 | Seat Belt Pretensioner - Left - Low Control (LHD)
OG | 2117 | Seat Belt Pretensioner - Right - Low Control (RHD)
34 | BN/WH | 2118 | Seat Belt Pretensioner - Left - High Control (LHD)
L-GN | 2116 | Seat Belt Pretensioner - Right - High Control (RHD)
35 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control (LHD)
BN/WH | 2118 | Seat Belt Pretensioner - Left - High Control (RHD)
36 | OG | 2117 | Seat Belt Pretensioner - Right - Low Control (LHD)
OG/WH | 2119 | Seat Belt Pretensioner - Left - Low Control (RHD)
37 | BN | 2106 | Side Impact Module - Left - Low Control (LHD)
D-BU | 2104 | Side Impact Module - Right - Low Control (RHD)
38 | D-GN | 2105 | Side Impact Module - Left - High Control (LHD)
GY | 2103 | Side Impact Module - Right - High Control (RHD)
39 | GY | 2103 | Side Impact Module - Right - High Control (LHD)
D-GN | 2105 | Side Impact Module - Left - High Control (RHD)
40 | D-BU | 2104 | Side Impact Module - Right - Low Control (LHD)
BN | 2106 | Side Impact Module - Left - Low Control (RHD)
41-51 | -- | -- | Not Used
52 | YE | 234 | Seat Belt Indicator Control
53 | -- | -- | Not Used
54 | L-BU | 327 | SIR Serial Data
55 | -- | -- | Not Used
56 | D-GN/WH | 1358 | DIC Switch Signal
57 | L-BU | 2221 | Vehicle Speed Sensor Signal
58 | -- | -- | Not Used
59 | L-GN | 1845 | Chime Control
60 | D-GN | 2308 | Passenger Air Bag Off Indicator Control
61 | BN/WH | 238 | Seat Belt Switch Signal
62-67 | -- | -- | Not Used
68 | L-GN/WH | 6625 | Right Middle Side Impact Sensing Module Low Reference (LHD)
GY/BK | 6621 | Left Middle Side Impact Sensing Module Low Reference (RHD)
69 | L-BU/BK | 6624 | Right Middle Side Impact Sensing Module Signal (LHD)
D-GN/WH | 6620 | Left Middle Side Impact Sensing Module Signal (RHD)
70 | D-GN/WH | 6620 | Left Middle Side Impact Sensing Module Signal (LHD)
L-BU/BK | 6624 | Right Middle Side Impact Sensing Module Signal (RHD)
71 | GY/BK | 6621 | Left Middle Side Impact Sensing Module Low Reference (LHD)
L-GN/WH | 6625 | Right Middle Side Impact Sensing Module Low Reference (RHD)
72-75 | -- | -- | Not Used

### Inflatable Restraint Side Impact Module - Left (AJ7)

#### Connector Part Information

- OEM: 7C83-5524-70
- Service: N/A
- Description: 2-Way F 040 III Series, Sealed Yazaki (YE)

#### Inflatable Restraint Side Impact Module - Left (AJ7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 2106 | Side Impact Module - Left - Low Control
2 | D-GN | 2105 | Side Impact Module - Left - High Control

### Inflatable Restraint Side Impact Module - Right (AJ7)

#### Connector Part Information

- OEM: 7C83-5524-70
- Service: N/A
- Description: 2-Way F 040 III Series, Sealed Yazaki (YE)

#### Inflatable Restraint Side Impact Module - Right (AJ7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 2104 | Side Impact Module - Right - Low Control
2 | GY | 2103 | Side Impact Module - Right - High Control

### Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 with C98)

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Series Sealed, Delphi (YE)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 with C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | 6621 | Left Side Impact Sensor - Low
2 | D-GN/WH | 6620 | Left Side Impact Sensor - High

### Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 without C98)

#### Connector Part Information

- OEM: 7283-6502-50
- Service: N/A
- Description: 2-Way F 040 III Series Sealed, Yazaki (OG)

#### Inflatable Restraint Side Impact Sensor (SIS) - Left (AJ7 without C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY/BK | 6621 | Left Side Impact Sensor - Low
2 | D-GN/WH | 6620 | Left Side Impact Sensor - High

### Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 with C98)

#### Connector Part Information

- OEM: 15356723
- Service: 15306439
- Description: 2-Way F GT 150 Series Sealed, Delphi (YE)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 with C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | 6625 | Right Side Impact Sensor - Low
2 | L-BU/BK | 6624 | Right Side Impact Sensor - High

### Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 without C98)

#### Connector Part Information

- OEM: 7283-6502-50
- Service: N/A
- Description: 2-Way F 040 III Series Sealed (OG)

#### Inflatable Restraint Side Impact Sensor (SIS) - Right (AJ7 without C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN/WH | 6625 | Right Side Impact Sensor - Low
2 | L-BU/BK | 6624 | Right Side Impact Sensor - High

### Inflatable Restraint Steering Wheel Module (WHB with C98)

#### Connector Part Information

- OEM: 0-1411142-1
- Service: N/A
- Description: 4-Way F Socet, Tyco (YE)

#### Inflatable Restraint Steering Wheel Module (WHB with C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 348 | Steering Wheel Module - Low Control
2 | WH | 347 | Steering Wheel Module - High Control
3 | PK | 3022 | Steering Wheel Module - Stage2 - Low Control
4 | WH | 3023 | Steering Wheel Module - Stage2 - High Control

### Inflatable Restraint Steering Wheel Module (AJ3 without C98)

#### Connector Part Information

- OEM: 1393433-8
- Service: N/A
- Description: 2-Way F 070 Series, Tyco (YE)

#### Inflatable Restraint Steering Wheel Module (AJ3 without C98)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 348 | Steering Wheel Module - Low Control
2 | WH | 347 | Steering Wheel Module - High Control

### Inflatable Restraint Steering Wheel Module Coil (AJ3 with UV8/WHB)

#### Connector Part Information

- OEM: MG 651050
- Service: N/A
- Description: 8-Way F 090-II Series, KET (WH)

#### Inflatable Restraint Steering Wheel Module Coil (AJ3 with UV8/WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 1796 | Steering Wheel Controls Signal
2 | BN/WH | 372 | Remote Radio Audio Output
3 | D-GN | 29 | Horn Control
4 | D-GN | 652 | Chime Module Bit2 Signal (UV8)
GY | 397 | Cruise Control On Switch Signal (K34)
5 | L-BU | 661 | Right Courtesy Lamp Control (UV8)
6 | L-BU | 662 | Radio Clock Signal (UV8)
7 | D-BU/WH | 653 | Chime Module Bit1 Signal (UV8)
BN | 717 | Cruise Power Output (K34)
8 | -- | -- | Not Used

### Instrument Panel Cluster (IPC) X1 (with WHB)

#### Connector Part Information

- OEM: 1534222-1
- Service: N/A
- Description: 32-Way F MQS Series, Tyco (GN)

#### Instrument Panel Cluster (IPC) X1 (with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 7007 | Vehicle Wake Up Signal
2 | RD/BK | 7008 | Ignition 3 Voltage - Run
3 | D-BU | 7002 | Run Relay Out
4 | BN/WH | 309 | Right Park Lamp Supply Voltage
5 | D-GN | 230 | Instrument Panel Lamps Dimming Control
6 | D-GN | 5060 | Low Speed GMLAN Serial Data
7-8 | -- | -- | Not Used
9 | OG/BK | 434 | Neutral Safety Switch Signal
10 | BN/WH | 238 | Seat Belt Switch - Left (-AJ3)
11 | -- | -- | Not Used
12 | PU | 1807 | Class 2 Serial Data (Primary)
13 | D-GN | 1807 | Class 2 Serial Data (Primary)
14 | YE | 710 | Class 2 Serial Data
15 | YE/BK | 710 | Class 2 Serial Data
16 | BK | 450 | Ground
17 | L-GN | 7009 | Ignition 0 Voltage - Acc/Run
18 | OG | 7004 | Ignition 1 Voltage - Run/Crank
19 | YE | 111 | Hazard Switch Signal
20 | PU | 638 | Power Window Motor Driver Down Control
21 | L-BU | 7003 | DLIS Relay Control
22 | -- | -- | Not Used
23 | RD/WH | 340 | Battery Positive Voltage
24 | RD/WH | 1340 | Battery Positive Voltage
25 | -- | -- | Not Used
26 | YE | 61 | Outside Ambient Air Temperature Sensor Signal
27 | PU | 878 | Cruise Control Release Signal
28 | D-BU | 7001 | GMLAN
29 | D-GN/WH | 762 | A/C Request Signal
30 | GY | 397 | Cruise Control On Switch Signal
31 | BN | 717 | Cruise Power Output
32 | BK | 650 | Ground

### Instrument Panel Cluster (IPC) X2 (with WHB)

#### Connector Part Information

- OEM: 1534222-2
- Service: N/A
- Description: 32-Way F MQS Series, Tyco (BU)

#### Instrument Panel Cluster (IPC) X2 (with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 749 | Security Indicator Control
2 | BN | 25 | Charge Indicator Signal
3 | L-GN | 80 | Key In Ignition Switch Signal
4 | D-GN/WH | 817 | Vehicle Speed Signal
5 | L-GN | 1845 | Chime Control
6 | -- | -- | Not Used
7 | GY/BK | 1357 | Instrument Panel Lamp Control
8 | D-GN/WH | 1358 | DIC Switch Signal
9 | BN | 7020 | Remote Control Door Reciver Signal
10 | -- | -- | Not Used
11 | YE | 1769 | Fog Lamp Switch Supply Voltage
12 | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
13 | L-GN | 867 | ABS Indicator Failure Control
14 | -- | -- | Not Used
15 | BK | 50 | Ground
16 | BK | 650 | Ground
17 | -- | -- | Not Used
18 | BN/WH | 419 | MIL Control
19 | BN/WH | 33 | Brake Warning Indicator Control
20 | -- | -- | Not Used
21 | YE | 172 | Low Fuel Indicator Control
22 | WH | 629 | High Beam Indicator - Feed - DRL
23 | WH | 156 | Courtesy Lamp Low Control
24 | YE | 712 | Left Headlamp Low Beam Supply Voltage
25 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
26 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
27-28 | -- | -- | Not used
29 | PU | 156 | Courtesy Lamp Low Control Signal
30-31 | -- | -- | Not used
32 | BK | 650 | Ground

### Instrument Panel Cluster (IPC) X1 (without WHB)

#### Connector Part Information

- OEM: 1565380-1
- Service: N/A
- Description: 28-Way F 025 Series, Tyco (NA)

#### Instrument Panel Cluster (IPC) X1 (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 1769 | Fog Lamp Switch Supply Voltage (T96)
2 | L-GN | 867 | ABS Indicator Failure Control
3 | -- | -- | Not Used
4 | YE | 1481 | Transmission Auxiliary Hold Signal (MLQ)
5 | PK | 239 | Ignition 1 Voltage
6 | BK | 450 | Ground
7-9 | -- | -- | Not Used
10 | YE | 61 | Ambient Temperature Sensor Signal (C68)
11 | BN/WH | 309 | Right Park Lamp Supply Voltage
12 | D-GN | 230 | Instrument Panel Lamps Dimming Control
13 | BN | 31 | Oil Pressure Indicator Control
14 | BN/WH | 419 | MIL Control
15-18 | -- | -- | Not Used
19 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
20 | D-GN | 135 | ECT Sensor Gauge Signal
21 | WH | 156 | Courtesy Lamp Low Control
22 | YE | 172 | Low Fuel Indicator Control
23 | YE | 712 | Left Headlamp Low Beam Supply Voltage
24 | RD/WH | 1340 | Battery Positive Voltage
25 | -- | -- | Not Used
26 | BN | 25 | Charge Indicator Control
27 | WH | 121 | Engine Speed Signal
28 | BK | 50 | Ground

### Instrument Panel Cluster (IPC) X2 (without WHB)

#### Connector Part Information

- OEM: 1318386-1
- Service: N/A
- Description: 16-Way F 025 Series, Tyco (NA)

#### Instrument Panel Cluster (IPC) X2 (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 33 | Brake Warning Indicator Control
2-4 | -- | -- | Not Used
5 | BN | 358 | Air Bag Indicator Control
6 | OG | 122 | Roof Off-Road Lamps Supply Voltage 1
7 | -- | -- | Not Used
8 | BK | 450 | Ground
9 | OG | 551 | Oil Level Sensor
10 | YE | 234 | Seat Belt Indicator Control (AJ3)
BN/WH | 238 | Seat Belt Indicator Control (-AJ3)
11 | PU/WH | 822 | VSS Low Signal (T44)
12 | D-GN/WH | 817 | Vehicle Speed Signal
13 | -- | -- | Not Used
14 | L-BU | 2221 | Vehicle Speed Sensor Signal
15 | PU | 30 | Fuel Level Sensor Signal
16 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage

### Intake Air Temperature (IAT) Sensor (without WHB)

#### Connector Part Information

- OEM: AMP 85202-1
- Service: N/A
- Description: 2-Way Junior Power Timer Series, Sealed Tyco (BK)

#### Intake Air Temperature (IAT) Sensor (without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 6118 | Intake Air Temperature (IAT) Sensor Signal
2 | BN | 808 | Low Reference

### Intake Air Temperature (IAT) Sensor - HVAC (C68)

#### Connector Part Information

- OEM: MG 610392
- Service: N/A
- Description: 2-Way M

#### Intake Air Temperature (IAT) Sensor - HVAC (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK/YE | -- | Intake Sensor Signal
2 | D-BU/WH | -- | Low Reference

### Knock Sensor (KS) (LDT/LXV)

#### Connector Part Information

- OEM: 85202-1
- Service: N/A
- Description: 2-Way F JPT Series, Sealed Tyco (BK)

#### Knock Sensor (KS) (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 496 | Knock Sensor (KS) Signal
2 | WH | 1876 | Low Reference

### Knock Sensor (KS) (LMU)

#### Connector Part Information

- OEM: AMP 368215-1
- Service: N/A
- Description: 3-Way F JPT Series, Sealed Tyco (GY)

#### Knock Sensor (KS) (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 496 | Knock Sensor (KS) Signal
2 | WH | 1876 | Low Reference
3 | BK/WH | 51 | Shield Ground

### Knock Sensor (KS) (L95/LV8/LXT)

#### Connector Part Information

- OEM: AMP 368215-1
- Service: N/A
- Description: 3-Way F JPT Series, Sealed Tyco (GY)

#### Knock Sensor (KS) (L95/LV8/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 496 | Knock Sensor (KS) Signal
2 | BN | 808 | Low Reference
3 | BN | 808 | Shield Ground

### Lamp Driver Module

#### Connector Part Information

- OEM: AK 368530-1
- Service: N/A
- Description: 6-Way F Econoseal J-Mark II (BK)

#### Lamp Driver Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | RD | 242 | Battery Positive Voltage
3 | BN | 33 | Brake Warning Indicator Control
4 | -- | -- | Not Used
5 | GY | 875 | Base Brake Failure Signal
6 | L-GN | 867 | ABS Failure Indicator Signal

### License Lamp

#### Connector Part Information

- OEM: MG 630679
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### License Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 850 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage

### Manifold Absolute Pressure (MAP) Sensor (LDT/LXV)

#### Connector Part Information

- OEM: 1928403966
- Service: 88988583
- Description: 3-Way F Kompakt 280 Series, Sealed (Bosch) (BK)

#### Manifold Absolute Pressure (MAP) Sensor (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 433 | 5-Volt Reference
2 | BN | 808 | Low Reference
3 | L-BU | 469 | Manifold Absolute Pressure Sensor Signal

### Manifold Absolute Pressure (MAP) Sensor (LMU)

#### Connector Part Information

- OEM: 12129946
- Service: 88987997
- Description: 3-Way F Metri-Pack 150 Series, Sealed (GY)

#### Manifold Absolute Pressure (MAP) Sensor (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BN | 469 | Low Reference
B | GY/BK | 433 | Manifold Absolute Pressure Sensor Signal
C | L-GN | 432 | 5-Volt Reference

### Manifold Absolute Pressure (MAP) Sensor (LV8)

#### Connector Part Information

- OEM: 12059595
- Service: 88986451
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Manifold Absolute Pressure (MAP) Sensor (LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | D-BU | 732 | Low Reference
B | L-GN | 432 | MAP Sensor Signal
C | PU | 719 | 5-Volt Reference

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LXV)

#### Connector Part Information

- OEM: 1-928-405-138
- Service: N/A
- Description: 5-Way F 2.8 Timer Series (Bosch), Sealed (BK)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor (LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | WH | 455 | Intake Air Temperature Sensor Signal
2 | OG/BK | 1732 | 5-Volt Reference
3 | L-BU | 469 | Mass Air Flow Sensor Signal
4 | BN | 456 | Low Reference
5 | BK | 51 | Ground

### Mode Actuator (C68)

#### Connector Part Information

- OEM: MG 651444
- Service: N/A
- Description: 3-Way F 030 Series, KET (WH)

#### Mode Actuator (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/D-BU | -- | 5-Volt Reference
2 | BK | -- | Ground
3 | D-BU | -- | Signal

### Octane Selection Switch (LDT/LXV)

#### Connector Part Information

- OEM: MG 620395
- Service: N/A
- Description: 3-Way M SDL Series, Sealed KET (WH)

#### Octane Selection Switch (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 892 | Octane Selection Signal 1
2 | BK | 51 | Ground
3 | D-GN | 890 | Octane Selection Signal 2

### Octane Selection Switch (L95/LXT)

#### Connector Part Information

- OEM: MG 620395
- Service: N/A
- Description: 3-Way M SDL Series, Sealed KET (WH)

#### Octane Selection Switch (L95/LXT)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 50 | Ground
3 | D-GN | 892 | Octane Selection Signal

### Octane Selection Switch (LMU/LV8)

#### Connector Part Information

- OEM: MG 620395
- Service: N/A
- Description: 3-Way M SDL Series, Sealed KET (WH)

#### Octane Selection Switch (LMU/LV8)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 890 | Octane Selection Signal 2
2 | BK | 50 | Ground
3 | BN | 892 | Octane Selection Signal 1 (LMU)
D-GN | 892 | Octane Selection Signal 1 (LV8)

### OnStar X1 (UE1)

#### Connector Part Information

- OEM: 0-0917981-1
- Service: N/A
- Description: 16-Way F 040/070 Hybrid MK-II Series, Tyco (WH)

#### OnStar X1 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 5060 | Low Speed GMLAN Serial Data
2 | BN/WH | 2517 | Keypad Red LED Signal
3 | YE/BK | 2516 | Keypad Green LED Signal
4-5 | -- | -- | Not Used
6 | L-GN/BK | 2515 | Keypad Supply Voltage
7 | BK | 450 | Ground
8 | BK | 450 | Ground
9 | -- | -- | Not Used
10 | PU | 1807 | Class 2 Serial Data (Primary)
11 | D-GN/WH | 2514 | Keypad Signal
12 | YE | 710 | Class 2 Serial Data
13 | GY/BK | 5167 | Battery Backup Low Reference
14 | RD/WH | 5235 | Battery Backup Supply Voltage
15 | RD/WH | 240 | Battery Positive Voltage
16 | RD/WH | 240 | Battery Positive Voltage

### OnStar X2 (UE1)

#### Connector Part Information

- OEM: 0-0917975-7
- Service: N/A
- Description: 12-Way F 040/070 Hybrid MK-II Series, Tyco (YE)

#### OnStar X2 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 667 | Mono Out (+)
2 | GY | 668 | Mono Out (-)
3 | PU | 1807 | Class 2 Serial Data (Primary)
4 | YE | 710 | Class 2 Serial Data
5-7 | -- | -- | Not Used
8 | D-GN | 1782 | Drain Wire
9 | GY | 655 | Cellular Microphone Signal
10 | D-GN | 654 | Cellular Telephone Microphone Low Reference
11-12 | -- | -- | Not Used

### OnStar Backup Battery (UE1)

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series, Sealed (BK)

#### OnStar Backup Battery (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | RD/WH | 5235 | Battery Backup Supply Voltage
B | GY/BK | 5167 | Battery Backup Low Reference

### OnStar Button Assembly (UE1)

#### Connector Part Information

- OEM: 12047886
- Service: 12101822
- Description: 8-Way F Metri-Pack 150 Series (BK)

#### OnStar Button Assembly (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | L-GN/BK | 2515 | Keypad Supply Voltage
B | D-GN/WH | 2514 | Keypad Signal
C-D | -- | -- | Not Used
E | BK | 450 | Ground
F | YE/BK | 2516 | Keypad Green LED Signal
G | BN/WH | 2517 | Keypad Red LED Signal
H | -- | -- | Not Used

### Outside Rearview Mirror - Driver (Hatchback with DM7)

#### Connector Part Information

- OEM: MG 651044
- Service: N/A
- Description: 6-Way F 090 II Series, KET (WH)

#### Outside Rearview Mirror - Driver (Hatchback with DM7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 650 | Ground
2 | -- | -- | Not Used
3 | L-BU | 82 | Driver Mirror Motor Left Control
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | YE | 88 | Driver Mirror Motor Up Control
6 | OG | 267 | Heated Mirror Element Supply Voltage

### Outside Rearview Mirror - Driver (Notchback with DM7)

#### Connector Part Information

- OEM: 173850
- Service: N/A
- Description: 8-Way 070 MLC Series, AMP (WH)

#### Outside Rearview Mirror - Driver (Notchback with DM7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 190 | Driver Folding Mirror Motor Extend Control
2 | L-BU | 191 | Driver Folding Mirror Motor Retract Control
3 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | YE | 88 | Driver Mirror Motor Up Control
7 | L-BU | 82 | Driver Mirror Motor Left Control
8 | BK | 650 | Ground

### Outside Rearview Mirror - Passenger (Hatchback with DM7)

#### Connector Part Information

- OEM: MG 651044
- Service: N/A
- Description: 6-Way F 090 II Series, KET (WH)

#### Outside Rearview Mirror - Passenger (Hatchback with DM7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 650 | Ground
2 | -- | -- | Not Used
3 | WH | 81 | Driver Mirror Motor Right Control
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | L-GN | 89 | Driver Mirror Motor Down Control
6 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage

### Outside Rearview Mirror - Passenger (Notchback with DM7)

#### Connector Part Information

- OEM: 173850
- Service: N/A
- Description: 8-Way F 070 MLC Series, Tyco (WH)

#### Outside Rearview Mirror - Passenger (Notchback with DM7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 5023 | Passenger Folding Mirror Motor Retract Control (DM4)
2 | YE | 5004 | Passenger Folding Mirror Motor Extend Control (DM4)
3 | OG | 267 | Heated Mirror/Rear Defog Relay Coil Supply Voltage
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | -- | -- | Not Used
6 | L-GN | 89 | Driver Mirror Motor Down Control
7 | WH | 81 | Driver Mirror Motor Right Control
8 | BK | 650 | Ground

### Outside Rearview Mirror Switch

#### Connector Part Information

- OEM: 173850
- Service: N/A
- Description: 8-Way 070 ML Series, Tyco (WH)

#### Outside Rearview Mirror Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 88 | Driver Mirror Motor Up Control
2 | GY/BK | 2232 | Folding Mirrors Signal (DL7)
3 | L-GN | 89 | Driver Mirror Motor Down Control
4 | GY | 90 | Passenger Mirror Motor Left Control
5 | L-BU | 82 | Driver Mirror Motor Left Control
6 | BK | 450 | Ground
7 | WH | 81 | Driver Mirror Motor Right Control
8 | BN | 641 | Ignition 3 Voltage

### Overhead Console Courtesy/Reading Lamps

#### Connector Part Information

- OEM: MG 610402
- Service: N/A
- Description: 8-Way F SDL Series, KET (WH)

#### Overhead Console Courtesy/Reading Lamps

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 100 | Sunroof Switch Open Signal
2 | YE | 110 | Sunroof Switch Close Signal
3 | BN | 641 | Ignition 3 Voltage
4 | BK | 450 | Ground
5 | GY | 157 | Courtesy Lamp Control
6 | -- | -- | Not Used
7 | RD/WH | 1340 | Battery Positive Voltage
8 | -- | -- | Not Used

### Park Lamp - Left Front (Hatchback with NA)

#### Connector Part Information

- OEM: 936184-2
- Service: N/A
- Description: 2-Way F.090 Series, Sealed Tyco (WH)

#### Park Lamp - Left Front (Hatchback with NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | PU | 709 | Left Park Lamp Supply Voltage

### Park Lamp - Right Front (Hatchback with NA)

#### Connector Part Information

- OEM: 936184-2
- Service: N/A
- Description: 2-Way F.090 Series, Sealed Tyco (WH)

#### Park Lamp - Right Front (Hatchback with NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | BN/WH | 309 | Right Park Lamp Supply Voltage

### Park/Neutral Position (PNP) Switch (LMU)

#### Connector Part Information

- OEM: 7283-1909-40
- Service: N/A
- Description: 10-Way F, Yazaki (GY)

#### Park/Neutral Position (PNP) Switch (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 323 | Neutral Start Signal
2 | GY | 773 | Transmission Range Switch Signal C
3 | BN/WH | 771 | Transmission Range Switch Signal A
4 | BK | 50 | Ground
5 | YE | 1479 | A/T Neutral Signal
6 | YE/BK | 772 | Transmission Range Switch Signal B
7 | PK | 841 | Ignition 1 Voltage
8 | BN | 24 | Backup Lamp Supply Voltage
9 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
10 | -- | -- | Not Used

### Park/Neutral Position (PNP) Switch (without LMU)

#### Connector Part Information

- OEM: 7283-1296-40
- Service: N/A
- Description: 9-Way F, Yazaki (GY)

#### Park/Neutral Position (PNP) Switch (without LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
2 | L-GN | 24 | Backup Lamp Supply Voltage
3 | PK | 841 | Ignition 1 Voltage (-WHB)
PK | 50 | Ground (WHB)
4 | YE/BK | 772 | Transmission Range Switch Signal B
5 | YE | 1479 | A/T Neutral Signal
6 | BK | 50 | Ground
7 | BN/WH | 771 | Transmission Range Switch Signal A
8 | GY | 773 | Transmission Range Switch Signal C
9 | BN | 323 | Neutral Start Signal

### Passenger Airbag Disable Switch

#### Connector Part Information

- OEM: 0-1743282-1
- Service: N/A
- Description: 8-Way F 0.64 MQS Series (BK)

#### Passenger Airbag Disable Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN/WH | -- | Passenger Airbag OFF Indicator Control
2 | BK | -- | Ground
3 | D-GN | -- | Occupant Sensor - Indicator Status - Off
4 | PU | -- | Manual Cutoff Switch
5 | BK | -- | Ground
6-8 | -- | -- | Not Used

### Passenger Presence System (PPS) Sensor

#### Connector Part Information

- OEM: 1-0967640-1
- Service: N/A
- Description: 4-Way F Connector (BK)

#### Passenger Presence System (PPS) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | -- | Ignition 1 Voltage
2 | D-BU/WH | -- | SIR Defeat Indicator Lamp Output - Passenger
3 | BK | -- | Ground
4 | -- | -- | Not Used

### Radio (UY4)

#### Connector Part Information

- OEM: 368136-1
- Service: N/A
- Description: 26-Way F 040/070 Hybrid Series, Tyco (NA)

#### Radio (UY4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 200 | Right Front Speaker Output (+)
2 | D-BU | 46 | Right Rear Speaker Output (+)
3 | BN/WH | 309 | Right Park Lamp Supply Voltage
4 | YE | 43 | Accessory Voltage
5 | D-GN | 145 | Antenna Relay Coil Supply Voltage
6 | -- | -- | Not Used
7 | D-BU | 1796 | Steering Wheel Controls Signal
8-9 | -- | -- | Not Used
10 | PK/BK | 6434 | CAN Bus High #2 Serial Data
11 | BN | 199 | Left Rear Speaker Output (+)
12 | BN | 201 | Left Front Speaker Output (+)
13 | RD/WH | 540 | Battery Positive Voltage
14 | D-GN | 117 | Right Front Speaker Output (-)
15 | L-BU | 115 | Right Rear Speaker Output (-)
16 | L-GN | 24 | Backup Lamp Supply Voltage
17-20 | -- | -- | Not Used
21 | BN/WH | 33 | Brake Warning Indicator Control
22 | -- | -- | Not Used
23 | GY/BK | 6435 | CAN Bus Low #2 Serial Data
24 | YE | 116 | Left Rear Speaker Output (-)
25 | GY | 118 | Left Front Speaker Output (-)
26 | BK | 650 | Ground

### Radio X1 (without UY4)

#### Connector Part Information

- OEM: 15464950
- Service: N/A
- Description: 14-Way F GT 150 Micro 64 Modular, (BK)

#### Radio X1 (without UY4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 540 | Battery Voltage
2 | BN | 201 | Left Front Speaker Output (+)
3 | L-GN | 200 | Right Front Speaker Output (+)
4-5 | -- | -- | Not Used
6 | D-GN | 145 | Antenna Relay Coil Supply Voltage (NB-UE1)
RD/WH | 440 | Battery Positive Voltage (UE1)
7 | BN/WH | 309 | Park Lamp Feed - Right
8 | BK | 650 | Ground
9 | GY | 118 | Speaker Return - Left Front
10 | D-GN | 117 | Speaker Return - Right Front
11 | -- | -- | Not Used
12 | BN/WH | 372 | Remote Radio Return - Audio
13 | D-GN | 5060 | Low Speed GMLAN Serial Data (WHB)
14 | D-GN | 5060 | Low Speed GMLAN Serial Data (WHB)
D-GN | 230 | Instrument Panel Lamps Dimming Control (-WHB)

### Radio X2 (without UY4)

#### Connector Part Information

- OEM: 15394150
- Service: 15394150
- Description: 16-Way F Micro 64 Series, (BK)

#### Radio X2 (without UY4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 230 | Instrument Panel Lamps Dimming Control
2-4 | -- | -- | Not Used
5 | BN | 199 | Left Rear Speaker Output (+)
6 | D-BU | 46 | Right Rear Speaker Output (+)
7 | OG | 667 | Mono Mix In (+)
8-11 | -- | -- | Not Used
12 | D-BU | 1796 | Steering Wheel Controls Signal
13 | YE | 116 | Left Rear Speaker Output (-)
14 | L-BU | 115 | Right Rear Speaker Output (-)
15 | GY | 668 | Mono Mix In (-)
16 | YE | 43 | Accessory Voltage

### Radio Antenna X1 (UE1)

#### Connector Part Information

- OEM: GT13GM-1/1S-HU(22)
- Service: N/A
- Description: 3-Way F GT13 Coaxial Series, Hirose (WH)

#### Radio Antenna X1 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 440 | Battery Positive Voltage
C | BK | 5112 | Radio Antena Coax
S | -- | -- | Not Used

### Radio Antenna X2 (UE1)

#### Connector Part Information

- OEM: 1438810-1
- Service: N/A
- Description: 1-Way F Coaxial Snap-Lock, Tyco (BK)

#### Radio Antenna X2 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 5112 | Radio Antena Coax

### Radio Antenna X1 (XMR)

#### Connector Part Information

- OEM: 638832-3
- Service: N/A
- Description: 1-Way F SMB RF Series, Tyco (BU)

#### Radio Antenna X1 (XMR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 5113 | Radio Antena Coax

### Radio Antenna X2 (XMR)

#### Connector Part Information

- OEM: 2FA1-NKRJ-C01-3
- Service: N/A
- Description: 1-Way F Coaxial Snap-Lock (BK)

#### Radio Antenna X2 (XMR)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 5113 | Radio Antena Coax

### Rear Compartment Lamp

#### Connector Part Information

- OEM: 36277
- Service: N/A
- Description: 2-Way F 6.3 Faston Series, AK (GY)

#### Rear Compartment Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 1340 | Battery Voltage
2 | GY/BK | 737 | Rear Compartment Lamp Control (NB)
BK | 737 | Rear Compartment Lamp Control (HB)

### Rear Compartment Lid Ajar Switch

#### Connector Part Information

- OEM: 174463-1
- Service: N/A
- Description: 2-Way F 070 Multi-Lock 070 Series, Tyco (WH)

#### Rear Compartment Lid Ajar Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 263 | Tamper Switch Signal
2 | BK | 450 | Ground

### Rear Compartment Lid Latch Release Actuator (Notchback)

#### Connector Part Information

- OEM: MG 651032
- Service: N/A
- Description: 3-Way F 090 II Series, KET (NA)

#### Rear Compartment Lid Latch Release Actuator (Notchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 450 | Ground
2 | BN | 253 | Trunk Release Relay Control
3 | GY/BK | 737 | Rear Compartment Lamp Control

### Rear Compartment Lid Latch Switch (Hatchback)

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Rear Compartment Lid Latch Switch (Hatchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/BK | 737 | Rear Compartment Lamp Control
2 | BK | 850 | Ground

### Rear Window Defogger Grid X1 (Hatchback)

#### Connector Part Information

- OEM: 174090-2
- Service: N/A
- Description: 1-Way F 250 Series, Tyco (BK)

#### Rear Window Defogger Grid X1 (Hatchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 1093 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid X2 (Hatchback)

#### Connector Part Information

- OEM: 174090-2
- Service: N/A
- Description: 1-Way F 250 Series, Tyco (BK)

#### Rear Window Defogger Grid X2 (Hatchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 850 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid (Notchback with UE1)

#### Connector Part Information

- OEM: MG 630063
- Service: N/A
- Description: 1-Way F 250 Series, KET (NA)

#### Rear Window Defogger Grid (Notchback with UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 1093 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid ( Notchback without UE1)

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (NA)

#### Rear Window Defogger Grid (Notchback without UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD | 1093 | Rear Defog Element Supply Voltage
2 | D-GN | 145 | Antenna Relay Coil Supply Voltage

### Rear Window Washer Fluid Pump (Hatchback)

#### Connector Part Information

- OEM: MG 640605-2
- Service: See Catalog
- Description: 2-Way F 090 WP Series, KET (BK)

#### Rear Window Washer Fluid Pump (Hatchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | L-GN/BK | 392 | Rear Window Washer Pump Control

### Rear Window Wiper Motor (Hatchback with C25)

#### Connector Part Information

- OEM: MG 610396
- Service: See Catalog
- Description: 4-Way F SDL Series Sealed, KET (WH)

#### Rear Window Wiper Motor (Hatchback with C25)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 639 | Ignition 1 Voltage
2 | GY | 393 | Rear Window Wiper Motor Control
3 | D-BU | 58 | Right Cornering Lamp Supply Voltage
4 | BK | 850 | Ground

### Rear Window Wiper Motor (Hatchback with C16)

#### Connector Part Information

- OEM: MG 610896
- Service: See Catalog
- Description: 8-Way F SDL-II Series, KET (WH)

#### Rear Window Wiper Motor (Hatchback with C16)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 393 | Rear Window Wiper Motor Control
2 | L-GN/BK | 392 | Rear Window Washer Pump Control
3 | BK | 850 | Ground
4-7 | -- | -- | Not Used
8 | PK | 639 | Ignition 1 Voltage

### Recirculation Actuator (C60)

#### Connector Part Information

- OEM: MG 610203
- Service: N/A
- Description: 7-Way F 118 (PA) Series, KET (NA)

#### Recirculation Actuator (C60)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | PK/WH | 1648 | Recirculation Door Control A
6 | -- | -- | Not Used
7 | L-GN/BK | 1647 | Recirculation Door Control B

### Recirculation Actuator (C68)

#### Connector Part Information

- OEM: MG 651444
- Service: N/A
- Description: 3-Way F 030 Series, KET (WH)

#### Recirculation Actuator (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/D-BU | -- | 5-Volt Reference
2 | BK | -- | Ground
3 | D-BU | -- | Signal

### Remote Control Door Lock Receiver (RCDLR) (UA5)

#### Connector Part Information

- OEM: MG 611336
- Service: N/A
- Description: 26-Way F PCB Series, KET (WH)

#### Remote Control Door Lock Receiver (RCDLR) (UA5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 29 | Horn Control
2 | BK | 450 | Ground
3 | -- | -- | Not Used
4 | L-BU | 263 | Tamper Switch Signal
5 | OG/BK | 737 | Rear Compartment Lamp Control
6 | -- | -- | Not Used
7 | PK/BK | 109 | Hood Ajar Switch Signal
8 | WH | 156 | Courtesy Lamp Low Control
9 | L-BU | 194 | Door Unlock Control (Notchback -WHB)
10 | GY/D-GN | 355 | Driver Door Lock Relay Lock Control
11 | YE | 356 | Driver Door Lock Relay Unlock Control
12 | L-BU | 262 | Driver Door Key Switch Signal
13 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
14 | BN | 253 | Trunk Release Relay Control
15 | PK | 239 | Ignition 1 Voltage
16 | -- | -- | Not Used
17 | BK/WH | 2051 | Serial Data Signal
18 | L-GN | 80 | Key In Ignition Switch Signal
19 | YE | 749 | Security Indicator Control
20 | PU | 265 | Passenger Door Key Switch Signal
21 | -- | -- | Not Used
22 | BN | 7020 | Remote Control Signal
23-24 | -- | -- | Not Used
25 | RD/WH | 340 | Battery Positive Voltage
26 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage

### Rough Road Sensor (without JM4)

#### Connector Part Information

- OEM: 174354-2
- Service: N/A
- Description: 2-Way M J-Mark II Series, Sealed Tyco (BK)

#### Rough Road Sensor (without JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | YE | 873 | Left Front Wheel Speed Sensor Low Reference

### Seat Belt Pretensioner - Driver (A70)

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way Connector (GN)

#### Seat Belt Pretensioner - Driver (A70)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG/WH | 2119 | Seat Belt Pretensioner - Left - Low Control
2 | BN/WH | 2118 | Seat Belt Pretensioner - Left - High Control

### Seat Belt Pretensioner - Passenger (A70)

#### Connector Part Information

- OEM: V23540-M5302-Y22
- Service: N/A
- Description: 2-Way Connector (GN)

#### Seat Belt Pretensioner - Passenger (A70)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 2117 | Seat Belt Pretensioner - Right - Low Control
2 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control

### Seat Belt Switch

#### Connector Part Information

- OEM: MG 610392
- Service: N/A
- Description: 2-Way F SDL Series, KET (WH)

#### Seat Belt Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 238 | Seat Belt Switch - Left
2 | BK | 650 | Ground

### Speaker - Left Front

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (WH)

#### Speaker - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 201 | Left Front Speaker Output (+)
2 | GY | 118 | Left Front Speaker Output (-)

### Speaker - Left Rear

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (WH)

#### Speaker - Left Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 116 | Left Rear Speaker Output (-)
2 | BN | 199 | Left Rear Speaker Output (+)

### Speaker - Left Tweeter

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Speaker - Left Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | GY | 118 | Left Front Speaker Output (-)
2 | BN | 201 | Left Front Speaker Output (+)

### Speaker - Right Front

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (WH)

#### Speaker - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 200 | Right Front Speaker Output (+)
2 | D-GN | 117 | Right Front Speaker Output (-)

### Speaker - Right Rear

#### Connector Part Information

- OEM: MG 610043
- Service: N/A
- Description: 2-Way F 250 Series, KET (WH)

#### Speaker - Right Rear

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 115 | Right Rear Speaker Output (+)
2 | D-BU | 46 | Right Rear Speaker Output (-)

### Speaker - Right Tweeter

#### Connector Part Information

- OEM: MG 610070
- Service: N/A
- Description: 2-Way F 090 (2.3 mm) Series, KET (WH)

#### Speaker - Right Tweeter

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 117 | Right Front Speaker Output (-)
2 | L-GN | 200 | Right Front Speaker Output (+)

### Starter Relay (MLQ without WHB)

#### Connector Part Information

- OEM: AK 36905
- Service: N/A
- Description: 9-Way Metri-Pack 150 Series (BU)

#### Starter Relay (MLQ without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not used
2 | YE | 5 | Crank Voltage
3 | -- | -- | Not used
4 | BN | 323 | Neutral Start Signal
5 | -- | -- | Not used
6 | PU | 6 | Starter Solenoid Crank Voltage
7 | -- | -- | Not used
8 | YE | 5 | Crank Voltage
YE | 5 | Crank Voltage
9 | -- | -- | Not used

### Stop Lamp Switch

#### Connector Part Information

- OEM: MG 610267
- Service: N/A
- Description: 4-Way F 250 D/L Series, KET (NA)

#### Stop Lamp Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 878 | Stop Lamp Supply Voltage
2 | L-BU | 20 | Stop Lamp Supply Voltage
3 | PK | 239 | Ignition 1 Voltage
4 | RD/WH | 340 | Battery Positive Voltage

### Sunload Sensor (C68)

#### Connector Part Information

- OEM: 174056-2
- Service: N/A
- Description: 2-Way F 040 Series, Tyco (BK)

#### Sunload Sensor (C68)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU/WH | -- | Low Reference
2 | YE/RD | -- | Sunload Sensor Signal

### Sunroof Control Module (CF5)

#### Connector Part Information

- OEM: AMP 174923
- Service: N/A
- Description: 6-Way F 070 Series Multi-Lock, Tyco (WH)

#### Sunroof Control Module (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | 110 | Sunroof Switch Close Signal
2 | -- | -- | Not Used
3 | RD/WH | 640 | Battery Positive Voltage
4 | BK | 450 | Ground
5 | -- | -- | Not Used
6 | BN | 100 | Sunroof Switch Open Signal

### Tail Lamp - Left (Hatchback with T9E)

#### Connector Part Information

- OEM: MG 610054
- Service: N/A
- Description: 8-Way F 090 (2.3 mm) Series, KET (NA)

#### Tail Lamp - Left (Hatchback with T9E)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 450 | Ground
3 | BK | 450 | Ground
4 | L-GN | 24 | Backup Lamp Supply Voltage
5 | OG | 122 | Roof Off-Road Lamps Supply Voltage 1
6 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
7 | PU | 709 | Left Park Lamp Supply Voltage
8 | L-BU | 20 | Stop Lamp Supply Voltage

### Tail Lamp - Left (Notchback)

#### Connector Part Information

- OEM: 936233-1
- Service: N/A
- Description: 8-Way F 090 Series, Tyco (BK)

#### Tail Lamp - Left (Notchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 122 | Rear Fog Lamp Supply Voltage (TRA)
2 | BK | 450 | Ground
BK | 450 | Ground
3 | BK | 450 | Ground
4 | L-GN | 24 | Backup Lamp Supply Voltage
5 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage
7 | PU | 709 | Left Park Lamp Supply Voltage
PU | 709 | Left Park Lamp Supply Voltage (FL5)
8 | PU | 709 | Left Park Lamp Supply Voltage (FL5)

### Tail Lamp - Right (Hatchback with T9E)

#### Connector Part Information

- OEM: MG 610054
- Service: N/A
- Description: 8-Way F 090 (2.3 mm) Series, KET (NA)

#### Tail Lamp - Right (Hatchback with T9E)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | BK | 450 | Ground
3 | BK | 450 | Ground
4 | L-GN | 24 | Backup Lamp Supply Voltage
5 | -- | -- | Not Used
6 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
7 | BN/WH | 309 | Right Park Lamp Supply Voltage
8 | L-BU | 20 | Stop Lamp Supply Voltage

### Tail Lamp - Right (Notchback)

#### Connector Part Information

- OEM: 936233-1
- Service: N/A
- Description: 8-Way F 090 Series, Tyco (BK)

#### Tail Lamp - Right (Notchback)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | OG | 122 | Rear Fog Lamp Supply Voltage (TRA)
2 | BK | 450 | Ground
BK | 450 | Ground
3 | BK | 450 | Ground
4 | L-GN | 24 | Backup Lamp Supply Voltage
5 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
6 | BN | 20 | Stop Lamp Supply Voltage
7 | BN/WH | 309 | Right Park Lamp Supply Voltage
BN/WH | 309 | Right Park Lamp Supply Voltage (FL5)
8 | BN/WH | 309 | Right Park Lamp Supply Voltage (FL5)

### Theft Deterrent Alarm

#### Connector Part Information

- OEM: KUM PB 625-02027
- Service: N/A
- Description: 2-Way F NMWP 04F-B Assembly (BK)

#### Theft Deterrent Alarm

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | YE | -- | Arm Alarm Signal
2 | RD/WH | -- | Battery Positive Voltage

### Theft Detterent Module (TDM) (BAH with WHB)

#### Connector Part Information

- OEM: HS015-04015
- Service: N/A
- Description: 4-Way F 090 CS Series, KUM (WH)

#### Theft Detterent Module (TDM) (BAH with WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 240 | Battery Positive Voltage
2 | YE | 43 | Accessory Voltage
3 | BK | 450 | Ground
4 | D-GN | 5060 | Low Speed GMLAN Serial Data

### Theft Detterent Module (TDM) (BAH without WHB)

#### Connector Part Information

- OEM: 35508-0700
- Service: N/A
- Description: 7-Way F (WH)

#### Theft Detterent Module (TDM) (BAH without WHB)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 239 | Ignition 1 Voltage
2 | RD/WH | 240 | Battery Positive Voltage
3 | -- | -- | Not Used
4 | BK | 450 | Ground
5 | L-BU/WH | 1800 | CKP Sensor 2 Signal
6 | BK/WH | 2051 | Serial Data Signal
7 | YE | 749 | Security Indicator Control

### Throttle Body (LMU)

#### Connector Part Information

- OEM: 174982-2
- Service: N/A
- Description: 8-Way F 070 J-Mark II Series Sealed, Tyco (BK)

#### Throttle Body (LMU)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 425 | Idle Speed Motor Feed
2 | GY | 416 | 5-Volt Reference
3 | -- | -- | Not Used
4 | D-GN | 534 | Idle Motor Position
5 | D-BU | 426 | Idle Speed Motor Return
6 | PK | 427 | Idle Switch Position
7 | D-BU | 417 | Throttle Position Signal
8 | BN | 808 | Low Reference

### Throttle Body (LDT/LXV)

#### Connector Part Information

- OEM: 15355297
- Service: N/A
- Description: 6-Way F GT 150 Series, Sealed (BK)

#### Throttle Body (LDT/LXV)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | YE | 581 | Throttle Actuator Control (TAC) Motor Control - 1
B | D-BU | 528 | Throttle Actuator Control (TAC) Motor Control - 2
C | PU | 427 | 5-Volt Reference
D | WH | 425 | TP Sensor 2 Signal
E | L-BU | 426 | Low Reference
F | BN/BK | 486 | TP Sensor 1 Signal

### Tire Pressure Module (UJ9)

#### Connector Part Information

- OEM: 64002-1215
- Service: N/A
- Description: 12-Way F 040 Series, Molex (GY)

#### Tire Pressure Module (UJ9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | RD/WH | 540 | Battery Positive Voltage
2 | GN/WH | 817 | Vehicle Speed Signal
3 | BK/WH | 2051 | Serial Data Signal
4 | BN/WH | 33 | Brake Warning Indicator Control
5 | L-BU | 74 | Park Lamp Switch Signal
6 | -- | -- | Not Used
7 | BN | 25 | Charge Indicator Control
8 | PK | 239 | Ignition 1 Voltage
9 | D-GN | 29 | Horn Control
10 | D-BU | 7001 | Low Tire Pressure Indicator Control
11 | BK | 450 | Ground
12 | -- | -- | Not Used

### Transmission Control Module (TCM) X1

#### Connector Part Information

- OEM: 1318756-1
- Service: N/A
- Description: 24-Way F 025/090 Series, AMP (WH)

#### Transmission Control Module (TCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | YE/BK | 1227 | Low Reference
3 | -- | -- | Not Used
4 | OG | 1226 | Pressure Control Solenoid Control
5 | D-BU | 1225 | Torque Converter Clutch Solenoid Control
6 | PK | 239 | Ignition 1 Voltage (-NA)
RD/WH | 440 | Battery Positive Voltage (NA)
7 | YE | 710 | Class 2 Serial Data
8 | YE | 710 | Class 2 Serial Data (NA)
9-10 | -- | -- | Not Used
11 | PU | 898 | Transmission Fluid Temperature Sensor Signal
12 | OG/BK | 586 | Transmission Fluid Temperature Sensor Low Reference
13 | -- | -- | Not Used
14 | PK | 1224 | Timing Valve Control
15 | YE/BK | 1223 | Shift Solenoid 2 Valve Control
16 | L-GN | 1222 | Shift Solenoid 1 Valve Control
17 | PU | 1807 | Class 2 Serial Data (Primary)
18 | PU | 1807 | Class 2 Serial Data (Primary) (NA)
19-22 | -- | -- | Not Used
23 | BK | 50 | Ground
24 | RD/WH | 440 | Battery Positive Voltage (-WHB)
YE | 111 | Vehicle Wake Up Signal (WHB)

### Transmission Control Module (TCM) X2

#### Connector Part Information

- OEM: 1318757-1
- Service: N/A
- Description: 26-Way F 025/090 Series, AMP (WH)

#### Transmission Control Module (TCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-GN | 24 | Backup Lamp Supply Voltage
2 | -- | -- | Not Used
3 | YE | 1481 | Hold Motor Indicator Control (-WHB)
4 | D-GN/WH | 1135 | Transmission Hold Signal (-WHB)
5 | -- | -- | Not Used
6 | WH | 6254 | Input Shaft Speed (ISS) Sensor High Signal
7 | BN/WH | 771 | Transmission Range Switch Signal A
8 | YE | 1479 | Park/Neutral Position (PNP) Switch Neutral Signal
9-15 | -- | -- | Not Used
16 | OG | 6253 | Input Shaft Speed (ISS) Sensor Low Signal
17 | -- | -- | Not Used
18 | GY | 773 | Transmission Range Switch Signal C
19 | YE/BK | 772 | Transmission Range Switch Signal B
20 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal
21 | PK | 239 | Ignition 1 Voltage (WHB)
22 | L-BU | 20 | Stop Lamp Supply Voltage
23 | BK/WH | 2051 | Serial Data Signal (-WHB)
24 | -- | -- | Not Used
25 | D-GN/WH | 8175 | Vehicle Speed Signal
26 | -- | -- | Not Used

### Turn Signal Lamp - Left Front (T84)

#### Connector Part Information

- OEM: 936184-2
- Service: N/A
- Description: 2-Way F 090 Series, Tyco (BK)

#### Turn Signal Lamp - Left Front (T84)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 50 | Ground
2 | L-BU | 14 | Left Turn Signal Supply Voltage

### Turn Signal Lamp - Left Front (FL2)

#### Connector Part Information

- OEM: 936187-2
- Service: N/A
- Description: 3-Way F 090 Series, Sealed Tyco (BK)

#### Turn Signal Lamp - Left Front (FL2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PU | 709 | Park Lamp Feed
2 | BK | 50 | Ground
3 | L-BU | 14 | Left Turn Signal Supply Voltage

### Turn Signal Lamp - Right Front (T84)

#### Connector Part Information

- OEM: 936184-2
- Service: N/A
- Description: 2-Way F 090 Series, Tyco (BK)

#### Turn Signal Lamp - Right Front (T84)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | D-BU | 15 | Right Turn Signal Supply Voltage

### Turn Signal Lamp - Right Front (FL2)

#### Connector Part Information

- OEM: 936187-2
- Service: N/A
- Description: 3-Way F 090 Series, Sealed Tyco (BK)

#### Turn Signal Lamp - Right Front (FL2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN/WH | 309 | Park Lamp Feed
2 | BK | 250 | Ground
3 | D-BU | 15 | Right Turn Signal Supply Voltage

### Turn Signal/Hazard Flasher Module

#### Connector Part Information

- OEM: AK 36906
- Service: N/A
- Description: 9-Way Metri-Pack 150 Series (GN)

#### Turn Signal/Hazard Flasher Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-3 | -- | -- | Not used
4 | BK | 450 | Ground
5 | -- | -- | Not used
6 | L-BU | 1508 | Turn/Hazard Module Supply Voltage
7 | -- | -- | Not used
8 | PU | 16 | Turn Signal Flasher Signal
9 | -- | -- | Not used

### Turn Signal/Multifunction Switch

#### Connector Part Information

- OEM: MG 610203
- Service: N/A
- Description: 7-Way F 118 (PA) Series, KET (NA)

#### Turn Signal/Multifunction Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Lamps Supply Voltage
2 | PU | 16 | Turn Signal Flasher Signal
3 | D-BU | 15 | Right Turn Signal Lamps Supply Voltage
4 | L-BU | 1346 | Headlamp Supply Voltage
L-BU | 1346 | Headlamp Supply Voltage (WHB)
5 | WH | 352 | Headlamp Relay Coil Supply Voltage
6 | BK/WH | 1352 | Headlamp Control
BK/WH | 1352 | Headlamp Control
7 | BK | 450 | Ground

### Turn Signal Repeater Lamp - Left (Hatchback without NA)

#### Connector Part Information

- OEM: MG 610320-5
- Service: N/A
- Description: 2-Way F SWP Series, KET (BK)

#### Turn Signal Repeater Lamp - Left (Hatchback without NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Supply Voltage
2 | BK | 50 | Ground

### Turn Signal Repeater Lamp - Left (Hatchback with NA)

#### Connector Part Information

- OEM: 936184-1
- Service: N/A
- Description: 2-Way F 090 Series, Tyco (WH)

#### Turn Signal Repeater Lamp - Left (Hatchback with NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 14 | Left Turn Signal Supply Voltage
2 | BK | 50 | Ground

### Turn Signal Repeater Lamp - Right (Hatchback without NA)

#### Connector Part Information

- OEM: MG 610320-5
- Service: N/A
- Description: 2-Way F SWP Series, KET (BK)

#### Turn Signal Repeater Lamp - Right (Hatchback without NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 15 | Right Turn Signal Supply Voltage
2 | BK | 250 | Ground

### Turn Signal Repeater Lamp - Right (Hatchback with NA)

#### Connector Part Information

- OEM: 936184-1
- Service: N/A
- Description: 2-Way F 090 Series, Tyco (WH)

#### Turn Signal Repeater Lamp - Right (Hatchback with NA)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-BU | 15 | Right Turn Signal Supply Voltage
2 | BK | 250 | Ground

### Vehicle Speed Sensor (VSS) (LDT/LXV with MLM)

#### Connector Part Information

- OEM: 12059595
- Service: 12059595
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Vehicle Speed Sensor (VSS) (LDT/LXV with MLM)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 51 | Ground (-WHB)
L-GN/BK | 822 | Low Reference (WHB)
B | L-BU | 817 | Vehicle Speed Signal
C | PK | 539 | Ignition 1 Voltage (-WHB)
D-GN | 605 | 5-Volt Reference (WHB)

### Vehicle Speed Sensor (VSS) (L95/LXT with M/T)

#### Connector Part Information

- OEM: 12059595
- Service: 12059595
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Vehicle Speed Sensor (VSS) (L95/LXT with M/T)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 50 | Ground
B | D-GN/WH | 817 | Vehicle Speed Signal
C | PK | 739 | Ignition 1 Voltage

### Vehicle Speed Sensor (VSS) (LMU/LV8 with M/T)

#### Connector Part Information

- OEM: 12059595
- Service: 12059595
- Description: 3-Way F Metri-Pack 150 Series, Sealed (BK)

#### Vehicle Speed Sensor (VSS) (LMU/LV8 with M/T)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BK | 50 | Ground
B | D-GN/WH | 817 | Vehicle Speed Signal
C | PK | 1739 | Ignition 1 Voltage

### Vehicle Speed Sensor (VSS) (XG2)

#### Connector Part Information

- OEM: MG 641234-5
- Service: N/A
- Description: 3-Way F, KET (BK)

#### Vehicle Speed Sensor (VSS) (XG2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 239 | Ignition 1 Voltage
2 | BK | 50 | Ground
3 | D-GN/WH | 817 | Vehicle Speed Signal

### Vehicle Speed Sensor (VSS) (without XG2)

#### Connector Part Information

- OEM: 7283-1232-30
- Service: N/A
- Description: 3-Way F, Yazaki (BK)

#### Vehicle Speed Sensor (VSS) (without XG2)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 239 | Ignition 1 Voltage
2 | BK | 50 | Ground
3 | D-GN/WH | 817 | Vehicle Speed Signal

### Wheel Speed Sensor (WSS) - Left Front (JM4)

#### Connector Part Information

- OEM: 174354-2
- Service: N/A
- Description: 2-Way M J-Mark II Series, Sealed Tyco (BK)

#### Wheel Speed Sensor (WSS) - Left Front (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 830 | Left Front Wheel Speed Sensor Signal
2 | YE | 873 | Left Front Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Left Rear (JM4)

#### Connector Part Information

OEM: 174354-2
Service: N/A
Description: 2-Way M J-Mark II Series, Sealed Tyco (BK)

#### Wheel Speed Sensor (WSS) - Left Rear (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 884 | Left Rear Wheel Speed Sensor Signal
2 | OG | 885 | Left Rear Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Right Front (JM4)

#### Connector Part Information

OEM: 174354-2
Service: N/A
Description: 2-Way M J-Mark II Series, Sealed Tyco (BK)

#### Wheel Speed Sensor (WSS) - Right Front (JM4)
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 833 | Right Front Wheel Speed Sensor Low Reference
2 | D-GN | 872 | Right Front Wheel Speed Sensor Signal

### Wheel Speed Sensor (WSS) - Right Rear (JM4)

#### Connector Part Information

OEM: 174354-2
Service: N/A
Description: 2-Way M J-Mark II Series, Sealed Tyco (BK)

#### Wheel Speed Sensor (WSS) - Right Rear (JM4)
Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BN | 882 | Right Rear Wheel Speed Sensor Signal
2 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference

### Window Motor - Driver (A31/A32)

#### Connector Part Information

OEM: 936224-1
Service: N/A
Description: 2-Way F 090-III Series, AMP (WH)

#### Window Motor - Driver (A31/A32)

Pin

Wire

Circuit

Function

1

BN

165

Power Window Motor Left Front Down Control

2

D-BU

164

Power Window Motor Left Front Up Control

### Window Motor - Driver (LHD with ABZ)

#### Connector Part Information

OEM: PB 625-06027
Service: N/A
Description: 6-Way F 090 NMWP Series, KUM (BK)

#### Window Motor - Driver (LHD with ABZ)

Pin

Wire

Circuit

Function

1

L-GN/BK

580

Battery Positive Voltage

2

BN

165

Power Window Motor Left Front Down Control

3

--

--

Not Used

4

BK

650

Ground

5

D-BU

164

Power Window Motor Left Front Up Control

6

BN/WH

6166

Front Door Window Short Time Down Control

### Window Motor - Driver (RHD with ABZ)

#### Connector Part Information

OEM: MG 610335
Service: N/A
Description: 6-Way F SWP Series, KET (NA)

#### Window Motor - Driver (RHD with ABZ)

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

BN

165

Power Window Motor Left Front Down Control

3

L-GN/BK

580

Battery Positive Voltage

4

BN/WH

6166

Front Door Window Short Time Down Control

5

D-BU

164

Power Window Motor Left Front Up Control

6

BK

650

Ground

### Window Motor - Left Rear (A31)

#### Connector Part Information

OEM: MG 610320-0
Service: N/A
Description: 2-Way F SWP Series, KET (NA)

#### Window Motor - Left Rear (A31)

Pin

Wire

Circuit

Function

1

BN

669

Power Window Motor Left Rear Down Control

2

D-GN

668

Power Window Motor Left Rear Up Control

### Window Motor - Passenger (A31)

#### Connector Part Information

OEM: 936224-1
Service: N/A
Description: 2-Way F 090-III Series, AMP (NA)

#### Window Motor - Passenger (A31)

Pin

Wire

Circuit

Function

1

BN

667

Power Window Motor Right Front Down Control

2

D-BU

666

Power Window Motor Right Front Up Control

### Window Motor - Right Rear (A31)

#### Connector Part Information

OEM: MG 610320-0
Service: N/A
Description: 2-Way F SWP Series, KET (NA)

#### Window Motor - Right Rear (A31)

Pin

Wire

Circuit

Function

1

BN

669

Power Window Motor Left Rear Down Control

2

D-GN

668

Power Window Motor Left Rear Up Control

### Window Switch - Driver (ABZ)

#### Connector Part Information

OEM: MG 612240
Service: N/A
Description: 14-Way F ASC Series, KET (WH)

#### Window Switch - Driver (ABZ)

Pin

Wire

Circuit

Function

1

D-BU

164

Power Window Motor Left Front Up Control

2

BN

165

Power Window Motor Left Front Down Control

3

L-GN/BK

580

Battery Positive Voltage

4

L-BU

166

Power Window Master Switch Right Front Up Signal (LHD)

BN

167

Power Window Master Switch Right Front Down Signal (RHD)

5

BN/WH

6166

Front Door Window Short Time Down Control

BN/WH

6166

Front Door Window Short Time Down Control

6

BN

167

Power Window Master Switch Right Front Down Signal (LHD)

D-BU

1307

Power Window Master Switch Lockout Signal (RHD)

7

D-BU

1307

Power Window Master Switch Lockout Signal (LHD)

L-BU

166

Power Window Motor Right Front Down Control (RHD)

8

D-GN

168

Power Window Master Switch Left Rear Up Signal

9

BN/WH

6166

Front Door Window Short Time Down Control

10

L-GN/BK

580

Battery Positive Voltage

11

BK

650

Ground

12

PU

169

Power Window Master Switch Left Rear Down Signal

13

L-GN

170

Power Window Master Switch Right Rear Up Signal

14

PU

171

Power Window Master Switch Right Rear Down Signal

### Window Switch - Driver (A31)

#### Connector Part Information

OEM: MG 612240
Service: N/A
Description: 14-Way F ASC Series, KET (WH)

#### Window Switch - Driver (A31)

Pin

Wire

Circuit

Function

1

PU

171

Power Window Master Switch Right Rear Down Signal

2

--

--

Not Used

3

L-GN

170

Power Window Master Switch Right Rear Up Signal

4

PU

169

Power Window Master Switch Left Rear Down Signal

5

L-GN/BK

--

Not Used

6

D-GN

168

Power Window Master Switch Left Rear Up Signal

7

BN

167

Power Window Master Switch Right Front Down Signal (LHD)

BN

165

Power Window Motor Left Front Down Control (RHD)

8

BK

650

Ground

9

L-BU

166

Power Window Master Switch Right Front Up Signal (LHD)

D-BU

164

Power Window Motor Left Front Up Control (RHD)

10

D-BU

1307

Power Window Master Switch Lockout Control

11

--

--

Not Used

12

BN

165

Power Window Motor Left Front Down Control (LHD)

BN

167

Power Window Master Switch Right Front Down Signal (RHD)

13

L-GN/BK

580

Battery Positive Voltage

14

D-BU

164

Power Window Motor Left Front Up Control (LHD)

L-BU

166

Power Window Master Switch Right Front Up Signal (RHD)

### Window Switch - Driver (A32)

#### Connector Part Information

OEM: MG 612231
Service: N/A
Description: 8-Way F ASC Series, KET (WH)

#### Window Switch - Driver (A32)

Pin

Wire

Circuit

Function

1

D-BU

164

Power Window Motor Left Front Up Control (LHD)

L-BU

166

Power Window Master Switch Right Front Up Signal (RHD)

2

--

--

Not Used

3

BN

167

Power Window Master Switch Right Front Down Signal (LHD)

BN

165

Power Window Motor Left Front Down Control (RHD)

4

--

--

Not Used

5

L-GN/BK

580

Battery Positive Voltage

6

BN

165

Power Window Motor Left Front Down Control (LHD)

BN

167

Power Window Master Switch Right Front Down Signal (RHD)

7

L-BU

166

Power Window Master Switch Right Front Up Signal (LHD)

D-BU

164

Power Window Motor Left Front Up Control (RHD)

8

BK

650

Ground

### Window Switch - Left Rear (A31)

#### Connector Part Information

OEM: MG 612228
Service: N/A
Description: 6-Way F ASC Series, KET (WH)

#### Window Switch - Left Rear (A31)

Pin

Wire

Circuit

Function

1

D-GN

168

Power Window Master Switch Left Rear Up Signal

2

PU

169

Power Window Master Switch Left Rear Down Signal

3

D-BU

668

Power Window Motor Left Rear Up Control

4

D-BU

1307

Power Window Master Switch Lockout Signal

5

--

--

Not Used

6

BN

669

Power Window Motor Left Rear Down Control

### Window Switch - Passenger (A31)

#### Connector Part Information

OEM: MG 612228
Service: N/A
Description: 6-Way F ASC Series, KET (WH)

#### Window Switch - Passenger (A31)

Pin

Wire

Circuit

Function

1

L-BU

166

Power Window Master Switch Right Front Up Signal

2

PU

167

Power Window Master Switch Right Front Down Signal

3

D-BU

666

Power Window Motor Right Front Up Control

4

D-BU

1307

Power Window Master Switch Lockout Signal

5

--

--

Not Used

6

BN

667

Power Window Motor Right Front Down Control

### Window Switch - Right Rear (A31)

#### Connector Part Information

OEM: MG 612228
Service: N/A
Description: 6-Way F ASC Series, KET (WH)

#### Window Switch - Right Rear (A31)

Pin

Wire

Circuit

Function

1

D-GN

168

Power Window Master Switch Left Rear Up Signal

2

PU

169

Power Window Master Switch Left Rear Down Signal

3

D-BU

668

Power Window Motor Left Rear Up Control

4

D-BU

1307

Power Window Master Switch Lockout Signal

5

--

--

Not Used

6

BN

669

Power Window Motor Left Rear Down Control

### Windshield Washer Fluid Pump

#### Connector Part Information

OEM: MG 640605-5
Service: See Catalog
Description: 2-Way F 090 WP Series, KET (WH)

#### Windshield Washer Pump

Pin

Wire

Circuit

Function

1

BK

50

Ground

2

PK

94

Windshield Washer Switch Signal

### Windshield Wiper Motor

#### Connector Part Information

OEM: 936257-2
Service: See Catalog
Description: 6-Way F MCP-E SLD Series, Sealed Tyco (BK)

#### Windshield Wiper Motor

Pin

Wire

Circuit

Function

1

--

--

Not Used

2

BN

96

Windshield Wiper Switch Pulse Delay Signal

3

PK

639

Ignition 3 Voltage

4

BK

50

Ground

5

PU

92

Windshield Wiper Motor High Speed

6

D-GN

95

Windshield Wiper Motor Low Speed

### Windshield Wiper/Washer Switch X1

#### Connector Part Information

OEM: MG 610154
Service: N/A
Description: 9-Way 118 Series, KET (NA)

#### Windshield Wiper/Washer Switch X1

Pin

Wire

Circuit

Function

1

GY

393

Rear Window Wiper Motor Control (C25)

2

L-GN/BK

392

Rear Window Washer Pump Control (C25)

3

D-BU

58

Rear Window Wiper Auto Stop (C25)

D-BU

58

Rear Window Wiper Auto Stop (-C98)

4

PK

94

Windshield Washer Switch Signal

5

PU

92

Windshield Wiper Motor High Speed

PU

92

Windshield Wiper Motor High Speed (C68)

6

L-BU

97

Windshield Wiper Switch Mist/Off/Low Signal

7

D-GN/RD

91

Windshield Wiper Switch Signal 2

8

PK

639

Ignition 1 Voltage

D-BU

58

Rear Window Wiper Auto Stop (-C98)

9

D-GN

95

Windshield Wiper Motor High Speed

### Windshield Wiper/Washer Switch X2

#### Connector Part Information

OEM: 0-0368501-1
Service: N/A
Description: 4-Way 070 Mulit-Lock Series, Tyco (WH)

#### Windshield Wiper/Washer Switch X2

Pin

Wire

Circuit

Function

1

YE

112

Windshield Wiper Switch Signal 1

2

BK/RD

450

Ground

3

D-BU

1977

Rear Fog Lamp Relay Control (T9E)

4

BK/RD

450

Ground (T9E)