For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antilock Brake System (ABS) Main Relay Operation Voltage | 9-16 V
Antilock Brake System (ABS) Type | 4 Channel 4 Sensor
Speed Ring

- Inside Diameter - Front

69.6 mm

2.7401 in

- Inside Diameter - Rear

58 mm

2.2835 in

- Outside Diameter - Front

83.7 mm

3.2952 in

- Outside Diameter - Rear

69 mm

2.7165 in

- Tooth Volume of the Speed Ring (Front)
- Tooth Volume of the Speed Ring (Rear)

47 EA

40 EA

Wheel Speed Sensor - Resistance | 1,215-1,485 Ω