For 1990-2009 cars

### Removal Procedure

1. Remove the seat back and/or the seat cushion. Refer to Front Seat Back Replacement , Front Seat Cushion Replacement , Rear Split Folding Seat Back Replacement and/or Rear Seat Back Replacement .
2. Remove the hog rings or the retaining clips from the seat back and/or the seat cushion.
3. Remove the seat cover from the seat back and/or the seat cushion.

### Installation Procedure

1. Install the seat cover onto the seat back and/or the seat cushion with the retaining clips or the new hog rings.
2. Install the seat back and/or the seat cushion. Refer to Front Seat Back Replacement , Front Seat Cushion Replacement , Rear Split Folding Seat Back Replacement and/or Rear Seat Back Replacement .