For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antilock Brake System (ABS) Main Relay Operation Voltage | 10-16 V
Antilock Brake System (ABS) Mode | 4 Channel 4 Sensor
Speed Ring

- Inside Diameter - Front

73.75 mm

2.9035 in

- Inside Diameter - Rear

67 mm

2.6378 in

- Outside Diameter - Front

83.72 mm

3.2961 in

- Outside Diameter - Rear

77 mm

3.0315 in

- Tooth Volume of the Speed Ring - Front

47 EA

- Tooth Volume of the Speed Ring - Rear

34 EA

Wheel Speed Sensor (Front) - Resistance | 998-1,208 Ω
Wheel Speed Sensor (Rear) - Resistance | 2,295-2,500 Ω