For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bleeder Screws | 9 N·m | 80 lb in
Bleeder Valves | 6 N·m | 53 lb in
Booster and Support Bracket-to-Dash Panel Nuts | 24 N·m | 18 lb ft
Booster Pushrod Hex Nut | 16 N·m | 12 lb ft
Booster-to-Support Bracket Nuts | 12 N·m | 9 lb ft
Brake Lines | 16 N·m | 12 lb ft
Brake Pedal-to-Pedal Bracket Hex Nut | 22 N·m | 16 lb ft
Caliper Mounting Bolt | 100 N·m | 74 lb ft
Dust Cover Screws | 4.5 N·m | 40 lb in
Front Brake Hose-to-Caliper Bolt | 40 N·m | 30 lb ft
Hub-to-Disc Screws | 4.5 N·m | 40 lb in
Master Cylinder Attaching Nuts | 18 N·m | 13 lb ft
Proportioning Valves | 40 N·m | 30 lb ft
Trim Panel Screws | 7 N·m | 62 lb in
Wheel Hub Caulking Nut -- Drum Brakes | 190 N·m | 140 lb ft