For 1990-2009 cars

### Stereo Cassette AM/FM Radio

The stereo cassette AM/FM radio is standard and the compact disc player is offered as optional equipment. All audio systems use 4 speakers: 2 speakers mounted in the front doors and 2 speakers mounted behind the rear seats.

### Roof Antenna

The roof antenna is located on the roof and is designed to separate the antenna pole from the antenna base. The antenna pole should be removed to prevent the painting damage before washing the vehicle. The roof antenna cannot be adjusted.

### Front and Rear Speakers

All audio systems use 4 speakers: 2 speakers mounted in the front doors and 2 speakers mounted in the rear deck lid sill plate, on the notchback. On the hatchback, the rear speakers are mounted in the luggage compartment wheelhouse trim panel. A coaxial two-way rear speaker is offered as an option.

### Tape Player and Cassette Care

The head and the capstan are the 2 parts of the tape player that should be cleaned. This service should be performed every 100 hours of cassette operation. In order to clean the head and the capstan, use a cotton swab dipped in rubbing alcohol. A cassette cleaning kit may also be used to clean the head and the capstan. Follow the cleaning kit instructions to clean the tape player. Do not touch the tape head with magnetized tools. If the head becomes magnetized, it will degrade cassettes played in the player. No service is performed on the cassettes. The cassette manufacturer handles warranties of the cassettes. Store cassettes away from extreme heat and direct sunlight.

### Compact Disc Care

Handle discs carefully. Store the discs in protective cases away from the sun, heat, and dust. If the surface is soiled, dampen a clean, soft cloth in a solution of mild neutral detergent and wipe the disc clean.