For 1990-2009 cars

## Fluid and Lubricant Recommendations USA and Canada

The Recommended Fluids and Lubricants information will be found in the Owner's Manual. Refer to the Maintenance Schedule subsection of the Owner's Manual.

You may be able to use the Search information function using the words Fluids or Lubricants.

## Fluid and Lubricant Recommendations Holden

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO JWS 3309 or conforming to Holden spec HN2414
Brake Fluid and Clutch Fluid | DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | DEX-COOL®
Engine Oil |

• | SAE 5W/30 or 10W/30

• | API SL or SM

• | ILSAC GF-3 or GF-4

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle | SAE 75W/90
Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® III
Weatherstrips | Silicone Grease

## Fluid and Lubricant Recommendations Except Canada, Holden, USA

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | ESSO JWS 3309 or Total-ISU Fluid III G
Automatic Transaxle Shift Linkage | Engine Oil
Brake Fluid and Clutch Fluid | DOT-3 or DOT-4
Clutch Linkage Pivot Points | Engine Oil
Engine Coolant | DEX-COOL® Coolant
Engine Oil |

• | SAE 5W-30

• | API SM

• | ILSAC GF-IV

Floor Shift Linkage Points | Engine Oil
Hood and Door Hinges Fuel Door Hinge Rear Compartment Lid Hinges | Engine Oil
Hood Latch Assembly

- Pivots and Spring Anchor

Engine Oil

- Release Pawl

Multipurpose type grease meeting requirements NLGI No. 1 or 2

Key Lock Cylinders | Silicone Lubricant
Manual Transaxle

- 1.2L DOHC Engine

SAE 75W-85

- 1.4L DOHC Engine

SAE 75W-90

- 1.5L SOHC Engine

SAE 75W-90

Manual Transaxle Shift Linkage | Multipurpose type grease meeting requirements NLGI No. 1 or 2
Power Steering System | DEXRON® II-D
Weatherstrips | Silicone Grease