For 1990-2009 cars

Caution: Refer to Brake Dust Caution in the Preface section.

1. Visually inspect the drum brake system universal spring (5) for the following conditions:

• | The spring being bent, damaged, or broken at any point along the spring

• | Excessive corrosion

• | Excessive stretching, twisting, or binding

2. If any of the conditions listed were found, the drum brake system universal spring requires replacement.