For 1990-2009 cars

Connector 1: | C100 Engine Harness to the Transmission Harness (MN5/MX0)
Connector 2: | C101 Engine Harness to the Body Harness (L61)
Connector 3: | C101 Engine Harness to the Body Harness (LE5)
Connector 4: | C102 Engine Harness to the Crankshaft Position Jumper (LSJ)
Connector 5: | C110 Forward Lamp Harness to the Right Headlamp Assembly
Connector 6: | C111 Forward Lamp Harness to the Left Headlamp Assembly
Connector 7: | C121 Forward Lamp Harness to the Body Harness
Connector 8: | C160 Engine Harness to the Fuel Injector Harness (L61/LE5)
Connector 9: | C161 Engine Harness to the Body Harness (LSJ)
Connector 10: | C162 Engine Harness to the Ignition Coil Harness (LSJ)
Connector 11: | C164 Engine Harness to the Fuel Injector Harness (LSJ)
Connector 12: | C170 Body Harness to the Right Front WSS Harness (JL4/JL9)
Connector 13: | C171 Body Harness to the Left Front WSS Harness (JL4/JL9)
Connector 14: | C200 I/P Harness to the Body Harness
Connector 15: | C201 I/P Harness to the Body Harness
Connector 16: | C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Coupe)
Connector 17: | C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Sedan/Pontiac G5/and Pursuit)
Connector 18: | C210 I/P Harness to the HVAC Harness
Connector 19: | C275 I/P Harness to the SIR Coil Assembly
Connector 20: | C302 Headliner Harness to Sun Roof Control Module
Connector 21: | C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness (JL4/JL9)
Connector 22: | C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness (w/o JL4/JL9)
Connector 23: | C307 Body Harness to A/T Shift Control Module
Connector 24: | C314 Body Harness to the Passenger Seat Harness (KA1)
Connector 25: | C315 Body Harness to the Driver Seat Harness (KA1)
Connector 26: | C316 Body Harness to the Passenger Seat Harness
Connector 27: | C319 Body Harness to Left Roof Rail Module Harness (ASF)
Connector 28: | C320 Body Harness to Right Roof Rail Module Harness (ASF)
Connector 29: | C321 Body Harness to the Headliner Harness (UE1)
Connector 30: | C321 Body Harness to the Headliner Harness (w/o UE1)
Connector 31: | C400 Battery Cable to the Body Harness
Connector 32: | C401 Body Harness to the Rear Compartment Lamp Harness
Connector 33: | C492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)
Connector 34: | C493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)
Connector 35: | C494 Body Harness to the License and Backup Lamp Harness (Pursuit/G5)
Connector 36: | C495 License Lamp Harness to Right Backup Lamp Assembly (Pursuit/G5)
Connector 37: | C496 License Lamp Harness to Left Backup Lamp Assembly (Pursuit/G5)
Connector 38: | C497 License Lamp Harness to License Lamp Assembly (Pursuit/G5)
Connector 39: | C500 Body Harness to the Driver Door Harness (w/DG7)
Connector 40: | C500 Body Harness to the Left Front Door Harness (w/o DG7)
Connector 41: | C600 Body Harness to the Passenger Door Harness (w/DG7)
Connector 42: | C600 Body Harness to the Right Front Door Harness (w/o DG7)
Connector 43: | C700 Body Harness to the Left Rear Door Harness (Sedan)
Connector 44: | C800 Body Harness to the Right Rear Door Harness (Sedan)

### C100 Engine Harness to the Transmission Harness (MN5/MX0)

#### Connector Part Information

- OEM: 15472125
- Service: 15305857
- Description: 14-Way F Micro-Pack 100W Series (BK)

#### Connector Part Information

- OEM: 15443076
- Service: 12160782
- Description: 20-Way M Micro-Pack 100W Series (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C100 Engine Harness to the Transmission Harness (MN5/MX0)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 1222 | 1-2 Shift Solenoid Valve Control | A | L-GN | 1222 | 1-2 Shift Solenoid Valve Control
B | YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | B | YE/BK | 1223 | 2-3 Shift Solenoid Valve Control
C | OG/BK | 1228 | PC Solenoid Valve High Control (Sol. A) | C | OG/BK | 1228 | PC Solenoid Valve High Control (Sol. A)
D | L-BU/WH | 1229 | PC Solenoid Valve Low Control (Sol. A) | D | L-BU/WH | 1229 | PC Solenoid Valve Low Control (Sol. A)
E | PK | 1039 | Ignition 1 Voltage | E | PK | 1039 | Ignition 1 Voltage
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | YE/BK | 1227 | TFT Sensor Signal | L | YE/BK | 1227 | TFT Sensor Signal
M | TN | 2762 | Low Reference | M | TN | 2762 | Low Reference
N | -- | -- | Not Used | N | -- | -- | Not Used
P | OG | 1226 | Transmission Fluid Pressure Switch Signal C | P | OG | 1226 | Transmission Fluid Pressure Switch Signal C
R | D-BU | 1225 | Transmission Fluid Pressure Switch Signal B | R | D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
S | OG/BK | 1230 | AT ISS High Signal | S | OG/BK | 1230 | AT ISS High Signal
T | TN/BK | 422 | TCC Solenoid Valve Control | T | TN/BK | 422 | TCC Solenoid Valve Control
U | YE | 657 | TCC Release Switch Signal | U | YE | 657 | TCC Release Switch Signal
V | D-BU/WH | 1231 | AT ISS Low Signal | V | D-BU/WH | 1231 | AT ISS Low Signal
W | -- | -- | Not Used | W | -- | -- | Not Used

### C101 Engine Harness to the Body Harness (L61)

#### Connector Part Information

- OEM: 15326861
- Service: 15306396
- Description: 14-Way M GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326856
- Service: 15326820
- Description: 14-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C101 Engine Harness to the Body Harness (L61)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | A | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
B | TN | 2501 | High Speed GMLAN Serial Data Bus- | B | TN | 2501 | High Speed GMLAN Serial Data Bus-
C | L-GN | 24 | Backup Lamp Supply Voltage | C | L-GN | 24 | Backup Lamp Supply Voltage
D | BN | 4 | Accessory Voltage | D | BN | 4 | Accessory Voltage
E | D-GN | 335 | Cooling Fan Relay Control | E | D-GN | 335 | Cooling Fan Relay Control
F | TN | 2501 | High Speed GMLAN Serial Data Bus- | F | TN | 2501 | High Speed GMLAN Serial Data Bus-
G | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | G | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
H | OG/BK | 472 | Inlet Air Temperature Sensor Signal | H | OG/BK | 472 | Inlet Air Temperature Sensor Signal
J | YE | 492 | MASS Air Flow Sensor Signal | J | YE | 492 | MASS Air Flow Sensor Signal
K | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal | K | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
L | BN | 436 | Air Pump Relay Control | L | BN | 436 | Air Pump Relay Control
M | BN/WH | 6354 | Transmission Output Speed Sensor Signal | M | BN/WH | 6354 | Transmission Output Speed Sensor Signal
N | PU/WH | 6356 | Transmission Output Speed Sensor - Low Reference | N | PU/WH | 6356 | Transmission Output Speed Sensor - Low Reference
P | -- | -- | Not Used | P | -- | -- | Not Used

### C101 Engine Harness to the Body Harness (LE5)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C101 Engine Harness to the Body Harness (LE5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | A | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
B | TN | 2501 | High Speed GMLAN Serial Data Bus- | B | TN | 2501 | High Speed GMLAN Serial Data Bus-
C | L-GN | 24 | Backup Lamp Supply Voltage | C | L-GN | 24 | Backup Lamp Supply Voltage
D | BN | 4 | Accessory Voltage | D | BN | 4 | Accessory Voltage

### C102 Engine Harness to the Crankshaft Position Jumper (LSJ)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C102 Engine Harness to the Crankshaft Position Jumper (LSJ)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PU | 574 | Low Reference | A | PU | 574 | Low Reference
B | YE | 573 | CKP Sensor 1 Signal | B | YE | 573 | CKP Sensor 1 Signal

### C110 Forward Lamp Harness to the Right Headlamp Assembly

#### Connector Part Information

- OEM: 12052848
- Service: 12101854
- Description: 6-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052849
- Service: 12101852
- Description: 6-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C110 Forward Lamp Harness to the Right Headlamp Assembly

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 250 | Ground | A | BK | 250 | Ground
B | D-BU | 15 | Right Turn Signal Lamp Supply Voltage | B | L-BU | 15 | Right Turn Signal Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | YE | 712 | Right Headlamp Low Beam Supply Voltage | D | OG | 712 | Right Headlamp Low Beam Supply Voltage
E | L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | E | PK | 311 | Right Headlamp High Beam Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### C111 Forward Lamp Harness to the Left Headlamp Assembly

#### Connector Part Information

- OEM: 12052848
- Service: 12101854
- Description: 6-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052849
- Service: 12101852
- Description: 6-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C111 Forward Lamp Harness to the Left Headlamp Assembly

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 150 | Ground | A | BK | 150 | Ground
B | L-BU | 14 | Left Turn Signal Lamp Supply Voltage | B | L-BU | 14 | Left Turn Signal Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | TN/WH | 312 | Left Headlamp Low Beam Supply Voltage | D | OG | 312 | Left Headlamp Low Beam Supply Voltage
E | D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | E | PK | 711 | Left Headlamp High Beam Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### C121 Forward Lamp Harness to the Body Harness

#### Connector Part Information

- OEM: 15326829
- Service: 88988924
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326833
- Service: 15326833
- Description: 6-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### C121 Forward Lamp Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YE | 1834 | Forward Discriminating Sensor Signal | A | YE | 1834 | Forward Discriminating Sensor Signal
B | TN/OG | 5045 | Discriminating Sensor - Low Reference | B | TN/OG | 5045 | Discriminating Sensor - Low Reference
C | D-GN/WH | 636 | Ambient Air Temperature Sensor Signal | C | D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
D | YE/BK | 61 | Low Reference | D | YE/BK | 61 | Low Reference
E | PK/BK | 109 | Hood Ajar Switch Signal (AP8) | E | TN/BK | 109 | Hood Ajar Switch Signal (AP8)
F | PU | 5531 | Hood Closed Switch Signal (AP8) | F | PU | 5531 | Hood Closed Switch Signal (AP8)

### C160 Engine Harness to the Fuel Injector Harness (L61/LE5)

#### Connector Part Information

- OEM: 15326836
- Service: 88986255
- Description: 8-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326840
- Service: See Catalog
- Description: 8-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C160 Engine Harness to the Fuel Injector Harness (L61/LE5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | TN | 1744 | Fuel Injector 1 Control | A | BK | 1744 | Fuel Injector 1 Control
B | L-GN/BK | 1745 | Fuel Injector 2 Control | B | L-GN/BK | 1745 | Fuel Injector 2 Control
C | PK/BK | 1746 | Fuel Injector 3 Control | C | PK/BK | 1746 | Fuel Injector 3 Control
D | L-BU/BK | 844 | Fuel Injector 4 Control | D | L-BU/BK | 844 | Fuel Injector 4 Control
E | PK/BK | 5292 | Ignition 1 Voltage | E | PK | 139 | Ignition 1 Voltage
F | OG/BK | 469 | Low Reference | F | OG/BK | 469 | Low Reference
G | L-GN | 432 | MAP Sensor Signal | G | L-GN | 432 | MAP Sensor Signal
H | GY | 2704 | 5-Volt Reference | H | GY | 2704 | 5-Volt Reference

### C161 Engine Harness to the Body Harness (LSJ)

#### Connector Part Information

- OEM: 15326835
- Service: 88986452
- Description: 8-Way F GT 150 Series Sealed

#### Connector Part Information

- OEM: 15326839
- Service: 88988566
- Description: 8-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C161 Engine Harness to the Body Harness (LSJ)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 24 | Backup Lamp Supply Voltage | A | L-GN | 24 | Backup Lamp Supply Voltage
B | L-BU | 6118 | IAT 2 Sensor Signal | B | L-BU | 6118 | IAT 2 Sensor Signal
C | D-GN | 335 | Low Speed Cooling Fan Relay Control | C | D-GN | 335 | Low Speed Cooling Fan Relay Control
D | TN | 891 | Boost Gage Signal | D | TN | 891 | Boost Gage Signal
E | GY | 2700 | 5-Volt Reference | E | GY | 2700 | 5-Volt Reference
F | RD/BK | 380 | A/C Refrigerant Pressure Sensor Signal | F | OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
G | BK | 2751 | Ground | G | BK/WH | 2751 | Ground
H | -- | -- | Not Used | H | -- | -- | Not Used

### C162 Engine Harness to the Ignition Coil Harness (LSJ)

#### Connector Part Information

- OEM: 15326835
- Service: 88986452
- Description: 8-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 88988175
- Service: 15326840
- Description: 8-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-G
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A, G: 2/A
- Core/Insulation Crimp: Pins B, C, D, E, F: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C162 Engine Harness to the Ignition Coil Harness (LSJ)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/WH | 5292 | Ignition 1 Voltage | A | PK/WH | 5292 | Ignition 1 Voltage
B | PU | 6413 | Low Reference | B | PU | 6413 | Low Reference
C | BN/WH | 6405 | IC 1 Control | C | BN/WH | 6405 | IC 1 Control
D | D-BU/WH | 6406 | IC 3 Control | D | D-BU/WH | 6406 | IC 3 Control
E | D-GN/WH | 6407 | IC 4 Control | E | D-GN/WH | 6407 | IC 4 Control
F | L-BU/WH | 6408 | IC 2 Control | F | L-BU/WH | 6408 | IC 2 Control
G | BK | 1350 | Ground | G | BK | 1350 | Ground
H | -- | -- | Not Available | H | -- | -- | Not Available

### C164 Engine Harness to the Fuel Injector Harness (LSJ)

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326827
- Service: 89046648
- Description: 5-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C164 Engine Harness to the Fuel Injector Harness (LSJ)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/WH | 5292 | Ignition 1 Voltage | A | PK/WH | 5292 | Ignition 1 Voltage
B | BK | 1744 | Fuel Injector 1 Control | B | BK | 1744 | Fuel Injector 1 Control
C | L-GN/BK | 1745 | Fuel Injector 2 Control | C | L-GN/BK | 1745 | Fuel Injector 2 Control
D | PK/BK | 1746 | Fuel Injector 3 Control | D | PK/BK | 1746 | Fuel Injector 3 Control
E | L-BU/BK | 844 | Fuel Injector 4 Control | E | L-BU/BK | 844 | Fuel Injector 4 Control

### C170 Body Harness to the Right Front WSS Harness (JL4/JL9)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C170 Body Harness to the Right Front WSS Harness (JL4/JL9)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-GN | 872 | Right Front Wheel Speed Sensor Signal | A | D-GN | 872 | Right Front Wheel Speed Sensor Signal
B | TN | 833 | Right Front Wheel Speed Sensor Low Reference | B | TN | 833 | Right Front Wheel Speed Sensor Low Reference

### C171 Body Harness to the Left Front WSS Harness (JL4/JL9)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C171 Body Harness to the Left Front WSS Harness (JL4/JL9)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-BU | 830 | Left Front Wheel Speed Sensor Signal | A | D-GN | 872 | Left Front Wheel Speed Sensor Signal
B | YE | 873 | Left Front Wheel Speed Sensor Low Reference | B | TN | 833 | Left Front Wheel Speed Sensor Low Reference

### C200 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15336219
- Service: 15336219
- Description: 16-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336224
- Service: 15336224
- Description: 16-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Pins: B, E, F, G, K, L, M
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins E, F, G: C/A
- Core/Insulation Crimp: Pins B, K, L: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, J, H
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins H: 2/A
- Core/Insulation Crimp: Pins: A, J: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B, E, F, G, K, L, M
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins G: 2/4
- Core/Insulation Crimp: Pins E, F: E/4
- Core/Insulation Crimp: Pins B, K, L, M: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A, H, J
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C200 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PK/BK | 1503 | Passenger Heated Seat High/Low Signal (KA1) | A | PK/BK | 1503 | Passenger Heated Seat High/Low Signal (KA1)
B | L-BU/BK | 1505 | Passenger Heated Seat Switch Signal (KA1) | B | L-BU/BK | 1505 | Passenger Heated Seat Switch Signal (KA1)
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used
E | L-GN | 200 | Right Front Speaker Output (+) | E | L-GN/BK | 200 | Right Front Speaker Output (+) (UQ3)
L-GN | 200 | Right Front Speaker (+) Output (UQ4)
F | D-GN | 117 | Right Front Speaker Output (-) | F | D-GN/BK | 117 | Right Front Speaker Output (-) (UQ3)
D-GN | 117 | Right Front Speaker Output (-) (UQ4)
G | L-BU/BK | 115 | Right Rear Speaker Output (-) (UQ3) | G | L-BU/BK | 115 | Right Rear Speaker Output (-) (UQ3)
G | L-BU | 115 | Right Rear Speaker Output (-) (UQ4) | G | L-BU | 115 | Right Rear Speaker Output (-) (UQ4)
H | D-BU | 46 | Right Rear Speaker Output (+) | H | D-BU/BK | 46 | Right Rear Speaker Output (+) (UQ3)
D-BU | 46 | Right Rear Speaker Output (+) (UQ4)
J | BARE | 814 | Drain Wire (U2K) | J | BARE | 814 | Drain Wire (U2K)
K | BN/WH | 367 | Left Audio Signal (+) (U2K) | K | BN/WH | 367 | Left Audio Signal (+) (U2K)
L | D-GN/WH | 368 | Right Audio Signal (+) (U2K) | L | D-GN/WH | 368 | Right Audio Signal (+) (U2K)
M | TN/WH | 372 | Audio Common (U2K) | M | TN/WH | 372 | Audio Common (U2K)
N-S | -- | -- | Not Used | N-S | -- | -- | Not Used

### C201 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15448129
- Service: 89046969
- Description: 40-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15475869
- Service: 88988307
- Description: 40-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Pins: A1, A2, A7, B1, B2, B3, B4, B5, B6, B8, B7, B9, B10, B11, C1, C2, C3, C4, C5, C6, D7, C8, C10, C11, C12, D1, C9, D8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins B7, B10, D7: C/A
- Core/Insulation Crimp: Pins C1, A1, A2, A7, B1, B2, B3, B4, B5, B6, B8, B9, B11, C2, C3, C4, C5, C6, C8, C10, C11, C12, D1, C9, D8: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A3, A5, A6, D3, D6
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins D: 62/A
- Core/Insulation Crimp: Pins A3, A5, A6, D3: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1, A2, A7, B1, B2, B3, B4, B5, B6, B8, B9, B11, C1, C2, C3, C4, C6, C8, C10, C9, B7, B10, C11, C12, C5, D1, D7, D8
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B7, B10, C11, C12, D7: 2/4
- Core/Insulation Crimp: Pins B6, B9, C3, C5, C6, D1, D8: E/4
- Core/Insulation Crimp: Pins C1, A1, A2, A7, B1, B2, B3, B4, B5, B8, B11, C2, C4, C8, C10, C9: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A3, A5, A6, D3, D4
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: D6
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C201 I/P Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-BU | 1162 | APP Sensor 2 Signal | A1 | L-BU | 1162 | APP Sensor 2 Signal
A2 | D-BU | 1161 | APP Sensor 1 Signal | A2 | D-BU | 1161 | APP Sensor 1 Signal
A3 | OG/BK | 2061 | Cellular Telephone Voice Low Reference (UE1) | A3 | OG/BK | 2061 | Cellular Telephone Voice Low Reference (UE1)
A4 | PK | 353 | I/P Module Suppression Indicator Control | A4 | PK | 353 | I/P Module Suppression Indicator Control
A5 | GY | 118 | Left Front Speaker Output (-) | A5 | GY | 118 | Left Front Speaker Output (-) (UQ4)
GY/BK | 118 | Left Front Speaker Output (-) (UQ3)
A6 | PK | 339 | Ignition 1 Voltage | A6 | PK | 339 | Ignition 1 Voltage
PK | 339 | Ignition 1 Voltage
A7 | D-GN | 5060 | Low Speed GMLAN Serial Data | A7 | D-GN | 5060 | Low Speed GMLAN Serial Data
A8 | -- | -- | Not Used | A8 | -- | -- | Not Used
B1 | PU | 1272 | Low Reference | B1 | PU | 1272 | Low Reference
B2 | BN | 1271 | Low Reference | B2 | BN | 1271 | Low Reference
B3 | BARE | 813 | Drain Wire (UE1) | B3 | BARE | 813 | Drain Wire (UE1)
B4 | PK/BK | 2062 | Cellular Telephone Voice Signal (UE1) | B4 | PK/BK | 2062 | Cellular Telephone Voice Signal (UE1)
B5 | YE | 575 | Starter Control | B5 | YE | 575 | Starter Control
B6 | PK/BK | 5291 | Ignition 1 Voltage | B6 | PK/BK | 5291 | Ignition 1 Voltage
B7 | D-BU/WH | 346 | Rear Subwoofer Speaker Output (+) (UQ3) | B7 | D-BU/WH | 346 | Rear Subwoofer Speaker Output (+) (UQ3)
B8 | TN | 1274 | 5-Volt Reference | B8 | TN | 1274 | 5-Volt Reference
B9 | BN/WH | 379 | CPP Switch Signal | B9 | BN/WH | 379 | CPP Switch Signal
B10 | L-GN/BK | 1794 | Rear Subwoofer Speaker Output (-) (UQ3) | B10 | L-GN/BK | 1794 | Rear Subwoofer Speaker Output (-) (UQ3)
B11 | WH/BK | 1164 | 5-Volt Reference | B11 | WH/BK | 1164 | 5-Volt Reference
B12 | TN/BK | 723 | SIR Enable Signal - Passenger | B12 | TN/BK | 723 | SIR Enable Signal - Passenger
C1 | PK | 1501 | Driver Heated Seat High/Low Signal (KA1) | C1 | PK | 1501 | Driver Heated Seat High/Low Signal (KA1)
C2 | TN | 891 | Boost Gage Signal (LSJ) | C2 | TN | 891 | Boost Gage Signal (LSJ)
C3 | PU | 420 | TCC Brake Switch/Cruise Control Release Signal (K34) | C3 | PU | 420 | TCC Brake Switch/Cruise Control Release Signal (K34)
C4 | L-BU | 1462 | Heated Seat Switch Signal (KA1) | C4 | L-BU | 1462 | Heated Seat Switch Signal (KA1)
C5 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | C5 | TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
C6 | TN | 2501 | High Speed GMLAN Serial Data Bus- | C6 | TN | 2501 | High Speed GMLAN Serial Data Bus-
C7 | D-GN | 1049 | ECM/PCM/VCM Class 2 Serial Data (LSJ) | C7 | D-GN | 1049 | ECM/PCM/VCM Class 2 Serial Data (LSJ)
C8 | BN/WH | 419 | MIL Control | C8 | BN/WH | 419 | MIL Control
C9 | L-GN | 1715 | Windshield Wiper Switch High Signal | C9 | L-GN | 1715 | Windshield Wiper Switch High Signal
C10 | PK/WH | 1970 | Headlamp Low Beam Relay Control | C10 | PK/WH | 1970 | Headlamp Low Beam Relay Control
C11 | YE | 116 | Left Rear Speaker Output (-) | C11 | YE | 116 | Left Rear Speaker Output (-) (UQ4)
YE/BK | 116 | Left Rear Speaker Output (-) (UQ3)
C12 | BN | 199 | Left Rear Speaker Output (+) | C12 | BN | 199 | Left Rear Speaker Output (+) (UQ4)
BN/BK | 199 | Left Rear Speaker Output (+) (UQ3)
D1 | TN | 201 | Left Front Speaker Output (+) | D1 | TN/BK | 201 | Left Front Speaker Output (+) (UQ3)
TN | 201 | Left Front Speaker Output (+) (UQ4)
D2 | -- | -- | Not Used | D2 | -- | -- | Not Used
D3 | RD/WH | 40 | Battery Positive Voltage | D3 | RD/WH | 40 | Battery Positive Voltage
D3 | RD/WH | 40 | Battery Positive Voltage
D4 | L-BU | 20 | Stop Lamp Switch Signal | D4 | L-BU | 20 | Stop Lamp Switch Signal
D5 | -- | -- | Not Used | D5 | -- | -- | Not Used
D6 | L-BU/BK | 315 | Right Subwoofer Speaker Output (-) (UQ3) | D6 | L-BU/BK | 315 | Right Subwoofer Speaker Output (-) (UQ3)
D7 | D-GN | 1795 | Right Subwoofer Speaker Output (+) (UQ3) | D7 | D-GN | 1795 | Right Subwoofer Speaker Output (+) (UQ3)
D8 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal (MN5/MX0) | D8 | D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal (MN5/MX0)

### C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Coupe)

#### Connector Part Information

- OEM: 15424636
- Service: 15306363
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15424638
- Service: 15306183
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Coupe)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-GN/OG | 3024 | I/P Module Stage 1 Low Control | A1 | OG | 3024 | I/P Module Stage 1 Low Control
A2 | RD/WH | 3025 | I/P Module Stage 1 High Control | A2 | YE | 3025 | I/P Module Stage 1 High Control
B1 | PK/BK | 3026 | I/P Module Stage 2 Low Control | B1 | PU | 3026 | I/P Module Stage 2 Low Control
B2 | L-BU/OG | 3027 | I/P Module Stage 2 High Control | B2 | GY | 3027 | I/P Module Stage 2 High Control

### C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Sedan/Pontiac G5/and Pursuit)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336477
- Service: 15306183
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C202 Passenger Inflatable Restraint I/P Module to the Body Harness (Cobalt Sedan/Pontiac G5/and Pursuit)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | L-GN/OG | 3024 | I/P Module Stage 1 Low Control | A1 | OG | 3024 | I/P Module Stage 1 Low Control
A2 | RD/WH | 3025 | I/P Module Stage 1 High Control | A2 | YE | 3025 | I/P Module Stage 1 High Control
B1 | PK/BK | 3026 | I/P Module Stage 2 Low Control | B1 | PU | 3026 | I/P Module Stage 2 Low Control
B2 | L-BU/OG | 3027 | I/P Module Stage 2 High Control | B2 | GY | 3027 | I/P Module Stage 2 High Control

### C210 I/P Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15326870
- Service: 88953160
- Description: 2-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326874
- Service: 15306379
- Description: 2-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C210 I/P Harness to the HVAC Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 550 | Ground | A | BK | 550 | Ground
B | BN | 141 | Ignition 3 Voltage | B | BN | 141 | Ignition 3 Voltage

### C275 I/P Harness to the SIR Coil Assembly

#### Connector Part Information

- OEM: 15479525
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C275 I/P Harness to the SIR Coil Assembly

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | A1 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
A2 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control | A2 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control
B1 | PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | B1 | PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
B2 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control | B2 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control

### C302 Headliner Harness to Sun Roof Control Module

#### Connector Part Information

- OEM: 12092162
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12092163
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A-C: E/C
- Core/Insulation Crimp: Pins D: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C302 Headliner Harness to Sun Roof Control Module

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 750 | Ground | A | WH | 750 | Ground
B | L-BU | 131 | Sunroof Limit Switch | B | YE | 131 | Sunroof Limit Switch
C | L-GN | 129 | Sunroof Motor Close Control | C | BK | 129 | Sunroof Motor Close Control
D | D-GN/WH | 127 | Sunroof Motor Open Control | D | D-GN | 127 | Sunroof Motor Open Control

### C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness (JL4/JL9)

#### Connector Part Information

- OEM: 12146437/12162144/12176335
- Service: 15305883/12102741/15305944
- Description: 4-Way F 150 (L-GY), 4-Way F 150 (BK), 8-Way F 280 Sealed (WH)

#### Connector Part Information

- OEM: 15326715
- Service: 15326715
- Description: 16-Way M Metri-Pack 150,150, 280 (GY) Series

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A3, B3, C3, D3, F3, G3
- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: Pins A3, C3: C/D
- Core/Insulation Crimp: Pins B3, D3, F3, G3: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: A1, A2, B1, B2, C2, D2
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

- Pins: H3
- Terminal/Tray: 12020116/2
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 1840 | Battery Positive Voltage | 1A | RD/WH | 1840 | Battery Positive Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control | 1B | WH | 1310 | EVAP Canister Vent Solenoid Control
C-D | -- | -- | Not Used | 1C-1D | -- | -- | Not Used
A | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL4/JL9) | 2A | BN | 882 | Right Rear Wheel Speed Sensor Signal (JL4/JL9)
B | WH | 883 | Right Rear Wheel Speed Sensor Low 2B Reference (JL4/JL9) | B2 | WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JL4/JL9)
C | BK | 884 | Left Rear Wheel Speed Sensor Signal (JL4/JL9) | 2C | TN | 884 | Left Rear Wheel Speed Sensor Signal (JL4/JL9)
D | RD | 885 | Left Rear Wheel Speed Sensor Low Reference (JL4/JL9) | 2D | OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JL4/JL9)
A | BK | 850 | Ground | 3A | BK | 850 | Ground
B | TN | 510 | Fuel Sender Low Reference | 3B | TN | 2759 | Fuel Sender Low Reference
C | GY | 120 | Fuel Pump Supply Voltage | 3C | GY | 120 | Fuel Pump Supply Voltage
D | PU | 1589 | Fuel Level Sensor Signal | 3D | PU | 1589 | Fuel Level Sensor Signal
E | -- | -- | Not Used | 3E | -- | -- | Not Used
F | GY/BK | 2709 | 5-Volt Reference | 3F | GY | 2709 | 5-Volt Reference
G | D-GN | 890 | Fuel Tank Pressure Sensor Signal | 3G | D-GN | 890 | Fuel Tank Pressure Sensor Signal
H | BK/WH | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L) | 3H | TN | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L)
3H | TN | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L)

### C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness (w/o JL4/JL9)

#### Connector Part Information

- OEM: 12146439
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (GY)

#### Connector Part Information

- OEM: 15326714
- Service: See Catalog
- Description: 12-Way M Metri-Pack Mixed Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Connector Part Information

- OEM: 12176335
- Service: 15305944
- Description: 8-Way F Metri-Pack 280 Flex Lock Series (WH)

#### Terminal Part Information

- Pins: A, C
- Terminal/Tray: 12110845/4
- Core/Insulation Crimp: A/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: B, D, F, G, H
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins B, F, G, H - E/C
- Core/Insulation Crimp: Pins D - E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1, B1, C1, D1
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

- Pins: A3, C3
- Terminal/Tray: 12084586/4
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: B3, D3, F3, G3
- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: H3
- Terminal/Tray: 12020116/2
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### C305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness (w/o JL4/JL9)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 1840 | Battery Positive Voltage | 1A | RD/WH | 1840 | Battery Positive Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control | 1B | WH | 1310 | EVAP Canister Vent Solenoid Control
C-D | -- | -- | Not Used | 1C-1D | -- | -- | Not Used
A | BK | 850 | Ground | 3A | BK | 850 | Ground
B | OG | 510 | Fuel Sender Low Reference | 3B | TN | 2759 | Fuel Sender Low Reference
C | GY | 120 | Fuel Pump Supply Voltage | 3C | GY | 120 | Fuel Pump Supply Voltage
D | PU | 1589 | Fuel Level Sensor Signal | 3D | PU | 1589 | Fuel Level Sensor Signal
E | -- | -- | Not Used | 3E | -- | -- | Not Used
F | GY/BK | 2709 | 5-Volt Reference | 3F | GY | 2709 | 5-Volt Reference
G | D-GN | 890 | Fuel Tank Pressure Sensor Signal | 3G | D-GN | 890 | Fuel Tank Pressure Sensor Signal
H | BK/WH | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L) | 3H | TN | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L)
3H | TN | 2759 | Fuel Tank Pressure Sensor Low Reference (2.2L/2.4L)

### C307 Body Harness to A/T Shift Control Module

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A-C: E/C
- Core/Insulation Crimp: Pins D: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C307 Body Harness to A/T Shift Control Module

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 8 | Instrument Panel Lamp Supply Voltage | A | -- | 8 | Instrument Panel Lamp Supply Voltage
B | D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage | B | -- | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
C | D-GN/WH | 1932 | Transmission Shift Select Switch (Park) Signal | C | -- | 1932 | Transmission Shift Select Switch (Park) Signal
D | BK | 1250 | Ground | D | -- | 1250 | Ground

### C314 Body Harness to the Passenger Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: See Catalog
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C314 Body Harness to the Passenger Seat Harness (KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 340 | Battery Positive Voltage | A | RD/WH | 340 | Battery Positive Voltage
B | L-BU/BK | 1505 | Passenger Heated Seat Switch Signal | B | L-BU | 1505 | Passenger Heated Seat Switch Signal
C | PK/BK | 1503 | Passenger Heated Seat High/Low Signal | C | PK | 1503 | Passenger Heated Seat High/Low Signal
D | BK | 1250 | Ground | D | BK | 1250 | Ground

### C315 Body Harness to the Driver Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: A, B, C, D
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins A, D: 2/A
- Core/Insulation Crimp: Pins B, C: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C315 Body Harness to the Driver Seat Harness (KA1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD/WH | 340 | Battery Positive Voltage | A | RD/WH | 340 | Battery Positive Voltage
B | L-BU | 1462 | Heated Seat Switch Signal | B | L-BU | 1462 | Heated Seat Switch Signal
C | PK | 1501 | Driver Heated Seat High/Low Signal | C | PK | 1501 | Driver Heated Seat High/Low Signal
D | BK | 1250 | Ground | D | BK | 1250 | Ground

### C316 Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332152
- Service: See Catalog
- Description: 10-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15332158
- Service: 88953270
- Description: 10-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A, B, C, D, E, F, G, J, K
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: H
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C316 Body Harness to the Passenger Seat Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | OG | 1362 | Seat Belt Switch - Right - Signal | A | OG | 1362 | Seat Belt Switch - Right - Signal
B | PK | 915 | 5-Volt Reference | B | PK | 915 | 5-Volt Reference
C | PK | 5057 | Low Reference | C | PK/BN | 5057 | Low Reference
D | PK | 353 | Passenger Air Bag Off Indicator Control | D | L-GN | 353 | Passenger Air Bag Off Indicator Control
E | TN/BK | 723 | Passenger Air Bag On Indicator Control | E | TN/BK | 723 | Passenger Air Bag On Indicator Control
F | YE | 914 | Low Reference | F | YE | 914 | Low Reference
G | PK | 1339 | Ignition 1 Voltage | G | PK | 1339 | Ignition 1 Voltage
H | BK/WH | 1251 | Ground | H | BK/WH | 1251 | Ground
J | PK | 5018 | Occupant Sensor - Serial Data | J | PU | 5018 | Occupant Sensor - Serial Data
K | D-BU | 913 | Passenger Seat Belt Tension Sensor Signal | K | D-BU | 913 | Passenger Seat Belt Tension Sensor Signal

### C319 Body Harness to Left Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: 15306370
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C319 Body Harness to Left Roof Rail Module Harness (ASF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PU/WH | 5019 | Roof Rail Module - Left - High Control | A | D-GN | 5019 | Roof Rail Module - Left - High Control
B | PK | 5020 | Roof Rail Module - Left - Low Control | B | WH | 5020 | Roof Rail Module - Left - Low Control

### C320 Body Harness to Right Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: 15306370
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C320 Body Harness to Right Roof Rail Module Harness (ASF)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | YE/BK | 5021 | Roof Rail Module - Right - High Control | A | YE/BK | 5021 | Roof Rail Module - Right - High Control
B | WH/BK | 5022 | Roof Rail Module - Right - Low Control | B | WH/BK | 5022 | Roof Rail Module - Right - Low Control

### C321 Body Harness to the Headliner Harness (UE1)

#### Connector Part Information

- OEM: 15336219
- Service: 15336219
- Description: 16-Way F GT 150, 280 Series

#### Connector Part Information

- OEM: 15336224
- Service: 15336224
- Description: 16-Way M GT 150, 280 Series

#### Terminal Part Information

- Pins: C, F, G, K, M, N, P, R
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins C: C/A
- Core/Insulation Crimp: Pins F, G, K, M, N, P, R: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, H, J
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins J: 2/A
- Core/Insulation Crimp: Pins A, H: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: S
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: C, F, G, K, M, N, P, R
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins C: 2/4
- Core/Insulation Crimp: Pins R: E/4
- Core/Insulation Crimp: Pins F, G, K, M, N, P: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A, H
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: J, S
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins J: 2/A
- Core/Insulation Crimp: Pins S: A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C321 Body Harness to the Headliner Harness (UE1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | GY | 157 | Courtesy Lamp Control | A | GY | 157 | Courtesy Lamp Control
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BK | 750 | Ground | C | BK | 750 | Ground
D-E | -- | -- | Not Used | D-E | -- | -- | Not Used
F | D-GN/WH | 2514 | Keypad Signal | F | D-GN/WH | 2514 | Keypad Signal
G | L-GN/BK | 2515 | Keypad Supply Voltage | G | L-GN/BK | 2515 | Keypad Supply Voltage
H | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | H | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
J | D-GN | 1301 | RAP Fuse Supply Voltage | J | D-GN | 1301 | RAP Fuse Supply Voltage
D-GN | 1301 | RAP Fuse Supply Voltage
K | BN/WH | 2517 | Keypad Red LED | K | BN/WH | 2517 | Keypad Red LED
L | -- | -- | Not Used | L | -- | -- | Not Used
M | YE/BK | 2516 | Keypad Green LED | M | YE/BK | 2516 | Keypad Green LED
N | GY | 655 | Cellular Telephone Microphone Signal | N | GY | 655 | Cellular Telephone Microphone Signal
P | BARE | 1489 | Drain Wire | P | BARE | 1489 | Drain Wire
R | L-GN | 24 | Backup Lamp Supply Voltage | R | L-GN | 24 | Backup Lamp Supply Voltage
S | PU | 293 | Rear Defog Element Supply Voltage | S | BK | 293 | Rear Defog Element Supply Voltage

### C321 Body Harness to the Headliner Harness (w/o UE1)

#### Connector Part Information

- OEM: 15326900
- Service: 15306380
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326904
- Service: 88988314
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: C, B, D, E
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins C, E: 2/A
- Core/Insulation Crimp: Pins B, D: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B, C, D
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: A, E
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins E: 2/A
- Core/Insulation Crimp: Pins A: A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C321 Body Harness to the Headliner Harness (w/o UE1)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PU | 293 | Rear Defog Element Supply Voltage | A | PU | 293 | Rear Defog Element Supply Voltage
B | GY | 157 | Interior Lamp Control | B | GY | 157 | Interior Lamp Control
C | BK | 750 | Ground | C | BK | 750 | Ground
D | D-BU/WH | 149 | Courtesy Lamp Supply Voltage | D | D-BU/WH | 149 | Courtesy Lamp Supply Voltage
E | D-GN | 1301 | Retained Accessory Power Fuse Supply Voltage | E | D-GN | 1301 | Retained Accessory Power Fuse Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### C400 Battery Cable to the Body Harness

#### Connector Part Information

- OEM: 12160893
- Service: 15306159
- Description: 1-Way F Metri-Pack 800 Series (BK)

#### Connector Part Information

- OEM: 12160894
- Service: See Catalog
- Description: 1-Way M Metri-Pack 800 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12092445/18
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Terminal Part Information

- Terminal/Tray: 12110700/24
- Core/Insulation Crimp: G/3/5
- Release Tool/Test Probe: 12150860/J-35616-45 (YE)

#### C400 Battery Cable to the Body Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | RD | 1 | Battery Positive Voltage | A | RD | 1 | Battery Positive Voltage

### C401 Body Harness to the Rear Compartment Lamp Harness

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A: E/A
- Core/Insulation Crimp: Pins B: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C401 Body Harness to the Rear Compartment Lamp Harness

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 750 | Ground | A | BK | 750 | Ground
B | OG/BK | 737 | Rear Compartment Lamp Control | B | OG/BK | 737 | Rear Compartment Lamp Control

### C492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B, C, D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 750 | Ground | A | BK | 750 | Ground
B | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | B | YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | L-GN | 24 | Backup Lamp Supply Voltage | D | L-GN | 24 | Backup Lamp Supply Voltage

### C493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 850 | Ground | A | BK | 850 | Ground
B | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | B | D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
C | BN | 9 | Park Lamp Supply Voltage | C | BN | 9 | Park Lamp Supply Voltage
D | L-GN | 24 | Backup Lamp Supply Voltage | D | L-GN | 24 | Backup Lamp Supply Voltage

### C494 Body Harness to the License and Backup Lamp Harness (Pursuit/G5)

#### Connector Part Information

- OEM:12160482
- Service: 12160482
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15499806
- Service: 15499806
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C494 Body Harness to the License and Backup Lamp Harness (Pursuit/G5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 24 | Backup Lamp Supply Voltage | A | L-GN | 24 | Backup Lamp Supply Voltage
B | BN | 9 | Park Lamp Supply Voltage | B | BN | 9 | Park Lamp Supply Voltage
C | BK | 750 | Ground | C | BK | 750 | Ground
D | -- | -- | Not Used | D | -- | -- | Not Used

### C495 License Lamp Harness to Right Backup Lamp Assembly (Pursuit/G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C495 License Lamp Harness to Right Backup Lamp Assembly (Pursuit/G5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 24 | Backup Lamp Supply Voltage | A | L-GN | 24 | Backup Lamp Supply Voltage
B | BK | 750 | Ground | B | BK | 750 | Ground

### C496 License Lamp Harness to Left Backup Lamp Assembly (Pursuit/G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C496 License Lamp Harness to Left Backup Lamp Assembly (Pursuit/G5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | L-GN | 24 | Backup Lamp Supply Voltage | A | L-GN | 24 | Backup Lamp Supply Voltage
B | BK | 750 | Ground | B | BK | 750 | Ground

### C497 License Lamp Harness to License Lamp Assembly (Pursuit/G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C497 License Lamp Harness to License Lamp Assembly (Pursuit/G5)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BN | 9 | Tail/License Lamps Supply Voltage | A | BN | 9 | Tail/License Lamps Supply Voltage
B | BK | 750 | Ground | B | BK | 750 | Ground

### C500 Body Harness to the Driver Door Harness (w/DG7)

#### Connector Part Information

- OEM: 15401211
- Service: 88953323
- Description: 40-Way F GT 150, 280 Series (GY)

#### Connector Part Information

- OEM: 15401208
- Service: 88956505
- Description: 40-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Pins: A1, B3, B5, B6, B11, B12, C3, C6, C7, C8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A2, A4, A5
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A3, A6, A7, D2, D3, D6, D7, D4, D5
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins A6: 4/4
- Core/Insulation Crimp: Pins: A3, A7, D2, D3, D6, D7, D4, D5: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1, B3, B5, B6, B11, B12, C3, C6, C7, C8
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B3, B5, B6: E/4
- Core/Insulation Crimp: Pins A1, B11, B12, C3, C6, C7, C8: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A2, A3, A4, A5, A6, A7, D2, D3, D6, D7, D4, D5
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins A3, A7, D2, D3, D6, D7, D4, D5: A/D
- Core/Insulation Crimp: Pins A6: C/D
- Core/Insulation Crimp: Pins A2, A4, A5: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C500 Body Harness to the Driver Door Harness (w/DG7)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | GY | 8 | Instrument Panel Lamp Supply Voltage | A1 | GY | 8 | Instrument Panel Lamp Supply Voltage
A2 | GY | 8 | Instrument Panel Lamp Supply Voltage | A2 | GY | 8 | Instrument Panel Lamp Supply Voltage
GY | 8 | Instrument Panel Lamp Supply Voltage
A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal (Sedan) | A3 | D-BU | 1307 | Power Window Master Switch Lockout Signal (Sedan)
A4 | GY/BK | 118 | Left Front Speaker Output (-) (UQ3) | A4 | GY/BK | 118 | Left Front Speaker Output (-) (UQ3)
A4 | GY | 118 | Left Front Speaker Output (-) (UQ3)
A4 | GY | 118 | Left Front Speaker Output (-) (UQ4) | A4 | GY | 118 | Left Front Speaker Output (-) (UQ4)
A5 | TN/BK | 201 | Left Front Speaker Output (+) (UQ3) | A5 | TN | 201 | Left Front Speaker Output (+) (UQ3)
A5 | TN | 201 | Left Front Speaker Output (+) (UQ3)
A5 | TN | 201 | Left Front Speaker Output (+) (UQ4) | A5 | TN | 201 | Left Front Speaker Output (+) (UQ4)
A6 | BK | 650 | Ground | A6 | BK | 650 | Ground
A7 | D-GN | 801 | RAP Fuse Supply Voltage | A7 | D-GN | 801 | RAP Fuse Supply Voltage
A8 | -- | -- | Not Used | A8 | -- | -- | Not Used
B1-B2 | -- | -- | Not Used | B1-B2 | -- | -- | Not Used
B3 | WH | 682 | Door Lock Lock/Unlock Signal | B3 | WH | 682 | Door Lock Lock/Unlock Signal
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | TN | 694 | Driver Door Lock Actuator Unlock Control | B5 | TN | 694 | Driver Door Lock Actuator Unlock Control
B6 | GY | 295 | Door Lock Actuator Lock Control | B6 | GY | 295 | Door Lock Actuator Lock Control
B7-B10 | -- | -- | Not Used | B7-B10 | -- | -- | Not Used
B11 | WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF) | B11 | WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
B12 | YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF) | B12 | YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF)
C1-C2 | -- | -- | Not Used | C1-C2 | -- | -- | Not Used
C3 | RD/WH | 440 | Battery Positive Voltage | C3 | RD/WH | 440 | Battery Positive Voltage
C4-C5 | -- | -- | Not Used | C4-C5 | -- | -- | Not Used
C6 | PU/WH | 889 | Passenger Mirror Motor Down Control | C6 | PU/WH | 889 | Passenger Mirror Motor Down Control
C7 | WH | 330 | Passenger Mirror Motor Supply Voltage | C7 | WH | 330 | Passenger Mirror Motor Supply Voltage (Coupe)
WH/BK | 330 | Passenger Mirror Motor Supply Voltage (Sedan)
C8 | OG/WH | 881 | Passenger Mirror Motor Right Control | C8 | OG/WH | 881 | Passenger Mirror Motor Right Control
C9-C12 | -- | -- | Not Used | C9-C12 | -- | -- | Not Used
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal | D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
D3 | TN | 167 | Power Window Master Switch Right Front Down Signal | D3 | TN | 167 | Power Window Master Switch Right Front Down Signal
D4 | D-GN | 168 | Power Window Master Switch Left Rear Up Signal (Sedan) | D4 | D-GN/YE | 168 | Power Window Master Switch Left Rear Up Signal (Sedan)
D5 | PU | 169 | Power Window Master Switch Left Rear Down Signal (Sedan) | D5 | PU | 169 | Power Window Master Switch Left Rear Down Signal (Sedan)
D6 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (Sedan) | D6 | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (Sedan)
D7 | PU | 171 | Power Window Master Switch Right Rear Down Signal (Sedan) | D7 | PU/WH | 171 | Power Window Master Switch Right Rear Down Signal (Sedan)
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### C500 Body Harness to the Left Front Door Harness (w/o DG7)

#### Connector Part Information

- OEM: 15336205
- Service: See Catalog
- Description: 12-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336209
- Service: See Catalog
- Description: 12-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C500 Body Harness to the Left Front Door Harness (w/o DG7)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 650 | Ground | A | BK | 650 | Ground
B | WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF) | B | WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
C | YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF) | C | YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF)
D | GY | 8 | Instrument Panel Lamp Supply Voltage | D | GY | 8 | Instrument Panel Lamp Supply Voltage
E | WH | 682 | Door Lock Lock/Unlock Signal | E | WH | 682 | Door Lock Lock/Unlock Signal
F | TN | 694 | Driver Door Lock Actuator Unlock Control | F | TN | 694 | Driver Door Lock Actuator Unlock Control
G | GY | 295 | Door Lock Actuator Lock Control | G | GY | 295 | Door Lock Actuator Lock Control
H-J | -- | -- | Not Used | H | -- | -- | Not Used
K | GY | 118 | Left Front Speaker Output (-) | K | GY | 118 | Left Front Speaker Output (-)
L | TN/BK | 201 | Left Front Speaker Output (+) | L | TN/BK | 201 | Left Front Speaker Output (+)
M | -- | -- | Not Used | M | -- | -- | Not Used

### C600 Body Harness to the Passenger Door Harness (w/DG7)

#### Connector Part Information

- OEM: 15401211
- Service: 88953323
- Description: 40-Way F GT 150, 280 Series (GY)

#### Connector Part Information

- OEM: 15401208
- Service: 88956505
- Description: 40-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Pins: B3, B5, B6, B7, B8, B11, B12, C7
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A2, D4, D5, D6
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D2, D3, D7
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B3, B5, B6, B7, B8, B11, B12, C7
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B3, B5, B6: E/4
- Core/Insulation Crimp: Pins B7, B8, B11, B12, C7: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A2, D2, D3, D4, D5 D7, D6
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins D2, D3, D7: A/D
- Core/Insulation Crimp: Pins A2, D6, D4, D5: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### C600 Body Harness to the Passenger Door Harness (w/DG7)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | GY | 8 | Instrument Panel Lamp Supply Voltage (1) | A2 | GY | 8 | Instrument Panel Lamp Supply Voltage (1)
GY | 8 | Instrument Panel Lamp Supply Voltage (1)
A3-A8 | -- | -- | Not Used | A3-A8 | -- | -- | Not Used
B1-B2 | -- | -- | Not Used | B1-B2 | -- | -- | Not Used
B3 | WH | 682 | Door Lock Lock/Unlock Signal | B3 | WH | 682 | Door Lock Lock/Unlock Signal
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | TN | 294 | Door Lock Actuator Unlock Control | B5 | TN | 294 | Door Lock Actuator Unlock Control
B6 | GY | 295 | Door Lock Actuator Lock Control | B6 | GY | 295 | Door Lock Actuator Lock Control
B7 | OG/WH | 881 | Right Mirror Motor Right Control | B7 | OG/WH | 881 | Right Mirror Motor Right Control
B8 | PU/WH | 889 | Right Mirror Motor Down Control | B8 | PU/WH | 889 | Right Mirror Motor Down Control
B9-B10 | -- | -- | Not Used | B9-B10 | -- | -- | Not Used
B11 | D-GN | 2134 | Right Front Side Impact Sensing Module Signal (ASF) | B11 | D-GN | 2134 | Right Front Side Impact Sensing Module Signal (ASF)
B12 | TN | 2133 | Right Front Side Impact Sensing Module Supply Voltage (ASF) | B12 | TN | 2133 | Right Front Side Impact Sensing Module Supply Voltage (ASF)
C1-C6 | -- | -- | Not Used | C1-C6 | -- | -- | Not Used
C7 | WH | 330 | Right Mirror Motor Supply Voltage | C7 | WH | 330 | Right Mirror Motor Supply Voltage
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal | D2 | L-BU | 166 | Power Window Master Switch Right Front Up Signal
D3 | TN | 167 | Power Window Master Switch Right Front Down Signal | D3 | TN | 167 | Power Window Master Switch Right Front Down Signal
D4 | D-GN/BK | 117 | Right Front Speaker Output (-) (UQ3) | D4 | D-GN | 117 | Right Front Speaker Output (-) (UQ3)
D4 | D-GN | 117 | Right Front Speaker Output (-) (UQ3)
D4 | D-GN | 117 | Right Front Speaker Output (-) (UQ4) | D4 | D-GN | 117 | Right Front Speaker Output (-) (UQ4)
D5 | L-GN/BK | 200 | Right Front Speaker Output (+) (UQ3) | D5 | L-GN | 200 | Right Front Speaker Output (+) (UQ3)
D5 | L-GN | 200 | Right Front Speaker Output (+) (UQ3)
D5 | L-GN | 200 | Right Front Speaker Output (+) (UQ4) | D5 | L-GN | 200 | Right Front Speaker Output (+) (UQ4)
D6 | BK | 650 | Ground | D6 | BK | 650 | Ground
D7 | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | D7 | D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### C600 Body Harness to the Right Front Door Harness (w/o DG7)

#### Connector Part Information

- OEM: 15336205
- Service: See Catalog
- Description: 12-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336209
- Service: See Catalog
- Description: 12-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C600 Body Harness to the Right Front Door Harness (w/o DG7)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BK | 650 | Ground | A | BK | 650 | Ground
B | D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF) | B | D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF)
C | TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF) | C | TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF)
D | GY | 8 | Instrument Panel Lamp Supply Voltage | D | GY | 8 | Instrument Panel Lamp Supply Voltage
E | WH | 682 | Door Lock Lock/Unlock Signal | E | WH | 682 | Door Lock Lock/Unlock Signal
F | TN | 294 | Door Lock Actuator Unlock Control | F | TN | 294 | Door Lock Actuator Unlock Control
G | GY | 295 | Door Lock Actuator Lock Control | G | GY | 295 | Door Lock Actuator Lock Control
H-J | -- | -- | Not Used | H-J | -- | -- | Not Used
K | D-GN | 117 | Right Front Speaker Output (-) | K | D-GN | 117 | Right Front Speaker Output (-)
L | L-GN | 200 | Right Front Speaker Output (+) | L | L-GN | 200 | Right Front Speaker Output (+)
M | -- | -- | Not Used | M | -- | -- | Not Used

### C700 Body Harness to the Left Rear Door Harness (Sedan)

#### Connector Part Information

- OEM: 15336212
- Service: 22715954
- Description: 14-Way F GT 150, 280 Series

#### Connector Part Information

- OEM: 15412364
- Service: 22708236
- Description: 14-Way M GT 150, 280 Series

#### Terminal Part Information

- Pins: B, C
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, G, H
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C700 Body Harness to the Left Rear Door Harness (Sedan)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU | 1307 | Power Window Master Switch Lockout Signal | A | D-BU/WH | 1307 | Power Window Master Switch Lockout Signal
B | TN | 294 | Door Lock Actuator Unlock Control | B | TN | 294 | Door Lock Actuator Unlock Control
C | GY | 295 | Door Lock Actuator Lock Control | C | GY | 295 | Door Lock Actuator Lock Control
D-F | -- | -- | Not Used | D-F | -- | -- | Not Used
G | D-GN | 168 | Power Window Master Switch Left Rear Up Signal | G | D-GN | 168 | Power Window Master Switch Left Rear Up Signal
H | PU | 169 | Power Window Master Switch Left Rear Down Signal | H | PU | 169 | Power Window Master Switch Left Rear Down Signal
J-P | -- | -- | Not Used | J-P | -- | -- | Not Used

### C800 Body Harness to the Right Rear Door Harness (Sedan)

#### Connector Part Information

- OEM: 15336211
- Service: 22715954
- Description: 14-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15401444
- Service: 15401444
- Description: 14-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### C800 Body Harness to the RR Door Harness (Sedan)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | D-BU | 1307 | Power Window Master Switch Lockout Signal (AU3) | A | D-BU/WH | 1307 | Power Window Master Switch Lockout Signal (AU3)
B | TN | 294 | Door Lock Actuator Unlock Control (AU3) | B | TN | 294 | Door Lock Actuator Unlock Control (AU3)
C | GY | 295 | Door Lock Actuator Lock Control (AU3) | C | GY | 295 | Door Lock Actuator Lock Control (AU3)
D-F | -- | -- | Not Used | D-F | -- | -- | Not Used
G | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (AU3) | G | L-GN | 170 | Power Window Master Switch Right Rear Up Signal (AU3)
H | PU | 171 | Power Window Master Switch Right Rear Down Signal (AU3) | H | PU | 171 | Power Window Master Switch Right Rear Down Signal (AU3)
J-P | -- | -- | Not Used | J-P | -- | -- | Not Used