For 1990-2009 cars

## Radiator Surge Tank Outlet Hose/Pipe Replacement LE5, L61

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the underhood electrical center. Refer to Underhood Electrical Center or Junction Block Bracket Replacement.

1 | Radiator Surge Tank Outlet Hose

#### Procedure

Reposition the surge tank outlet hose clamp using J 38185 .

#### Special Tools

J-38185 Hose Clamp Pliers

## Radiator Surge Tank Outlet Hose/Pipe Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the underhood electrical center. Refer to Underhood Electrical Center or Junction Block Bracket Replacement.

1 | Radiator Surge Tank Outlet Hose

#### Procedure

Reposition the surge tank outlet hose clamp using J 38185 .

#### Special Tools

J-38185 Hose Clamp Pliers