For 1990-2009 cars

## Radiator Inlet Hose Replacement LE5, L61

#### Special Tools

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Lower the vehicle.
3. Remove the air cleaner outlet resonator. Refer to Air Cleaner Outlet Duct Replacement.
4. Reposition the radiator inlet hose clamp at the radiator using J 38185 .
5. Remove the radiator inlet hose from the radiator.
6. Reposition the radiator inlet hose clamp at the engine using J 38185 .
7. Remove the radiator inlet hose from the engine.

### Installation Procedure

1. Install the radiator inlet hose to the radiator.
2. Reposition the radiator inlet hose clamp to secure the hose using J 38185 .
3. Install the radiator inlet hose to the engine.
4. Reposition the radiator inlet hose clamp to secure the hose using J 38185 .
5. Install the air cleaner outlet resonator. Refer to Air Cleaner Outlet Duct Replacement.
6. Fill the cooling system. Refer to Cooling System Draining and Filling.

## Radiator Inlet Hose Replacement LNF

#### Special Tools

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Lower the vehicle.
3. Remove the right headlamp. Refer to Headlamp Replacement.
4. Reposition the radiator air baffle.
5. Reposition the radiator inlet hose clamp at the radiator using J 38185 .
6. Remove the radiator inlet hose from the radiator (1).
7. Reposition the radiator inlet hose clamp at the engine using J 38185 .
8. Remove the radiator inlet hose from the engine (1).

### Installation Procedure

1. Install the radiator inlet hose to the radiator (1).
2. Reposition the radiator inlet hose clamp to secure the hose using J 38185 .
3. Install the radiator inlet hose to the engine (1).
4. Reposition the radiator inlet hose clamp to secure the hose using J 38185 .
5. Install the right headlamp. Refer to Headlamp Replacement.
6. Reposition the radiator air baffle.
7. Fill the cooling system. Refer to Cooling System Draining and Filling.