For 1990-2009 cars

# Sunroof Switch Bezel Comes Loose From Headliner (Replace Bezel and Retainer, If Necessary)

Subject: | Sunroof Switch Bezel Comes Loose From Headliner (Replace Bezel and Retainer, If Necessary)

Models: | 2005-2008 Chevrolet Cobalt

| 2005-2006 Pontiac Pursuit (Canada Only)

| 2007-2008 Pontiac G5

This bulletin is being revised to correct the models involved. Please discard Corporate Bulletin Number 05-08-110-006A (Section 08-Body and Accesories).

Do This | Don't Do This
--- | ---
Replace the sunroof bezel and retainer (if necessary). | DO NOT replace the headliner.

### Condition

Some customers may comment that the sunroof switch bezel comes loose from the headliner.

### Cause

This condition may be caused by a broken sunroof switch bezel tab.

### Correction

1. Inspect the sunroof switch bezel retainer. If it appears to be bent, deformed or mutilated, replace the retainer with a new one.
2. Replace the sunroof switch bezel.
3. Firmly push the sunroof switch and bezel into the headliner module in order to secure the bezel to the retainer.

### Parts Information

Part Number | Description
--- | ---
22716443 | Bezel - Sun RF SW
15812992 | Retainer - Sun RF SW BZL

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C2864 | Switch Bezel - Sunroof -- Replace | Use Published Labor Time.