For 1990-2009 cars

# SIR/Airbag Light Illuminated, DTC B0081 (Passenger Presence System (PPS) Code) Stored (Inspect PPS System Connectors)

Subject: | SIR/Airbag Light Illuminated, DTC B0081 (Passenger Presence System (PPS) Code) Stored (Inspect PPS System Connectors)

Models: | 2006-2008 Chevrolet Cobalt

| 2007-2008 Pontiac G5

### Condition

Some customers may comment that the SIR light is illuminated.

Upon investigation, the technician may find DTC B0081 stored (Passenger Presence System code).

### Correction

Technicians are to inspect the electrical connections to all the PPS components.

1. Inspect the PPS module connector, the pressure sensor connector and the seat connector (all located under the front passenger seat).
2. Inspect the connector of the belt tension sensor (BTS) that is part of the retractor assembly (located between the floor pan and the carpet under the front passenger seat).
3. Clear the codes.
4. Verify that the DTC does not reset.

### Warranty Information

For vehicles repaired under warranty use:

Labor Operation | Description | Labor Time
--- | --- | ---
N6624 | Wiring and/or Connector - Occupant Safety - Repair or Replace | Use Published Labor Operation Time