For 1990-2009 cars

Connector 1: | 1-2 Shift Solenoid (1-2SS) Valve (MN5/MXO)
Connector 2: | 2-3 Shift Solenoid (2-3SS) Valve (MN5/MXO)
Connector 3: | A/C Compressor Clutch (C67)
Connector 4: | A/C Refrigerant Pressure Sensor (C67)
Connector 5: | A/T Shift Lock Control Solenoid (MN5/MXO)
Connector 6: | Accelerator Pedal Position (APP) Sensor (L61/LE5)
Connector 7: | Accelerator Pedal Position (APP) Sensor (LNF)
Connector 8: | Air Temperature Actuator
Connector 9: | Ambient Air Temperature Sensor
Connector 10: | Ambient Light Sensor
Connector 11: | Audio Amplifier X1 (UQ3)
Connector 12: | Audio Amplifier X2 (UQ3)
Connector 13: | Audio Amplifier X3 (UQ3)
Connector 14: | Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (MN5/MXO)
Connector 15: | Automatic Transmission Input Shaft Speed (AT ISS) Sensor (MN5/MXO)
Connector 16: | Auxiliary Power Outlet
Connector 17: | Backup Lamp - Left (Cobalt Coupe)
Connector 18: | Backup Lamp - Left (G5 Coupe)
Connector 19: | Backup Lamp - Left (Sedan)
Connector 20: | Backup Lamp - Right (Cobalt Coupe)
Connector 21: | Backup Lamp - Right (G5 Coupe)
Connector 22: | Backup Lamp - Right (Sedan)
Connector 23: | Backup Lamp Switch (M86)
Connector 24: | Battery (-)
Connector 25: | Battery (+)
Connector 26: | Battery Current Sensor
Connector 27: | Blower Motor
Connector 28: | Blower Motor Resistor
Connector 29: | Body Control Module (BCM) X1
Connector 30: | Body Control Module (BCM) X2
Connector 31: | Body Control Module (BCM) X3
Connector 32: | Body Control Module (BCM) X4
Connector 33: | Brake Booster Vacuum Sensor (LNF)
Connector 34: | Brake Fluid Level Switch
Connector 35: | Brake Pedal Position Sensor
Connector 36: | Camshaft Position (CMP) Actuator Solenoid - Exhaust (LE5/LNF)
Connector 37: | Camshaft Position (CMP) Actuator Solenoid - Intake (LE5/LNF)
Connector 38: | Camshaft Position (CMP) Sensor (L61)
Connector 39: | Camshaft Position (CMP) Sensor - Exhaust (LE5/LNF)
Connector 40: | Camshaft Position (CMP) Sensor - Intake (LE5/LNF)
Connector 41: | Cellular Microphone (UE1)
Connector 42: | Center High Mounted Stop Lamp (CHMSL)
Connector 43: | Cigar Lighter (DT4)/Auxiliary Power Outlet (without DT4)
Connector 44: | Clutch Pedal Position (CPP) Sensor (M86/MU3)
Connector 45: | Coolant Level Switch (LNF)
Connector 46: | Cooling Fan - 1 (LNF)
Connector 47: | Cooling Fan - 2 (LNF)
Connector 48: | Cooling Fan Motor (L61/LE5)
Connector 49: | Cooling Fan Resistor (LE5)
Connector 50: | Crankshaft Position (CKP) Sensor
Connector 51: | Data Link Connector (DLC)
Connector 52: | Digital Radio Receiver (U2K)
Connector 53: | Dome Lamp (- CF5)
Connector 54: | Door Ajar Switch - Driver
Connector 55: | Door Ajar Switch - Left Rear (Sedan)
Connector 56: | Door Ajar Switch - Right Front
Connector 57: | Door Ajar Switch - Right Rear (Sedan)
Connector 58: | Door Latch - Driver (AU3)
Connector 59: | Door Latch - Left Rear (Sedan) (AU3)
Connector 60: | Door Latch - Passenger (AU3)
Connector 61: | Door Latch - Right Rear (Sedan) (AU3)
Connector 62: | Door Lock Switch - Driver (AU3)
Connector 63: | Door Lock Switch - Front Passenger (AU3)
Connector 64: | Electronic Brake Control Module (EBCM) (JM4)
Connector 65: | Electronic Brake Control Module (EBCM) (JL4/JL9)
Connector 66: | Electronic Power Steering (EPS) Control Module X1
Connector 67: | Electronic Power Steering (EPS) Control Module X2
Connector 68: | Electronic Power Steering (EPS) Control Module X3
Connector 69: | Engine Control Module (ECM) X1 (L61/LE5)
Connector 70: | Engine Control Module (ECM) X1 (LNF)
Connector 71: | Engine Control Module (ECM) X2 (L61)
Connector 72: | Engine Control Module (ECM) X2 (LE5)
Connector 73: | Engine Control Module (ECM) X2 (LNF)
Connector 74: | Engine Coolant Temperature (ECT) Sensor (L61/LE5)
Connector 75: | Engine Coolant Temperature (ECT) Sensor (LNF)
Connector 76: | Engine Oil Pressure (EOP) Switch
Connector 77: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 78: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Connector 79: | Fog Lamp - Left Front (T37)
Connector 80: | Fog Lamp - Right Front (T37)
Connector 81: | Fog Lamp Switch (T37)
Connector 82: | Fuel Injector 1 (L61/LE5)
Connector 83: | Fuel Injector 1 (LNF)
Connector 84: | Fuel Injector 2 (L61/LE5)
Connector 85: | Fuel Injector 2 (LNF)
Connector 86: | Fuel Injector 3 (L61/LE5)
Connector 87: | Fuel Injector 3 (LNF)
Connector 88: | Fuel Injector 4 (L61/LE5)
Connector 89: | Fuel Injector 4 (LNF)
Connector 90: | Fuel Pump (FP) and Sender Assembly
Connector 91: | Fuel Rail Pressure Sensor (FPS) (LNF)
Connector 92: | Fuel Tank Pressure (FTP) Sensor
Connector 93: | Generator X1 (L61/LE5)
Connector 94: | Generator X1 (LNF)
Connector 95: | Generator X2
Connector 96: | Hazard Switch
Connector 97: | Headlamp High/Low Beam/DRL - Left
Connector 98: | Headlamp High/Low Beam/DRL - Right
Connector 99: | Heated Oxygen Sensor (HO2S) 1 (L61/LE5)
Connector 100: | Heated Oxygen Sensor (HO2S) 1 (LNF)
Connector 101: | Heated Oxygen Sensor (HO2S) 2 (L61/LE5)
Connector 102: | Heated Oxygen Sensor (HO2S) 2 (LNF)
Connector 103: | Heated Seat Element - Driver Back (KA1)
Connector 104: | Heated Seat Element - Driver Cushion (KA1)
Connector 105: | Heated Seat Element - Passenger Back (KA1)
Connector 106: | Heated Seat Element - Passenger Cushion (KA1)
Connector 107: | Heated Seat Module - Driver (KA1)
Connector 108: | Heated Seat Module - Passenger (KA1)
Connector 109: | Heated Seat Switch - Driver (KA1)
Connector 110: | Heated Seat Switch - Passenger (KA1)
Connector 111: | High Pressure Fuel Pump (LNF)
Connector 112: | Hood Ajar Switch (AP3)
Connector 113: | Horn
Connector 114: | Horn Switch
Connector 115: | HVAC Control Module X1
Connector 116: | HVAC Control Module X2
Connector 117: | HVAC Control Module X3
Connector 118: | Ignition Coil/Module 1
Connector 119: | Ignition Coil/Module 2
Connector 120: | Ignition Coil/Module 3
Connector 121: | Ignition Coil/Module 4
Connector 122: | Ignition Lock Cylinder Control Solenoid
Connector 123: | Ignition Switch
Connector 124: | Inflatable Restraint Front End Sensor
Connector 125: | Inflatable Restraint Front Passenger Presence System (PPS) Module
Connector 126: | Inflatable Restraint Front Passenger Presence System (PPS) Sensor
Connector 127: | Inflatable Restraint Instrument Panel (I/P) Module X1
Connector 128: | Inflatable Restraint Instrument Panel (I/P) Module X2
Connector 129: | Inflatable Restraint Passenger Air Bag On/Off Indicator
Connector 130: | Inflatable Restraint Passenger Seat Belt Tension Sensor
Connector 131: | Inflatable Restraint Roof Rail Module - Left (ASF)
Connector 132: | Inflatable Restraint Roof Rail Module - Right (ASF)
Connector 133: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (ASF)
Connector 134: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (without ASF)
Connector 135: | Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)
Connector 136: | Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)
Connector 137: | Inflatable Restraint Steering Wheel Module X1
Connector 138: | Inflatable Restraint Steering Wheel Module X2
Connector 139: | Inflatable Restraint Steering Wheel Module Coil X1
Connector 140: | Inflatable Restraint Steering Wheel Module Coil X2
Connector 141: | Inflatable Restraint Steering Wheel Module Coil X3
Connector 142: | INLINE Fuse - 50 AMP
Connector 143: | Inside Rearview Mirror (UE1)
Connector 144: | Inside Rearview Mirror (without UE1)
Connector 145: | Instrument Panel Cluster (IPC)
Connector 146: | Intake Air Pressure and Temperature Sensor (LNF)
Connector 147: | I/P Dimmer Switch
Connector 148: | Knock Sensor (KS)
Connector 149: | Knock Sensor (KS) 2 (LNF)
Connector 150: | License Lamp
Connector 151: | Manifold Absolute Pressure (MAP) Sensor (L61/LE5)
Connector 152: | Manifold Absolute Pressure (MAP) Sensor (LNF)
Connector 153: | Marker Lamp - Left Front
Connector 154: | Marker Lamp - Left Rear (Coupe)
Connector 155: | Marker Lamp - Left Rear (Sedan)
Connector 156: | Marker Lamp - Right Front
Connector 157: | Marker Lamp - Right Rear (Coupe)
Connector 158: | Marker Lamp - Right Rear (Sedan)
Connector 159: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 160: | Mode Actuator
Connector 161: | Outside Rearview Mirror - Driver (DG7)
Connector 162: | Outside Rearview Mirror - Passenger (DG7)
Connector 163: | Outside Rearview Mirror Switch (DG7)
Connector 164: | Park Brake Switch
Connector 165: | Park/Neutral Position (PNP) Switch (MN5/MXO)
Connector 166: | Park/Turn Signal Lamp - Left Front
Connector 167: | Park/Turn Signal Lamp - Right Front
Connector 168: | Pressure Control (PC) Solenoid Valve (MN5/MXO)
Connector 169: | PRNDL Lamp
Connector 170: | Radio X1
Connector 171: | Radio X2
Connector 172: | Rear Compartment Courtesy Lamp
Connector 173: | Rear Compartment Lid Release Actuator
Connector 174: | Rear Compartment Lid Release Switch
Connector 175: | Rear Window Defogger Grid X1
Connector 176: | Rear Window Defogger Grid X2
Connector 177: | Recirculation Actuator
Connector 178: | Remote Control Door Lock Receiver (RCDLR) (AU0)
Connector 179: | Seat Belt Retractor Pretensioner - Driver
Connector 180: | Seat Belt Retractor Pretensioner - Passenger
Connector 181: | Seat Belt Switch - Driver
Connector 182: | Seat Belt Switch - Passenger
Connector 183: | Secondary Air Injection (AIR) Pump (NU6)
Connector 184: | Secondary Air Injection (AIR) Solenoid (NU6)
Connector 185: | Speaker - Left Front Door (UQ3)
Connector 186: | Speaker - Left Front Door (UQ4)
Connector 187: | Speaker - Left Front Door Tweeter (UQ3)
Connector 188: | Speaker - Left Rear (UQ3)
Connector 189: | Speaker - Left Rear (UQ4)
Connector 190: | Speaker - Right Front Door (UQ3)
Connector 191: | Speaker - Right Front Door (UQ4)
Connector 192: | Speaker - Right Front Door Tweeter (UQ3)
Connector 193: | Speaker - Right Rear (UQ3)
Connector 194: | Speaker - Right Rear (UQ4)
Connector 195: | Speaker - Subwoofer (UQ3)
Connector 196: | Starter X1
Connector 197: | Starter X2 (To Battery)
Connector 198: | Starter X2 (To Generator)
Connector 199: | Steering Angle Sensor (JL4/JL9)
Connector 200: | Steering Wheel Controls - Left (K34)
Connector 201: | Steering Wheel Controls Right (K34 with UK3)
Connector 202: | Sunroof Motor (CF5)
Connector 203: | Sunroof Switch (CF5)
Connector 204: | Tail/Stop and Turn Signal Lamp - Left (Coupe)
Connector 205: | Tail/Stop and Turn Signal Lamp - Left (Sedan)
Connector 206: | Tail/Stop and Turn Signal Lamp - Right (Coupe)
Connector 207: | Tail/Stop and Turn Signal Lamp - Right (Sedan)
Connector 208: | Theft Deterrent Control Module
Connector 209: | Throttle Actuator Control (TAC) Module
Connector 210: | Torque Converter Clutch Pulse Width Modulation (TCC PWM) Solenoid Valve (MN5/MXO)
Connector 211: | Traction Control Switch (JL4/JL9)
Connector 212: | Transmission Control Module (TCM) (MN5/MXO)
Connector 213: | Turbo Bypass Valve Solenoid (LNF)
Connector 214: | Turbocharger Boost Gauge (LNF)
Connector 215: | Turbocharger Boost Pressure Sensor (LNF)
Connector 216: | Turbocharger Wastegate Solenoid (LNF)
Connector 217: | Turn Signal/Multifunction Switch X1
Connector 218: | Turn Signal/Multifunction Switch X2
Connector 219: | Vehicle Communication Interface Module (VCIM) X1 (UE1)
Connector 220: | Vehicle Communication Interface Module (VCIM) X2 (UE1)
Connector 221: | Vehicle Communication Interface Module (VCIM) X3 (UE1)
Connector 222: | Vehicle Speed Sensor (VSS) (L61/LE5)
Connector 223: | Vehicle Speed Sensor (VSS) (LNF)
Connector 224: | Wheel Speed Sensor (WSS) - Left Front (JM4/JL9/JL4)
Connector 225: | Wheel Speed Sensor (WSS) - Left Rear (L61/LE5 with JM4/JL9/JL4)
Connector 226: | Wheel Speed Sensor (WSS) - Left Rear (LNF with JM4/JL9/JL4)
Connector 227: | Wheel Speed Sensor (WSS) - Right Front (JM4/JL9/JL4)
Connector 228: | Wheel Speed Sensor (WSS) - Right Rear (L61/LE5 with JM4/JL9/JL4)
Connector 229: | Wheel Speed Sensor (WSS) - Right Rear (LNF with JM4/JL9/JL4)
Connector 230: | Window Motor - Driver (AU3/DG7)
Connector 231: | Window Motor - Front Passenger (AU3/DG7)
Connector 232: | Window Motor - Left Rear (Sedan) (AU3/DG7)
Connector 233: | Window Motor - Right Rear (Sedan) (AU3/DG7)
Connector 234: | Window Switch - Driver (Coupe) (AU3/DG7)
Connector 235: | Window Switch - Driver X1 (Sedan) (AU3/DG7)
Connector 236: | Window Switch - Driver X2 (Sedan) (AU3/DG7)
Connector 237: | Window Switch - Front Passenger (AU3/DG7)
Connector 238: | Window Switch - Left Rear (Sedan) (AU3/DG7)
Connector 239: | Window Switch - Right Rear (Sedan) (AU3/DG7)
Connector 240: | Windshield Washer Fluid Pump
Connector 241: | Windshield Wiper Motor
Connector 242: | Windshield Wiper/Washer Switch
Connector 243: | Yaw and Lateral Acceleration Sensor (JL4/JL9)

### 1-2 Shift Solenoid (1-2SS) Valve (MN5/MXO)

#### Connector Part Information

- OEM: 15473843
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 1-2 Shift Solenoid (1-2SS) Valve (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 RD | 839 | Ignition 1 Voltage
B | 0.35 L-GN | 1222 | 1-2 Shift Solenoid Valve Control

### 2-3 Shift Solenoid (2-3SS) Valve (MN5/MXO)

#### Connector Part Information

- OEM: 15473843
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### 2-3 Shift Solenoid (2-3SS) Valve (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 RD | 839 | Ignition 1 Voltage
B | 0.35 YE | 1223 | 2-3 Shift Solenoid Valve Control

### A/C Compressor Clutch (C67)

#### Connector Part Information

- OEM: 12162017
- Service: 12101937
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### A/C Compressor Clutch (C67)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 59 | A/C Compressor Clutch Supply Voltage
B | 0.35 BK | 150 | Ground

### A/C Refrigerant Pressure Sensor (C67)

#### Connector Part Information

- OEM: 13532244
- Service: 88988107
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### A/C Refrigerant Pressure Sensor (C67)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 5514 | Low Reference (LNF)
0.5 PU/WH | 6256 | Low Reference (L61, LE5 with M86)
0.5 BK/WH | Low Reference (LE5 with MN5)
2 | 0.5 GY | 2700 | 5-Volt Reference (LNF)
6255 | 5-Volt Reference (L61/LE5)
3 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal

### A/T Shift Lock Control Solenoid (MN5/MXO)

#### Connector Part Information

- OEM: 12047662
- Service: 12102900
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/C
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### A/T Shift Lock Control Solenoid (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
B | 0.5 YE | 1932 | Transmission Shift Select Switch (Park) Signal

### Accelerator Pedal Position (APP) Sensor (L61/LE5)

#### Connector Part Information

- OEM: 15326830
- Service: 88988944
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | 5-Volt Reference - 2
B | 0.35 L-BU | 1162 | APP Sensor 2 Signal
C | 0.35 TN | 1274 | Low Reference
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | APP Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference - 1

### Accelerator Pedal Position (APP) Sensor (LNF)

#### Connector Part Information

- OEM: 15326833
- Service: See Catalog
- Description: 6-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-3A (GY)

#### Accelerator Pedal Position (APP) Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1272 | 5-Volt Reference - 2
B | 0.35 L-BU | 1162 | APP Sensor 2 Signal
C | 0.35 TN | 1274 | Low Reference
D | 0.35 BN | 1271 | Low Reference
E | 0.35 D-BU | 1161 | APP Sensor 1 Signal
F | 0.35 WH/BK | 1164 | 5-Volt Reference - 1

### Air Temperature Actuator

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Air Temperature Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35PK | 339 | Ignition 1 Voltage
6 | 0.35 WH/BK | 1236 | Passenger Air Temperature Door Control
7 | 0.35 BK/WH | 550 | Ground
8 | -- | -- | Not Used
9 | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
10 | 0.35 L-BU/BK | 1688 | 5-Volt Reference - 2

### Ambient Air Temperature Sensor

#### Connector Part Information

- OEM: 12052642
- Service: 12101856
- Description: 2-Way F Metri-Pack 150 Series Sealed (GN)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ambient Air Temperature Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
B | 0.35 YE/BK | 61 | Low Reference

### Ambient Light Sensor

#### Connector Part Information

- OEM: 12059249
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ambient Light Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
B | 0.35 YE/BK | 1138 | DRL Ambient Light Sensor Low Reference

### Audio Amplifier X1 (UQ3)

#### Connector Part Information

- OEM: 15465061
- Service: 88988659
- Description: 8-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Audio Amplifier X1 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 D-BU/WH | 346 | Rear Subwoofer Speaker Output (+)
2 | 0.8 L-GN/BK | 1794 | Rear Subwoofer Speaker Output (-)
3 | 0.8 D-GN | 1795 | Rear Subwoofer Speaker Output (+)
4 | 0.8 L-BU/BK | 315 | Rear Subwoofer Speaker Output (-)
5 | 2 BK/WH | 1051 | Ground
6-7 | -- | -- | Not Used
8 | 2 RD/WH | 640 | Battery Positive Voltage

### Audio Amplifier X2 (UQ3)

#### Connector Part Information

- OEM: 15489823
- Service: 888952777
- Description: 16-Way M 1.5 Series Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2, 11, 12
- Terminal/Tray: 8240-0127/22
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: 3, 4, 9, 10
- Terminal/Tray: 8240-0128/22
- Core/Insulation Crimp: Pins 3, 4: C/A
- Core/Insulation Crimp: Pins 9, 10: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Audio Amplifier X2 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE/BK | 116 | Left Rear Speaker Output (-)
2 | 0.5 BN | 199 | Left Rear Speaker Output (+)
3 | 0.8 D-BU | 46 | Right Rear Speaker Output (+)
4 | 0.8 L-BU/BK | 115 | Right Rear Speaker Output (-)
5-8 | -- | -- | Not Used
9 | 1 D-GN | 117 | Right Front Speaker Output (-)
10 | 1 L-GN | 200 | Right Front Speaker Output (+)
11 | 0.5 TN | 201 | Left Front Speaker Output (+)
12 | 0.5 GY | 118 | Left Front Speaker Output (-)
13-16 | -- | -- | Not Used

### Audio Amplifier X3 (UQ3)

#### Connector Part Information

- OEM: 15416970
- Service: 15394150
- Description: 16-Way F Micro 64 Unsealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Audio Amplifier X3 (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 1999 | Left Rear Low Level Audio Signal (-)
2 | 0.35 TN | 1946 | Right Rear Low Level Audio Signal (-)
3 | 0.35 BN/WH | 599 | Left Rear Low Level Audio Signal (+)
4 | 0.35 D-BU | 546 | Right Rear Low Level Audio Signal (+)
5-7 | -- | -- | Not Used
8 | 0.35 PK | 314 | Radio On Signal
9 | 0.35 L-GN/WH | 512 | Right Front Low Level Audio Signal (+)
10 | 0.35 D-GN | 1947 | Left Front Low Level Audio Signal (-)
11 | 0.35 L-GN | 1948 | Right Front Low Level Audio Signal (-)
12 | 0.35 TN | 511 | Left Front Low Level Audio Signal (+)
13-15 | -- | -- | Not Used
16 | 0.35 L-GN | 1011 | Remote Radio Control Signal

### Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (MN5/MXO)

#### Connector Part Information

- OEM: 15480749
- Service: Non-Serviceable
- Description: 6-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Fluid Pressure (TFP) Manual Valve Position Switch (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 D-BU | 1225 | TFP Switch Signal B
C | 0.35 OG | 1226 | TFP Switch Signal C
D | 0.35 WH | 1804 | Torque Converter Clutch Release Switch Signal
E | 0.35 BN | 1227 | Transmission Fluid Temperature (TFT) Sensor Signal
F | 0.35 GY | 452 | Low Reference

### Automatic Transmission Input Shaft Speed (AT ISS) Sensor (MN5/MXO)

#### Connector Part Information

- OEM: 15473843
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series P2S (NA)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Automatic Transmission Input Shaft Speed (AT ISS) Sensor (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1230 | Input Speed Sensor (ISS) High Signal
B | 0.5 D-GN | 1231 | ISS Low Signal

### Auxiliary Power Outlet

#### Connector Part Information

- OEM: 12176446
- Service: 15305985
- Description: 3-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Pins: A, C (- DT4)
- Terminal/Tray: 12110842/4
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A, C (DT4)
- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Auxiliary Power Outlet

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD/WH | 40 | Battery Positive Voltage
B | -- | -- | Not Used
C | 1 BK | 1250 | Ground

### Backup Lamp - Left (Cobalt Coupe)

#### Connector Part Information

- OEM: 15491912
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Backup Lamp - Left (Cobalt Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
2 | 0.5 BK | 750 | Ground

### Backup Lamp - Left (G5 Coupe)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Backup Lamp - Left (G5 Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 24 | Backup Lamp Supply Voltage
B | 0.5 BK | 750 | Ground

### Backup Lamp - Left (Sedan)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Backup Lamp - Left (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
B | 0.5 BK | 750 | Ground
0.5 BK | 750 | Ground

### Backup Lamp - Right (Cobalt Coupe)

#### Connector Part Information

- OEM: 15491912
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Right (Cobalt Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
2 | 0.5 BK | 850 | Ground

### Backup Lamp - Right (G5 Coupe)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Backup Lamp - Right (G5 Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 24 | Backup Lamp Supply Voltage
B | 0.5 BK | 750 | Ground

### Backup Lamp - Right (Sedan)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

- Pins: B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Backup Lamp - Right (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
B | 0.5 BK | 850 | Ground
0.5 BK | 850 | Ground

### Backup Lamp Switch (M86)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Backup Lamp Switch (M86)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 539 | Ignition 1 Voltage
B | 0.5 L-GN | 24 | Backup Lamp Supply Voltage

### Battery (-)

#### Terminal Part Information

- Terminal: R61014-002
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (-)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
- | 32 BK | 50 | Ground

### Battery (+)

#### Terminal Part Information

- Terminal: R3311-033
- Core/Insulation Crimp: N/A
- Description: Battery Terminal

#### Battery (+)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 50 RD | 1 | Battery Positive Voltage
5 RD | 1 | Battery Positive Voltage

### Battery Current Sensor

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Battery Current Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 596 | 5-Volt Reference - 1
B | 0.5 BK | 650 | Sensor Low Reference (Coupe)
0.35 BK | 650 | Sensor Low Reference (Sedan)
C | 0.35 WH | 5075 | Current Sensor Signal

### Blower Motor

#### Connector Part Information

- OEM: 12064749
- Service: 12101888
- Description: 2-Way F Metri-Pack 480 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3 OG | 52 | High Blower Motor Control
B | 3 BN | 141 | Ignition 3 Voltage

### Blower Motor Resistor

#### Connector Part Information

- OEM: 12129566
- Service: 15305940
- Description: 4-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Blower Motor Resistor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 TN | 63 | Blower Motor Medium 1 Control
B | 2 L-BU | 72 | Medium 2 Blower Motor Control
C | 3 OG | 52 | High Blower Motor Control
D | 2 YE | 60 | Low Blower Motor Control

### Body Control Module (BCM) X1

#### Connector Part Information

- OEM: 15393122
- Service: 88987847
- Description: 72-Way F Micro 64 (GY)

#### Terminal Part Information

- Pins: 1, 6-8, 13-20, 22, 26, 33, 35, 36, 44, 47, 51, 54, 55, 57, 60-68, 70
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

- Pins: 31
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal (Sedan)
2 | -- | -- | Not Used
3 | 0.35 PU | 5531 | Hood Closed Switch Signal (AP8)
4 | 0.35 PK/BK | 109 | Hood Ajar Switch Signal (AP8)
5 | -- | -- | Not Used
6 | 0.35 WH | 682 | Door Lock Lock/Unlock Signal
7 | 0.35 WH | 682 | Door Lock Lock/Unlock Signal
8 | 0.35 WH | 1080 | Park Lamp Relay Control
9-12 | -- | -- | Not Used
13 | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
14 | 0.35 L-BU | 1134 | Park Brake Switch Signal
15 | 0.35 YE | 5199 | Run/Crank Relay Coil Control
16 | 0.35 WH | 193 | Rear Defog Relay Control
17 | 0.5 D-BU | 15 | Right Front Turn Signal Lamp Supply Voltage
18 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
19 | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
20 | 0.35 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal (Sedan)
21 | -- | -- | Not Used
22 | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
23-25 | -- | -- | Not Used
26 | 0.35 L-GN | 1478 | Coolant Level Switch Signal (LNF)
27-30 | -- | -- | Not Used
31 | 0.35 WH | 5065 | CHMSL Relay Coil Supply Voltage
32 | -- | -- | Not Used
33 | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage (MN5/MX0)
34 | -- | -- | Not Used
35 | 0.35 L-BU | 14 | Left Front Turn Signal Lamp Supply Voltage
36 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data (UE1)
37-39 | -- | -- | Not Used
40 | 0.35 L-BU | 1788 | Traction Control Switch Signal (JL4/JL9)
41-43 | -- | -- | Not Used
44 | 0.35 TN/WH | 1969 | Headlamp High Beam Relay Control
45-46 | -- | -- | Not Used
47 | 0.5 YE | 196 | Windshield Wiper Motor Park Switch Signal
48-50 | -- | -- | Not Used
51 | 0.35 D-GN | 113 | Windshield Wiper Switch Signal
52-53 | -- | -- | Not Used
54 | 0.35 YE | 317 | Fog Lamp Relay Control (T37)
55 | 0.35 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
56 | -- | -- | Not Used
57 | 0.35 BN | 253 | Trunk Release Relay Control
58-59 | -- | -- | Not Used
60 | 0.35 TN | 28 | Horn Relay Control
61 | 0.5 BK | 1250 | Ground
62 | 0.35 RD/WH | 1240 | Battery Positive Voltage (without LNF)
63 | 0.35 GY | 596 | 5-Volt Reference - 1 (without LNF)
64 | 0.5 BK | 650 | Ground (without LNF)
65-66 | -- | -- | Not Used
67 | 0.35 YE/BK | 61 | Low Reference
68 | 0.35 WH | 5075 | Current Sensor Signal (without LNF)
69 | -- | -- | Not Used
70 | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
71 | 0.35 L-GN/BK | 592 | DRL Relay Control
72 | -- | -- | Not Used

### Body Control Module (BCM) X2

#### Connector Part Information

- OEM: 15393121
- Service: 88987848
- Description: 72-Way F Micro 64 (GY)

#### Terminal Part Information

- Pins: 1-5, 9, 10-12, 14-17, 19, 20, 26, 38, 44, 47, 51, 54-58, 61, 62, 66-69, 72
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

- Pins: 70
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN/WH | 2500 | High Speed GMLAN Serial Data (+)
2 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
3 | 0.35 YE | 10 | Headlamp Switch Signal
4 | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
5 | 0.35 BN/WH | 301 | Park Lamp Switch On Signal
6-8 | -- | -- | Not Used
9 | 0.35 WH | 111 | Hazard Switch Signal
10 | 0.35 TN | 1576 | Rear Compartment Lid Release Switch
11 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
12-13 | -- | -- | Not Used
14 | 0.35 TN | 28 | Horn Relay Control
15 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
16 | 0.35 OG | 192 | Front Fog Lamp Switch Signal (T37)
17 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
18 | 0.35 WH | 5359 | 5-Volt Reference
19 | 0.5 BN | 2501 | High Speed GMLAN Serial Data (-)
20 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-)
21-25 | -- | -- | Not Used
26 | 0.35 D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal
27-30 | -- | -- | Not Used
31 | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
32-37 | -- | -- | Not Used
38 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
39-43 | -- | -- | Not Used
44 | 0.35 L-GN/BK | 1137 | DRL Ambient Light Sensor Signal
45-46 | -- | -- | Not Used
47 | 0.35 YE/BK | 1138 | DRL Ambient Light Sensor Low Reference
48-50 | -- | -- | Not Used
51 | 0.35 BN | 1356 | Flash To Pass Switch Signal
52-55 | -- | -- | Not Used
56 | 0.35 WH | 1390 | Off/Run/Crank Voltage
57 | 0.35 GY | 112 | Windshield Wiper Switch Signal
58 | 0.35 PU | 719 | Low Reference
59 | 0.35 BN | 5360 | Low Reference
60 | -- | -- | Not Used
61 | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
62 | 0.35 WH/BK | 1073 | Ignition Key Resistor Signal
63-65 | -- | -- | Not Used
66 | 0.35 YE/BK | 1418 | Left Rear Turn Signal Switch Signal
67 | 0.35 D-GN/WH | 1419 | Right Rear Turn Signal Switch Signal
68 | 0.35 L-BU | 292 | Rear Defog Switch Signal
69 | 0.35 L-GN | 66 | A/C Request Signal (C67)
70 | -- | -- | Not Used
71 | 0.35 PU | 5234 | Passenger Seatbelt Reminder
72 | 0.35 WH | 193 | Rear Defog Relay Control

### Body Control Module (BCM) X3

#### Connector Part Information

- OEM: 15492675
- Service: 15404825
- Description: 41-Way F Metri-Pack 280, 800 Series (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3)
A2 | 0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3) (Sedan)
0.5 TN | 294 | Door Lock Actuator Unlock Control (AU3) (Sedan)
A3 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
A4 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3) (Driver)
0.5 GY | 295 | Door Lock Actuator Lock Control (AU3) (Passenger)
A5 | 0.5 GY | 295 | Door Lock Actuator Lock Control (AU3) (Sedan)
0.5 GY | 295 | Door Lock Actuator Lock Control (AU3) (Sedan)
A6 | -- | -- | Not Used
A7 | 0.35 BN | 9 | Park Lamp Supply Voltage
A8 | 0.35 PK | 339 | Run/Crank Ignition 1 Voltage (KA1)
A9 | 0.5 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
A10 | 0.5 GY | 157 | Courtesy Lamp Control
A11 | -- | -- | Not Used
A12 | 0.5 D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
B1 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
B2 | -- | -- | Not Used
B3 | 0.35 RD/WH | 1240 | Battery Positive Voltage (L61 or LE5)
0.5 RD/WH | 1240 | Battery Positive Voltage
B4 | -- | -- | Not Used
B5 | 0.35 BN | 4 | Accessory Voltage
0.35 BN | 4 | Accessory Voltage (MN5)
B6-B7 | -- | -- | Not Available
B8-B11 | -- | -- | Not Used
B12 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (L61/LE5)
0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (L61/LE5)
C1-C2 | -- | -- | Not Available
C3 | 1 D-GN | 1301 | Retained Accessory Power Fuse Supply Voltage
C4 | -- | -- | Not Used
C5 | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
C6-C7 | -- | -- | Not Available
C8-C11 | -- | -- | Not Used
C12 | 0.35 OG | 228 | Windshield Washer Pump Control
D1 | 5 RD/BK | 142 | Battery Positive Voltage
D2 | -- | -- | Not Available
D3 | -- | -- | Not Used
D4 | 0.5 RD/WH | 840 | Battery Positive Voltage
D5 | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D6 | 3 PK | 739 | Run/Crank Ignition 1 Voltage
D7 | 0.35 PK | 1339 | Ignition 1 Voltage
0.35 PK | 1339 | Ignition 1 Voltage
D8-D9 | -- | -- | Not Used
D10 | 3 RD/BK | 442 | Battery Positive Voltage
D11 | -- | -- | Not Used
D12 | 3 RD/WH | 242 | Battery Positive Voltage

### Body Control Module (BCM) X4

#### Connector Part Information

- OEM: 15492668
- Service: 88988776
- Description: 68-Way F Metri-Pack 280 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Body Control Module (BCM) X4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 2 RD/WH | 640 | Battery Positive Voltage (UQ3)
A2-A12 | -- | -- | Not Used
B1 | 0.35 OG | 228 | Windshield Washer Pump Control
B2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
B3-B12 | -- | -- | Not Used
C1 | 0.5 RD/WH | 1440 | Battery Positive Voltage
C2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C3-C5 | -- | -- | Not Used
C6-C7 | -- | -- | Not Available
C8 | 0.35 BN | 4 | Accessory Voltage
C9-C10 | -- | -- | Not Used
C11 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C12 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
D1 | 0.35 RD/WH | 1040 | Battery Positive Voltage
D2 | -- | -- | Not Used
D3 | 0.35 YE | 5199 | Run/Crank Voltage
D4 | 3 BN | 141 | Ignition 3 Voltage
D5 | -- | -- | Not Used
D6-D7 | -- | -- | Not Available
D8-D9 | -- | -- | Not Used
D10 | 1 RD/WH | 1140 | Battery Positive Voltage
0.5 RD/WH | 1140 | Battery Positive Voltage
D11-D12 | -- | -- | Not Used
E1-E5 | -- | -- | Not Used
E6 | 0.35 PK | 439 | Ignition 1 Voltage
0.35 PK | 439 | Ignition 1 Voltage (LNF)
E7-E11 | -- | -- | Not Used
E12 | 2 BK | 550 | Ground
F1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
0.35 RD/WH | 1540 | Battery Positive Voltage
F2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (LNF)
F3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (KA1)
0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (KA1)
F4 | 0.35 PK | 339 | Ignition 1 Voltage
F5 | 0.5 PK | 339 | Ignition 1 Voltage
F6 | 0.5 PK | 339 | Ignition 1 Voltage
F7-F8 | -- | -- | Not Used
F9 | 0.55 PK | 1539 | Ignition 1 Voltage
0.35 PK | 1539 | Ignition 1 Voltage (K34)
F10-F12 | -- | -- | Not Used

### Brake Booster Vacuum Sensor (LNF)

#### Connector Part Information

- OEM: 15365614
- Service: See Catalog
- Description: 3-Way F 1.5 Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Brake Booster Vacuum Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 6257 | 5-Volt Reference
2 | 0.5 L-GN/BK | 6258 | Low Reference
3 | 0.5 D-BU | 1809 | Brake Vacuum Sensor Signal

### Brake Fluid Level Switch

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A: E/4
- Core/Insulation Crimp: Pins B: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Brake Fluid Level Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 849 | Brake Fluid Level Sensor Signal
B | 0.5 BK | 650 | Ground

### Brake Pedal Position Sensor

#### Connector Part Information

- OEM: 15332132
- Service: See Catalog
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Brake Pedal Position Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH | 5359 | 5-Volt Reference
B | 0.35 YE | 5361 | Brake Pedal Position Sensor Signal
C | 0.35 BN | 5360 | Low Reference

### Camshaft Position (CMP) Actuator Solenoid - Exhaust (LE5/LNF)

#### Connector Part Information

- OEM: 15336004
- Service: 15306187
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Actuator Solenoid - Exhaust (LE5/LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-GN | 5282 | CMP Actuator Solenoid Control Exhaust (LE5)
0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (LNF)
B | 0.5 BN/WH | 6754 | Low Reference (LE5)
0.5 L-GN | 5282 | Low Reference (LNF)

### Camshaft Position (CMP) Actuator Solenoid - Intake (LE5/LNF)

#### Connector Part Information

- OEM: 15335987
- Service: 15306430
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Camshaft Position (CMP) Actuator Solenoid - Intake (LE5/LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 5284 | CMP Actuator Solenoid Control Intake (LE5)
0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (LNF)
B | 0.5 BN | 6753 | Low Reference (LE5)
0.5 PU | 5284 | Low Reference (LNF)

### Camshaft Position (CMP) Sensor (L61)

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor (L61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 5300 | 5-Volt Reference
B | 0.5 TN | 5301 | Low Reference
C | 0.5 OG | 5275 | CMP Sensor Signal

### Camshaft Position (CMP) Sensor - Exhaust (LE5/LNF)

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Exhaust (LE5/LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE/BK | 5297 | 5-Volt Reference (LE5)
0.35 GY | 705 | 5-Volt Reference 2 (LNF)
B | 0.35 GY | 5296 | Low Reference (LE5)
0.35 TN | 552 | Low Reference (LNF)
C | 0.35 D-GN | 5273 | CMP Sensor Signal

### Camshaft Position (CMP) Sensor - Intake (LE5/LNF)

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Intake (LE5/LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 5300 | 5-Volt Reference (LE5)
0.5 GY | 705 | 5-Volt Reference 2 (LNF)
B | 0.5 TN | 5301 | Low Reference (LE5)
552 | Low Reference (LNF)
C | 0.5 OG | 5275 | CMP Sensor Signal

### Cellular Microphone (UE1)

#### Connector Part Information

- OEM: 12047663
- Service: 12058709
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Cellular Microphone (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | BARE | 1489 | Drain Wire
B | 0.35 GY | 655 | Cellular Microphone Signal

### Center High Mounted Stop Lamp (CHMSL)

#### Connector Part Information

- OEM: 12059110
- Service: 88953271
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Center High Mounted Stop Lamp (CHMSL)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 20 | Stop Lamp Supply Voltage
B | 0.8 BK | 750 | Ground

### Cigar Lighter (DT4)/Auxiliary Power Outlet (without DT4)

#### Connector Part Information

- OEM: 12176445
- Service: 15305919
- Description: 3-Way F Metri-Pack 280 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 12110844/4
- Core/Insulation Crimp: Pins A: E/A
- Core/Insulation Crimp: Pins C: C/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Cigar Lighter (DT4)/Auxiliary Power Outlet (without DT4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 RD/WH | 40 | Battery Positive Voltage
B | -- | -- | Not Used
C | 0.8 BK | 550 | Ground

### Clutch Pedal Position (CPP) Sensor (M86/MU3)

#### Connector Part Information

- OEM: 15332132
- Service: See Catalog
- Description: 3-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Clutch Pedal Position (CPP) Sensor (M86/MU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 7360 | Low Reference (M86)
0.5 TN | 2759 | Low Reference (MU3)
B | 0.35 L-GN | 6338 | Clutch Pedal Position Sensor Signal
C | 0.35 D-BU/WH | 7361 | 5-Volt Reference (M86)
0.5 GY | 2709 | 5-Volt Reference (MU3)

### Coolant Level Switch (LNF)

#### Connector Part Information

- OEM: 12052641
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Coolant Level Switch (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN | 1478 | Coolant Level Switch Signal
B | 0.5 BK | 650 | Ground

### Cooling Fan - 1 (LNF)

#### Connector Part Information

- OEM: 15383305
- Service: 88988311
- Description: 2-Way F Metri-Pack 480 Series Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: 12191448/3
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 15315247/J-35616-40 (BU)

#### Cooling Fan - 1 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 L-BU | 409 | Cooling Fan Motor Supply Voltage
2 | -- | -- | Not Available
3 | 3 WH | 504 | Cooling Fan Motor Low Reference

### Cooling Fan - 2 (LNF)

#### Connector Part Information

- OEM: 15383305
- Service: 88988311
- Description: 2-Way F Metri-Pack 480 Series Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: 12191448/3
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 15315247/J-35616-40 (BU)

#### Cooling Fan - 2 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 GY | 532 | Cooling Fan Motor Supply Voltage
2 | -- | -- | Not Available
3 | 3 BK | 1050 | Ground

### Cooling Fan Motor (L61/LE5)

#### Connector Part Information

- OEM: 15451371
- Service: 88988310
- Description: 3-Way F Metri-Pack 480 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191448/3
- Core/Insulation Crimp: F/3
- Release Tool/Test Probe: 15315247/J-35616-40 (BU)

#### Cooling Fan Motor (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 L-BU | 409 | Cooling Fan Motor Supply Voltage (L61)
3 YE | 5358 | Auxiliary Cooling Fan Motor Supply Voltage (LE5)
2 | 3 GY | 532 | Cooling Fan Motor Supply Voltage
3 | 3 BK | 1050 | Ground

### Cooling Fan Resistor (LE5)

#### Connector Part Information

- OEM: 15486525
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Cooling Fan Resistor (LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 L-BU | 409 | Cooling Fan Motor Supply Voltage
2 | 3 YE | 5358 | Auxiliary Cooling Fan Motor Supply Voltage

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 15325738
- Service: 88987978
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Crankshaft Position (CKP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-GN | 2867 | 5-Volt Reference
2 | 0.5 PU | 574 | Low Reference
3 | 0.5 YE | 573 | Crankshaft Position Sensor Signal

### Data Link Connector (DLC)

#### Connector Part Information

- OEM: 15488184
- Service: 15317575
- Description: 16-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Data Link Connector (DLC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2-3 | -- | -- | Not Used
4 | 0.5 BK | 550 | Ground
5 | 0.5 BK/WH | 1051 | Signal Ground
6 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data (+)
7-13 | -- | -- | Not Used
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data (-)
15 | -- | -- | Not Used
16 | 0.5 RD/WH | 40 | Battery Positive Voltage

### Digital Radio Receiver (U2K)

#### Connector Part Information

- OEM: 15416970
- Service: 15394150
- Description: 16-Way F Micro 64 Modular (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Digital Radio Receiver (U2K)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 367 | Left Audio Signal (+)
3 | 0.35 D-GN/WH | 368 | Right Audio Signal (+)
4 | -- | -- | Not Used
5 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
6-8 | -- | -- | Not Used
9 | 0.5 BK | 650 | Ground
10 | 0.35 TN/WH | 372 | Audio Common (-)
11 | BARE | 814 | Drain Wire
12-15 | -- | -- | Not Used
16 | 0.5 RD/WH | 1240 | Battery Positive Voltage

### Dome Lamp (- CF5)

#### Connector Part Information

- OEM: 12045813
- Service: 12101889
- Description: 4-Way F Metri-Pack 150 Series (WH)

#### Terminal Part Information

- Pins: A, B, D
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Dome Lamp (- CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 GY | 157 | Interior Lamp Control
C | -- | -- | Not Used
D | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Door Ajar Switch - Driver

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A: E/4
- Core/Insulation Crimp: Pins B: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Ajar Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY/BK | 745 | Left Front Door Ajar Switch Signal
B | 0.35 BK | 650 | Ground

### Door Ajar Switch - Left Rear (Sedan)

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A: E/4
- Core/Insulation Crimp: Pins B: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Ajar Switch - Left Rear (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU/BK | 747 | Left Rear Door Ajar Switch Signal
B | 0.35 BK | 650 | Ground

### Door Ajar Switch - Right Front

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: Pins A: E/4
- Core/Insulation Crimp: Pins B: E/1
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Ajar Switch - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/WH | 746 | Right Front Door Ajar Switch Signal
B | 0.5 BK | 650 | Ground

### Door Ajar Switch - Right Rear (Sedan)

#### Connector Part Information

- OEM: 15449028
- Service: 88987978
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Door Ajar Switch - Right Rear (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 748 | Right Rear Door Ajar Switch Signal
B | 0.35 BK | 650 | Ground

### Door Latch - Driver (AU3)

#### Connector Part Information

- OEM: 15489983
- Service: 88988881
- Description: 4-Way F Timer Micro III Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used

### Door Latch - Left Rear (Sedan) (AU3)

#### Connector Part Information

- OEM: 15489983
- Service: 88988881
- Description: 4-Way F Timer Micro III Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Left Rear (Sedan) (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used

### Door Latch - Passenger (AU3)

#### Connector Part Information

- OEM: 15489983
- Service: 8988881
- Description: 4-Way F Timer Micro III Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used

### Door Latch - Right Rear (Sedan) (AU3)

#### Connector Part Information

- OEM: 15489983
- Service: 88988881
- Description: 4-Way F Timer Micro III Sealed (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Latch - Right Rear (Sedan) (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
3 | 0.5 GY | 295 | Door Lock Actuator Lock Control
4 | -- | -- | Not Used

### Door Lock Switch - Driver (AU3)

#### Connector Part Information

- OEM: 15417063
- Service: See Catalog
- Description: 3-Way F Micro-Pack 64 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Lock Switch - Driver (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1250 | Ground
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 0.5 WH | 682 | Door Lock Lock/Unlock Signal

### Door Lock Switch - Front Passenger (AU3)

#### Connector Part Information

- OEM: 15417063
- Service: See Catalog
- Description: 3-Way F Micro-Pack 64 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Door Lock Switch - Front Passenger (AU3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 1250 | Ground
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (1)
C | 0.5 WH | 682 | Door Lock Lock/Unlock Signal

### Electronic Brake Control Module (EBCM) (JM4)

#### Connector Part Information

- OEM: 13515286
- Service: 88988597
- Description: 26-Way F Receptacle Sealed (BK)

#### Terminal Part Information

- Pins: 1, 14, 26
- Terminal/Tray: 60012931/21
- Core/Insulation Crimp: C/1
- Release Tool/Test Probe: 12122378/J-35616-4A (PU)

- Pins: 2-6, 8, 9, 11, 12, 20-24
- Terminal/Tray: 60040451/21
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12093647/J-35616-40 (BU)

#### Electronic Brake Control Module (EBCM) (JM4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 2 RD/WH | 740 | Battery Positive Voltage
2 | 0.5 OG | 885 | Left Rear Wheel Speed Sensor Low Reference
3 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
4 | -- | -- | Not Used
5 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
6 | 0.5 TN | 833 | Right Front Wheel Speed Sensor Low Reference
7 | -- | -- | Not Used
8 | 0.5 YE | 873 | Left Front Wheel Speed Sensor Low Reference
9 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal
10 | -- | -- | Not Used
11 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
12 | 0.5 WH | 883 | Right Rear Wheel Speed Sensor Low Reference
13 | -- | -- | Not Used
14 | 3 RD/BK | 542 | Battery Positive Voltage
15-19 | -- | -- | Not Used
20 | 0.35 PK | 1439 | Ignition 1 Voltage
21 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
22 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
23 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
24 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
25 | -- | -- | Not Used
26 | 3 BK | 350 | Ground

### Electronic Brake Control Module (EBCM) (JL4/JL9)

#### Connector Part Information

- OEM: 13608606
- Service: See Catalog
- Description: 47-Way F MK25/60 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Electronic Brake Control Module (EBCM) (JL4/JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 3 RD/BK | 542 | Battery Positive Voltage
2-4 | -- | -- | Not Used
5 | 0.5 GY | 1056 | Steering Wheel Position Sensor 5V Reference Voltage
6-7 | -- | -- | Not Used
8 | 0.5 PK | 1439 | Ignition 1 Voltage
9-10 | -- | -- | Not Used
11 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
12 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
13 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
14 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
15 | -- | -- | Not Used
16 | 3 BK | 350 | Ground
17 | -- | -- | Not Used
18 | 0.5 PK/BK | 6434 | CAN Bus High Serial Data
19 | 0.5 GY/BK | 6435 | CAN Bus Low Serial Data
20-21 | -- | -- | Not Used
22 | 0.5 D-GN | 2087 | 12V Reference
23-25 | -- | -- | Not Used
26 | 0.5 L-GN | 6257 | 5-Volt Reference (JL4 with LNF)
27 | 0.5 L-GN/BK | 6258 | Low Reference (JL4 with LNF)
28 | -- | -- | Not Used
29 | 0.5 L-BU | 2088 | Steering Wheel Position Sensor Low Reference
30-31 | -- | -- | Not Used
32 | 2 RD/WH | 740 | Battery Positive Voltage
33 | 0.5 TN | 833 | Right Front Wheel Speed Sensor Low Reference
34 | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
35 | -- | -- | Not Used
36 | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal
37 | 0.5 OG | 885 | Left Rear Wheel Speed Sensor Low Reference
38-39 | -- | -- | Not Used
40 | 0.5 OG/BK | 556 | Steering Wheel Position Sensor Low Reference
41 | 0.5 D-BU | 1809 | Brake Booster Vacuum Sensor Signal (LNF)
42 | 0.5 WH | 883 | Right Rear Wheel Speed Sensor Low Reference
43 | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal
44 | -- | -- | Not Used
45 | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal
46 | 0.5 YE | 873 | Left Front Wheel Speed Sensor Low Reference
47 | -- | -- | Not Used

### Electronic Power Steering (EPS) Control Module X1

#### Connector Part Information

- OEM: 10721337
- Service: 88952816
- Description: 2-Way F 375 58 (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-3251/10
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12094430/J-35616-22 (RD)

#### Electronic Power Steering (EPS) Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 5 RD/BK | 642 | Battery Positive Voltage
2 | 5 BK | 1150 | Ground

### Electronic Power Steering (EPS) Control Module X2

#### Connector Part Information

- OEM: 15438391
- Service: 88988409
- Description: 6-Way F 040 (GY)

#### Terminal Part Information

- Terminal/Tray: 173681-2/17
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-16 (L-GN)

#### Electronic Power Steering (EPS) Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
2 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
3 | -- | -- | Not Used
4 | 0.5 BN/WH | 2500 | High Speed GMLAN Serial Data Bus (+)
5 | 0.5 BN | 2501 | High Speed GMLAN Serial Data Bus (-)
6 | 0.5 PK | 1539 | Ignition 1 Voltage

### Electronic Power Steering (EPS) Control Module X3

#### Connector Part Information

- OEM: 7123-4123-30
- Service: 88952816
- Description: 2-Way F (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Electronic Power Steering (EPS) Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 0.35 RD | 5 | Motor Control
- | 0.35 BK | 5 | Motor Control

### Engine Control Module (ECM) X1 (L61/LE5)

#### Connector Part Information

- OEM: 15499466
- Service: See Catalog
- Description: 73-Way F MX 123 Series Sealed (BK)

#### Terminal Part Information

- Pins: 73
- Terminal/Tray: 7116-4151-02/9
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: 1, 3-6, 13, 18, 21, 24, 25, 27, 30, 31, 34, 36, 37, 39, 41-44, 47, 49, 54-56, 58, 66-68
- Terminal/Tray: 33467-0003/23
- Core/Insulation Crimp: H/H
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

- Pins: 19, 20, 70
- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X1 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-BU | 1161 | APP Sensor 1 Signal
2 | -- | -- | Not Used
3 | 0.35 BN | 4 | Accessory Voltage
4 | -- | -- | Not Used
5 | 0.35 D-GN | 335 | Low Speed Cooling Fan Relay Control
6 | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
7-10 | -- | -- | Not Used
11 | 0.35 OG/GN | 7360 | Low Reference (M86)
12 | -- | -- | Not Used
13 | 0.35 YE | 5991 | Powertrain Relay Control
14-17 | -- | -- | Not Used
18 | 0.35 L-BU | 1162 | APP Sensor 2 Signal
19 | 0.5 PK/BK | 1039 | Ignition 1 Voltage
20 | 0.5 RD/WH | 840 | Battery Positive Voltage
21 | 0.35 PU | 1272 | Low Reference
22-23 | -- | -- | Not Used
24 | 0.35 TN | 2759 | Low Reference
25 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C67)
26 | -- | -- | Not Used
27 | 0.35 BN/WH | 419 | MIL Control
28-29 | -- | -- | Not Used
30 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control (C67)
31 | -- | -- | Not Used
32 | 0.35 PU/WH | 6386 | Starter Control
33 | -- | -- | Not Used
34 | 0.35 PU/WH | 6356 | VSS Signal Low
35-36 | -- | -- | Not Used
37 | 0.35 YE | 492 | Mass Air Flow Sensor Signal
38 | -- | -- | Not Used
39 | 0.35 PU | 1589 | Fuel Level Sensor Signal
40 | -- | -- | Not Used
41 | 0.35 BN | 1271 | Low Reference
42 | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
43 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data (+) (1)
44 | 0.35 TN | 2501 | High Speed GMLAN Serial Data (-) (1)
45 | 0.35 D-BU/WH | 7361 | 5-Volt Reference 2 (M86)
46 | -- | -- | Not Used
47 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
48 | -- | -- | Not Used
49 | 0.35 D-BU | 473 | Coolant Fan Relay Output - Coil
50-53 | -- | -- | Not Used
54 | 0.35 BN/WH | 6354 | VSS Signal High
55 | 0.35 L-BU | 20 | Stop Lamp Supply Voltage
56 | 0.35 D-GN | 1433 | PNP/Clutch Start Switch Signal (M86)
57 | 0.35 D-GN | --6307 | Park/Neutral Signal
58 | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal
59-60 | -- | -- | Not Used
61 | 0.35 L-GN | 6338 | Clutch Pedal Position Sensor Signal (M86)
62-65 | -- | -- | Not Used
66 | 0.35 GY | 2709 | 5-Volt Reference 1
67 | 0.35 TN | 1274 | 5-Volt Reference 1
68 | 0.35 BN | 436 | Air Injection Reaction Pump Motor Relay Output - Coil (NU6)
69 | -- | -- | Not Used
70 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
71-72 | -- | -- | Not Used
73 | 0.8 PK/BK | 5290 | Ignition 1 Voltage

### Engine Control Module (ECM) X1 (LNF)

#### Connector Part Information

- OEM: 15438366
- Service: 88988373
- Description: 96-Way Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Engine Control Module (ECM) X1 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid Control
2 | 0.5 PU | 5284 | Camshaft Phaser Intake Solenoid Control
3-4 | -- | -- | Not Used
5 | 0.35 YE | 7301 | High Pressure Fuel Pump Actuator High Control
6 | 0.35 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
7 | 0.5 OG | 5275 | Camshaft Position Intake Sensor Signal
8-9 | -- | -- | Not Used
10 | 0.35 OG | 225 | Generator Turn On Signal
11-12 | -- | -- | Not Used
13 | 0.35 BN/WH | 2130 | Low Reference
14 | -- | -- | Not Used
15 | 0.35 GY | 705 | 5-Volt Reference 2
16 | 0.35 D-GN | 6391 | Turbo Bypass Valve Control
17 | 0.35 TN/BK | 231 | Oil Pressure Switch Signal
18 | 0.35 YE | 258 | Wastegate Solenoid Control
19-23 | -- | -- | Not Used
24 | 0.5 YE | 581 | TAC Motor Control - 1
25 | 0.35 TN | 891 | Boost Gauge Signal
26 | 0.35 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
27 | 0.35 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4
28 | 0.35 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
29 | 0.35 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2
30 | 0.35 GY | 23 | Generator Field Duty Cycle Signal
31-33 | -- | -- | Not Used
34 | 0.5 D-GN | 5273 | Camshaft Position Exhaust Sensor Signal
35 | 0.35 YE | 573 | CKP Sensor Signal
36 | 0.35 YE | 2918 | FRP Sensor Signal
37 | 0.5 L-GN | 432 | MAP Sensor Signal
38 | 0.35 GY | 598 | 5-Volt Reference 1
39 | 0.35 GY | 2701 | 5-Volt Reference 3
40 | 0.35 TN | 407 | Low Reference
41 | 0.35 TN | 552 | Low Reference
42 | 0.35 TN | 808 | Low Reference
43 | 0.35 GY | 597 | 5-Volt Reference
44 | 0.35 TN | 2761 | Low Reference
45 | 0.35 L-GN | 2867 | 5-Volt Reference 3
46 | 0.35 PU | 574 | Low Reference
47 | -- | -- | Not Used
48 | 0.5 BN | 582 | TAC Motor Control 2
49-50 | -- | -- | Not Used
51 | 0.35 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
52 | 0.35 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
53 | 0.35 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3
54 | 0.35 BN/WH | 419 | MIL Control
55 | 0.35 PU | 2121 | IC 1 Control
56 | 0.35 D-GN/WH | 2124 | IC 4 Control
57-58 | -- | -- | Not Used
59 | 0.5 D-BU | 496 | KS 1 Signal
60 | 0.35 GY | 2303 | KS 2 Signal
61-63 | -- | -- | Not Used
64 | 0.5 OG/BK | 469 | Low Reference
65 | -- | -- | Not Used
66 | 0.35 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal
67 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
68 | 0.35 WH | 5279 | Heated Oxygen Sensor Pump Current Sensor 1
69-72 | -- | -- | Not Used
73 | 0.35 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
74 | -- | -- | Not Used
75 | 0.35 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1
76-77 | -- | -- | Not Used
78 | 0.35 BN | 2129 | Low Reference
79 | 0.35 L-BU | 2123 | IC 3 Control
80 | 0.35 OG/WH | 2122 | IC 2 Control
81 | -- | -- | Not Used
82 | 0.35 YE | 410 | ECT Sensor Signal
83 | 0.5 GY | 1716 | KS 1 Signal
84 | 0.35 L-BU | 1876 | KS 2 Signal
85 | -- | -- | Not Used
86 | 0.35 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
87 | -- | -- | Not Used
88 | 0.35 TN | 2752 | Low Reference
89 | 0.35 PU | 486 | TP Sensor 2 Signal
90 | 0.35 D-GN | 485 | TP Sensor 1 Signal
91 | 0.35 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current Sensor 1
92 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1
93-94 | -- | -- | Not Used
95 | 0.5 GY | 2704 | 5-Volt Reference 1
96 | 0.5 GY/WH | 3113 | HO2S Heater Low Control -- Sensor 1

### Engine Control Module (ECM) X2 (L61)

#### Connector Part Information

- OEM: 13577506
- Service: See Catalog
- Description: 73-Way F MX 123 Series Sealed (GY)

#### Terminal Part Information

- Pins: 73
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 5, 9, 13, 20, 22-24, 26, 30-31, 33, 35, 39, 41-43, 45-46, 49-51, 54, 58, 67
- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: C
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

- Pins: 6-8, 10, 16, 32, 37-38, 40, 48, 53, 57, 59, 65-66, 68
- Terminal/Tray: 33467-0003/23
- Core/Insulation Crimp: C
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X2 (L61)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 6331 | AIR Solenoid Signal (NU6)
3 | 0.5 PU | 421 | AIR Solenoid Relay Control (NU6)
4 | 0.35 TN | 2761 | Low Reference
5 | 0.5 PU | 574 | Low Reference
6 | 0.35 TN | 1744 | Fuel Injector (1) Control
7 | 0.35 PK/BK | 1746 | Fuel Injector (3) Control
8 | 0.35 L-BU/BK | 844 | Fuel Injector (4) Control
9 | 0.35 BN | 2129 | Low Reference
10 | 0.35 L-GN/BK | 1745 | Fuel Injector (2) Control
11-12 | -- | -- | Not Used
13 | 0.35 GY/BK | 2704 | 5-Volt Reference 1
14-15 | -- | -- | Not Used
16 | 0.5 YE | 581 | TAC Motor Control (1)
17-19 | -- | -- | Not Used
20 | 0.5 TN | 5301 | Low Reference
21 | -- | -- | Not Used
22 | 0.35 PU | 2121 | Ignition Control (1)
23 | 0.35 L-BU | 2123 | Ignition Control (3)
24 | 0.35 D-GN/WH | 2124 | Ignition Control (4)
25 | -- | -- | Not Used
26 | 0.35 OG/WH | 2122 | Ignition Control (2)
27-29 | -- | -- | Not Used
30 | 0.35 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
31 | 0.35 OG | 225 | Generator Turn On Signal
32 | 0.5 BN | 582 | TAC Motor Control (2)
33 | 0.5 D-BU | 5300 | 5-Volt Reference 1
34 | -- | -- | Not Used
35 | 0.5 GY | 6255 | 5-Volt Reference 1
36 | -- | -- | Not Used
37 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1
38 | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
39 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal
40 | 0.5 TN | 2752 | Low Reference
41 | 0.5 PU/WH | 6256 | Low Reference
42 | 0.35 TN | 2760 | Low Reference
43 | 0.35 GY/WH | 23 | Generator Field Duty Cycle Signal
44 | -- | -- | Not Used
45 | 0.5 YE | 573 | Crankshaft Position Sensor Signal
46 | 0.5 OG | 5275 | CMP Sensor Signal
47 | -- | -- | Not Used
48 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
49 | 0.5 OG/BK | 469 | Low Reference
50 | 0.5 GY | 1716 | Knock Sensor Signal
51 | 0.5 D-BU | 496 | Knock Sensor Signal
52 | -- | -- | Not Used
53 | 0.5 GY | 2701 | 5-Volt Reference 2
54 | 0.5 L-GN | 2867 | 5-Volt Reference 2
55 | 0.5 WH | 6452 | 5-Volt Reference 1 (NU6)
56 | -- | -- | Not Used
57 | 0.5 D-GN | 485 | Throttle Position Sensor (1) Signal
58 | 0.35 YE | 410 | Engine Coolant Temperature Sensor Signal
59 | 0.5 PU | 486 | Throttle Position Sensor (2) Signal
60-63 | -- | -- | Not Used
64 | 0.35 TN | 407 | Low Reference (NU6)
65 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control Sensor 1
66 | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control Sensor 2
67 | 0.35 TN/BK | 231 | Oil Pressure Switch Signal
68 | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
69-72 | -- | -- | Not Used
73 | 2 BK/WH | 451 | Signal Ground

### Engine Control Module (ECM) X2 (LE5)

#### Connector Part Information

- OEM: 13610160
- Service: See Catalog
- Description: 73-Way F MX 123 Series Sealed (GY)

#### Terminal Part Information

- Pins: 73
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: 5, 9, 13, 20, 22-24, 26, 30-31, 33, 35, 39, 41-43, 45-46, 49-51, 54, 58, 67
- Terminal/Tray: 33467-0005/23
- Core/Insulation Crimp: C
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

- Pins: 6-8, 10, 16, 32, 37-38, 40, 48, 53, 57, 59, 65-66, 68
- Terminal/Tray: 33467-0003/23
- Core/Insulation Crimp: C
- Release Tool/Test Probe: J-38125-213/J-35616-64B (L-BU)

#### Engine Control Module (ECM) X2 (LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 6331 | AIR Solenoid Signal (NU6)
3 | 0.5 PU | 421 | AIR Solenoid Relay Control (NU6)
4 | 0.35 TN | 2761 | Low Reference
5 | 0.5 PU | 574 | Low Reference
6 | 0.35 TN | 1744 | Fuel Injector (1) Control
7 | 0.35 PK/BK | 1746 | Fuel Injector (3) Control
8 | 0.35 L-BU/BK | 844 | Fuel Injector (4) Control
9 | 0.35 BN | 2129 | Low Reference
10 | 0.35 L-GN/BK | 1745 | Fuel Injector (2) Control
11-12 | -- | -- | Not Used
13 | 0.35 GY | 2704 | 5-Volt Reference 1 (M86)
0.35 PU/WH | 5-Volt Reference 1 (MN5)
14 | 0.5 L-GN | 5282 | Camshaft Phaser Exhaust Solenoid 1
15 | 0.5 PU | 5284 | Cam Solenoid Control
16 | 0.5 YE | 581 | TAC Motor Control (1)
17-19 | -- | -- | Not Used
20 | 0.5 TN | 5301 | Low Reference
21 | 0.5 GY | 5296 | Low Reference
22 | 0.35 PU | 2121 | Ignition Control (1)
23 | 0.35 L-BU | 2123 | Ignition Control (3)
24 | 0.35 D-GN/WH | 2124 | Ignition Control (4)
25 | -- | -- | Not Used
26 | 0.35 OG/WH | 2122 | Ignition Control (2)
27-29 | -- | -- | Not Used
30 | 0.35 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control
31 | 0.35 OG | 225 | Generator Turn On Signal
32 | 0.5 BN | 582 | TAC Motor Control (2)
33 | 0.5 D-BU | 5300 | 5-Volt Reference 1
34 | 0.5 YE/BK | 5297 | 5-Volt Reference 1
35 | 0.5 GY | 6255 | 5-Volt Reference (C67)
36 | -- | -- | Not Used
37 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal Sensor 1
38 | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
39 | 0.5 L-GN | 432 | Manifold Absolute Pressure Sensor Signal
40 | 0.5 TN | 2752 | Low Reference
41 | 0.5 PU/WH | 6256 | Low Reference (C67 with M86)
0.5 BK/WH | Low Reference (C67 with MN5)
42 | 0.35 TN | 2760 | Low Reference
43 | 0.35 GY/WH | 23 | Generator Field Duty Cycle Signal
44 | -- | -- | Not Used
45 | 0.5 YE | 573 | Crankshaft Position Sensor Signal
46 | 0.5 OG | 5275 | CMP Sensor Signal 1
47 | 0.5 D-GN | 5273 | CMP Sensor Signal 2
48 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal Sensor 1
49 | 0.5 OG/BK | 469 | Low Reference
50 | 0.5 GY | 1716 | Knock Sensor Signal
51 | 0.5 D-BU | 496 | Knock Sensor Signal
52 | -- | -- | Not Used
53 | 0.5 GY | 2701 | 5-Volt Reference 2
54 | 0.5 L-GN | 2867 | 5-Volt Reference 2
55-56 | -- | -- | Not Used
57 | 0.5 D-GN | 485 | Throttle Position Sensor (1) Signal
58 | 0.35 YE | 410 | Engine Coolant Temperature Sensor Signal
59 | 0.5 PU | 486 | Throttle Position Sensor (2) Signal
60 | 0.5 BN | 6753 | CMP Actuator Solenoid Bank 1 -- Intake Low Reference
61 | 0.5 BN/WH | 6754 | CMP Actuator Solenoid Bank 1 -- Exhaust Low Reference
62-63 | -- | -- | Not Used
64 | 0.35 TN | 407 | Low Reference (NU6)
65 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control Sensor 1
66 | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control Sensor 2
67 | 0.35 TN/BK | 231 | Oil Pressure Switch Signal
68 | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
69-72 | -- | -- | Not Used
73 | 2 BK/WH | 451 | Signal Ground

### Engine Control Module (ECM) X2 (LNF)

#### Connector Part Information

- OEM: 1 928 404 916
- Service: See Catalog
- Description: 58-Way (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: Terminal Repair Kit
- Release Tool/Test Probe: Terminal Repair Kit

#### Engine Control Module (ECM) X2 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.8 BK/WH | 451 | Ground
2 | 0.8 BK/WH | 451 | Ground
3 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
4 | 0.8 BK/WH | 451 | Ground
5 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
6 | 0.8 PK/BK | 5290 | Ignition 1 Voltage
7 | 0.5 GY/WH | 3122 | Heated Oxygen Sensor Heater Low Control Sensor 2
8 | -- | -- | Not Used
9 | 0.35 TN | 2759 | Low Reference
10 | 0.35 D-GN/WH | 465 | Fuel Pump Relay Control
11 | 0.35 TN | 5514 | A/C Refrigerant Pressure Sensor Low Reference (C67)
12 | -- | -- | Not Used
13 | 0.35 YE | 492 | MAF Sensor Signal
14 | 0.35 GY | 2709 | 5-Volt Reference 1
15 | 0.35 D-BU | 1161 | APP Sensor 1 Signal
16-18 | -- | -- | Not Used
19 | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
20-21 | -- | -- | Not Used
22 | 0.35 TN | 2760 | Low Reference
23 | 0.5 TN/WH | 3121 | Heated Oxygen Sensor Low Signal Sensor 2
24 | -- | -- | Not Used
25 | 0.35 L-BU | 1162 | APP Sensor 2 Signal
26 | -- | -- | Not Used
27 | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
28-33 | -- | -- | Not Used
34 | 0.35 BN | 1271 | Low Reference
35 | 0.35 GY | 2700 | 5-Volt Reference 3 (C67)
36 | 0.35 PU | 1589 | Fuel Level Sensor Signal
37 | 0.35 L-GN | 6338 | Clutch Pedal Position Sensor Signal
38 | 0.5 PU | 3120 | Heated Oxygen Sensor High Signal Sensor 2
39 | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C67)
40 | 0.5 PU | 401 | OSS Low Signal
41 | 0.35 BN | 4 | Accessory Voltage
42 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
43 | -- | -- | Not Used
44 | 0.35 D-GN/WH | 459 | A/C Compressor Clutch Relay Control (C67)
45 | 0.35 D-BU | 473 | High Speed Cooling Fan Relay Control
46 | 0.35 D-GN | 335 | Cooling Fan Relay Control
47 | 0.35 PU | 1272 | Low Reference
48 | 0.35 TN | 1274 | 5-Volt Reference 3
49 | 0.35 WH/BK | 1164 | 5-Volt Reference 2
50 | 0.35 L-BU | 6289 | Induction Air Temperature Sensor Signal
51 | -- | -- | Not Used
52 | 0.8 L-BU | 20 | Stop Lamp Supply Voltage
53 | 0.5 YE | 400 | OSS High Signal
54 | 0.5 PK | 1039 | Ignition 1 Voltage
55 | 0.5 TN | 2501 | High Speed GMLAN Serial Data BUS (-)
56 | 0.5 RD/WH | 840 | Battery Positive Voltage
57 | 0.35 PU/WH | 6386 | Starter Relay Coil Control
58 | 0.35 YE | 5991 | Powertrain Relay Coil Control

### Engine Coolant Temperature (ECT) Sensor (L61/LE5)

#### Connector Part Information

- OEM: 15449028
- Service: 88987993
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 2761 | Low Reference
B | 0.5 YE | 410 | ECT Sensor Signal

### Engine Coolant Temperature (ECT) Sensor (LNF)

#### Connector Part Information

- OEM: 13584122
- Service: 88987993
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN | 2761 | Low Reference
B | 0.5 YE | 410 | ECT Sensor Signal

### Engine Oil Pressure (EOP) Switch

#### Connector Part Information

- OEM: 12065299
- Service: 12085500
- Description: 1-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Engine Oil Pressure (EOP) Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/BK | 231 | Oil Pressure Switch Signal

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PK/BK | 5291 | Ignition 1 Voltage (L61/LNF)
0.5 PK/WH | Ignition 1 Voltage (LE5)
B | 0.5 D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 RD/WH | 1840 | Battery Positive Voltage
B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control

### Fog Lamp - Left Front (T37)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Left Front (T37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 150 | Ground

### Fog Lamp - Right Front (T37)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Fog Lamp - Right Front (T37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 2234 | Front Fog Lamp Supply Voltage
B | 0.5 BK | 250 | Ground

### Fog Lamp Switch (T37)

#### Connector Part Information

- OEM: 15419483
- Service: 89046742
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Fog Lamp Switch (T37)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK/WH | 1051 | Ground
B | -- | -- | Not Used
C | 0.35 OG | 192 | Front Fog Lamp Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Fuel Injector 1 (L61/LE5)

#### Connector Part Information

- OEM: 12610756
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 139 | Ignition 1 Voltage
2 | 0.5 BK | 1744 | Fuel Injector (1) Control

### Fuel Injector 1 (LNF)

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 4801 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 1
2 | 0.5 BN/WH | 4901 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 1

### Fuel Injector 2 (L61/LE5)

#### Connector Part Information

- OEM: 12610756
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 139 | Ignition 1 Voltage
2 | 0.5 L-GN/BK | 1745 | Fuel Injector (2) Control

### Fuel Injector 2 (LNF)

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-BU | 4802 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 2
2 | 0.5 D-BU/WH | 4902 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 2

### Fuel Injector 3 (L61/LE5)

#### Connector Part Information

- OEM: 12610756
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 139 | Ignition 1 Voltage
2 | 0.5 PK/BK | 1746 | Fuel Injector (3) Control

### Fuel Injector 3 (LNF)

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 4803 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 3
2 | 0.5 D-GN/WH | 4903 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 3

### Fuel Injector 4 (L61/LE5)

#### Connector Part Information

- OEM: 12610756
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 PK | 139 | Ignition 1 Voltage
2 | 0.5 L-BU/BK | 844 | Fuel Injector (4) Control

### Fuel Injector 4 (LNF)

#### Connector Part Information

- OEM: 1 928 403 874
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 L-BU | 4804 | Direct Fuel Injector (DFI) High Voltage Control Cylinder 4
2 | 0.5 L-BU/WH | 4904 | Direct Fuel Injector (DFI) High Voltage Supply Cylinder 4

### Fuel Pump (FP) and Sender Assembly

#### Connector Part Information

- OEM: 15326631
- Service: See Catalog
- Description: 4-Way F APEX 2.8 MM (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Pump (FP) and Sender Assembly

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 BK | 850 | Ground
B | 1 GY | 120 | Fuel Pump Supply Voltage
C | 0.8 PU | 1589 | Fuel Level Sensor Signal
D | 0.5 OG/BK | 510 | Low Reference

### Fuel Rail Pressure Sensor (FPS) (LNF)

#### Connector Part Information

- OEM: 1 928 403 966
- Service: See Catalog
- Description: 3-Way F 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Rail Pressure Sensor (FPS) (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 808 | Sensor Low Reference
2 | 0.5 YE | 2918 | Fuel Rail Pressure Sensor Signal
3 | 0.5 GY | 598 | 5-Volt Reference 1

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 88908720
- Service: See Catalog
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/RD | 890 | Fuel Tank Pressure Sensor Signal
2 | 0.5 BK/WH | 2759 | Low Reference
3 | 0.5 GY/BK | 2709 | 5-Volt Reference - 1

### Generator X1 (L61/LE5)

#### Connector Part Information

- OEM: 12186308
- Service: 89046837
- Description: 2-Way F Timer JR-Power Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Generator X1 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 OG | 225 | Generator Turn On Signal
2 | 0.35 GY | 23 | Generator Field Duty Cycle Signal

### Generator X1 (LNF)

#### Connector Part Information

- OEM: 15355066
- Service: 15306329
- Description: 4-Way, 2 Usable, F Metri-Pack 150 Series Sealed (BG)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Generator X1 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Available
B | 0.35 OG | 225 | Generator Turn On Signal
C | 0.35 GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Available

### Generator X2

#### Terminal Part Information

- Terminal: 12146365
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Generator X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
-- | 13 BK | 1 | Battery Positive Voltage

### Hazard Switch

#### Connector Part Information

- OEM: 12089248
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Hazard Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | -- | -- | Not Used
D | 0.35 WH | 111 | Hazard Switch Signal

### Headlamp High/Low Beam/DRL - Left

#### Connector Part Information

- OEM: 12048369
- Service: 12117260
- Description: 3-Way F Metri-Pack 280 Series Sealed (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp High/Low Beam/DRL - Left

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 712 | Left Headlamp Low Beam Supply Voltage
B | 0.8 BK | 150 | Ground
C | 0.8 PK | 711 | Left Headlamp High Beam Supply Voltage

### Headlamp High/Low Beam/DRL - Right

#### Connector Part Information

- OEM: 12048369
- Service: 12117260
- Description: 3-Way F Metri-Pack 280 Series Sealed (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Headlamp High/Low Beam/DRL - Right

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 312 | Right Headlamp Low Beam Supply Voltage
B | 0.8 BK | 250 | Ground
C | 0.8 PK | 311 | Right Headlamp High Beam Supply Voltage

### Heated Oxygen Sensor (HO2S) 1 (L61/LE5)

#### Connector Part Information

- OEM: 12176897
- Service: 15305903
- Description: 4-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Oxygen Sensor (HO2S) 1 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3111 | HO2S Low Signal sensor 1
B | 0.5 PU/WH | 3110 | HO2S High Signal Sensor 1
C | 0.5 GY/WH | 3113 | HO2S Heater Low Control Sensor 1
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### Heated Oxygen Sensor (HO2S) 1 (LNF)

#### Connector Part Information

- OEM: 10863919
- Service: See Catalog
- Description: 6-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Oxygen Sensor (HO2S) 1 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 5279 | Heated Oxygen Sensor Pump Current - Sensor 1
2 | 0.5 TN/WH | 3111 | Heated Oxygen Sensor Low Signal - Sensor 1
3 | 0.5 GY/WH | 3113 | Heated Oxygen Sensor Heater Low Control - Sensor 1
4 | 0.5 PK/BK | 5291 | Ignition 1 Voltage
5 | 0.5 L-GN | 5278 | Heated Oxygen Sensor Input Pump Current - Sensor 1
6 | 0.5 PU/WH | 3110 | Heated Oxygen Sensor High Signal - Sensor 1

### Heated Oxygen Sensor (HO2S) 2 (L61/LE5)

#### Connector Part Information

- OEM: 12160825
- Service: 12167158
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) 2 (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | HO2S Low Signal Sensor 2
B | 0.5 PU | 3120 | HO2S High Signal Sensor 2
C | 0.5 GY/WH | 3122 | HO2S Heater Low Control Sensor 2
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### Heated Oxygen Sensor (HO2S) 2 (LNF)

#### Connector Part Information

- OEM: 15326423
- Service: 12167158
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) 2 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 TN/WH | 3121 | HO2S Low Signal Sensor 2
B | 0.5 PU | 3120 | HO2S High Signal Sensor 2
C | 0.5 GY/WH | 3122 | HO2S Heater Low Control Sensor 2
D | 0.5 PK/BK | 5291 | Ignition 1 Voltage

### Heated Seat Element - Driver Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Seat Element - Driver Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 BK | 1250 | Ground
B | 0.8 OG | 2077 | Heated Seat Cushion Element Supply Voltage

### Heated Seat Element - Driver Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Driver Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 2077 | Heated Seat Element Supply
B | 0.8 OG | 2077 | Heated Seat Element Supply
C | 0.8 GY/BK | 2080 | Heated Seat Temperature Sensor Signal
D | 1 BK | 1250 | Ground

### Heated Seat Element - Passenger Back (KA1)

#### Connector Part Information

- OEM: 12059254
- Service: 12126020
- Description: 2-Way F Metri-Pack 150 Series (GN)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Seat Element - Passenger Back (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 BK | 1250 | Ground
B | 0.8 OG | 2077 | Heated Seat Cushion Element Supply Voltage

### Heated Seat Element - Passenger Cushion (KA1)

#### Connector Part Information

- OEM: 12047786
- Service: 12085536
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Element - Passenger Cushion (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 OG | 2077 | Heated Seat Element Supply
B | 0.8 OG | 2077 | Heated Seat Element Supply
C | 0.8 GY | 2080 | Heated Seat Temperature Sensor Signal
D | 1 BK | 1250 | Ground

### Heated Seat Module - Driver (KA1)

#### Connector Part Information

- OEM: 15-97-5081
- Service: 89046731
- Description: 8-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Module - Driver (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.5 PK | 1501 | Driver Heated Seat High/Low Signal
4 | 1 BK | 1250 | Ground
5 | 1 RD/WH | 340 | Battery Positive Voltage
6 | 0.8 GY | 2080 | Driver Heated Seat Cushion Temperature Sensor Low Reference
7 | 0.8 OG | 2077 | Heated Seat Cushion Element Supply Voltage
8 | 0.5 L-BU | 1462 | Heated Seat Switch Signal

### Heated Seat Module - Passenger (KA1)

#### Connector Part Information

- OEM: 15-97-5081
- Service: 89046731
- Description: 8-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Heated Seat Module - Passenger (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | 0.35 PK | 1503 | Passenger Heated Seat High/Low Signal
4 | 1 BK | 1250 | Ground
5 | 1 RD/WH | 340 | Battery Positive Voltage
6 | 0.8 GY | 2080 | Passenger Heated Seat Cushion Temperature Sensor Low Reference
7 | 0.8 OG | 2077 | Heated Seat Cushion Element Supply Voltage
8 | 0.35 L-BU | 1505 | Heated Seat Switch Signal

### Heated Seat Switch - Driver (KA1)

#### Connector Part Information

- OEM: 12177194
- Service: 15305927
- Description: 6-Way F Metri-Pack 150 Series (WH)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Seat Switch - Driver (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 1501 | Driver Heated Seat High/Low Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | -- | -- | Not Used
D | 0.35 PK | 339 | Ignition 1 Voltage
E | 0.35 BK/WH | 651 | Ground
F | 0.35 L-BU | 1462 | Heated Seat Switch Signal

### Heated Seat Switch - Passenger (KA1)

#### Connector Part Information

- OEM: 12177195
- Service: 15305931
- Description: 6-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12129484/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Seat Switch - Passenger (KA1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK/BK | 1503 | Passenger Heated Seat High/Low Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | -- | -- | Not Used
D | 0.35 PK | 339 | Ignition 1 Voltage
E | 0.35 BK/WH | 651 | Ground
F | 0.35 L-BU/BK | 1505 | Passenger Heated Seat Switch Signal

### High Pressure Fuel Pump (LNF)

#### Connector Part Information

- OEM: 15339756
- Service: See Catalog
- Description: 2-Way F Kompakt 2.8 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### High Pressure Fuel Pump (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PU | 7300 | High Pressure Fuel Pump Actuator Low Control
2 | 0.35 YE | 7301 | High Pressure Fuel Pump Actuator High Control

### Hood Ajar Switch (AP3)

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F GT 150 Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Hood Ajar Switch (AP3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK/BK | 109 | Hood Ajar Switch Signal
B | 0.35 PU | 5531 | Hood Closed Switch Signal
C | 0.35 BK | 150 | Ground

### Horn

#### Connector Part Information

- OEM: 15419715
- Service: 88988313
- Description: 2-Way F GT 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Horn

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 29 | Horn Control
B | 0.5 BK | 150 | Ground

### Horn Switch

#### Connector Part Information

- OEM: 12059251
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Horn Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN | 28 | Horn Relay Control
2 | 0.35 BK/WH | 151 | Ground
0.35 BK/WH | 151 | Ground

### HVAC Control Module X1

#### Connector Part Information

- OEM: 15416970
- Service: 15394150
- Description: 16-Way F Micro-Pack 64 Modular (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### HVAC Control Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 L-GN | 2275 | Mode Door Position Signal
2-3 | -- | -- | Not Used
4 | 0.35 L-BU/BK | 1688 | 5-Volt Reference - 2
5 | 0.35 L-GN/BK | 1647 | Open Recirculation Door Control - B
6 | 0.35 PK/WH | 1648 | Close Recirculation Door Control - A
7 | 0.5 PK | 339 | Ignition 1 Voltage
8 | 0.5 PK | 339 | Ignition 1 Voltage
9 | 0.35 D-BU | 1646 | Auxiliary Air Temperature Door Position Signal
10 | -- | -- | Not Used
11 | 0.35 D-GN | 71 | Off Blower Motor Control
12 | 0.35 L-BU/BK | 1688 | 5-Volt Reference - 2
13 | 0.35 WH/BK | 1236 | Auxiliary Air Temperature Door Control
14 | 0.35 TN | 2273 | Mode Door Control
15 | 0.35 BK/WH | 550 | Ground
16 | 0.35 BK/WH | 550 | Ground

### HVAC Control Module X2

#### Connector Part Information

- OEM: 15480081
- Service: 88988315
- Description: 8-Way F Micro-Pack 64 (BK)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### HVAC Control Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A1 | 0.35 PK | 339 | Ignition 1 Voltage
A2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
A3 | -- | -- | Not Used
A4 | 0.35 RD/WH | 1540 | Battery Positive Voltage
A5 | 0.8 BK | 550 | Ground
A6 | 0.35 L-GN | 66 | A/C Request Signal (C67)
A7 | 0.35 WH | 193 | Rear Defog Relay Control
A8 | 0.35 L-BU | 292 | Rear Defog Switch Signal

### HVAC Control Module X3

#### Connector Part Information

- OEM: 12064998
- Service: 15306189
- Description: 8-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### HVAC Control Module X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 71 | OFF Blower Motor Control
B | 3 BK | 550 | Ground
C-D | -- | -- | Not Used
E | 3 OG | 52 | Blower Motor High Control
F | 2 L-BU | 72 | Medium 2 Blower Motor Control
G | 2 TN | 63 | Blower Motor Medium 1 Control
H | 2 YE | 60 | Blower Motor Low Control

### Ignition Coil/Module 1

#### Connector Part Information

- OEM: 15466325
- Service: 88988338
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil/Module 1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 1350 | Ground
B | 0.35 BN | 2129 | Low Reference
C | 0.35 PU | 2121 | Ignition Control (1)
D | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 2

#### Connector Part Information

- OEM: 15466325
- Service: 88988338
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil/Module 2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 1350 | Ground
B | 0.35 BN | 2129 | Low Reference (L61/LE5)
0.35 BN/WH | 2130 | Low Reference (LNF)
C | 0.35 OG/WH | 2122 | Ignition Control (2)
D | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 3

#### Connector Part Information

- OEM: 15466325
- Service: 88988338
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil/Module 3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 1350 | Ground
B | 0.35 BN | 2129 | Low Reference
C | 0.35 L-BU | 2123 | Ignition Control (3)
D | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 4

#### Connector Part Information

- OEM: 15466325
- Service: 88988338
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 7116-4102-08/9
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094430/J-35616-2A (GY)

#### Ignition Coil/Module 4

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 1350 | Ground
B | 0.35 BN | 2129 | Low Reference (LE5/L61)
0.35 BN/WH | 2130 | Low Reference (LNF)
C | 0.35 D-GN/WH | 2124 | Ignition Control (4)
D | 0.5 PK/BK | 5292 | Ignition 1 Voltage

### Ignition Lock Cylinder Control Solenoid

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Ignition Lock Cylinder Control Solenoid

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN/WH | 1932 | Shift Select Switch Park Signal
B | 0.35 BN | 4 | Accessory Voltage

### Ignition Switch

#### Connector Part Information

- OEM: 15324806
- Service: 88987854
- Description: 6-Way F 035 Series ILAG5 (GN)

#### Terminal Part Information

- Terminal/Tray: IL-AG5-C1-5000/20
- Core/Insulation Crimp: K/K
- Release Tool/Test Probe: J-38125-211/J-35616-64B (L-BU)

#### Ignition Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 RD/WH | 1040 | Battery Positive Voltage
3 | 0.35 YE | 5199 | Run/Crank Voltage
4 | 0.35 BN | 4 | Accessory Voltage
5 | 0.35 WH | 1390 | Off/Run/Crank Voltage
6 | 0.35 WH/BK | 1073 | Key-In Ignition Switch

### Inflatable Restraint Front End Sensor

#### Connector Part Information

- OEM: 15356727
- Service: 15306405
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/OG | 5045 | Discriminating Sensor - Low Reference
B | 0.35 YE | 1834 | Forward Discriminating Sensor Signal

### Inflatable Restraint Front Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15431682
- Service: See Catalog
- Description: 18-Way F Micro-Pack 100W Series Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2, 4, 6, 7, 9, 14-16, 18
- Terminal/Tray: Service With Terminated Lead
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12122523/J-35616-6 (BN)

- Pins: 5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Front Passenger Presence System (PPS) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/BK | 723 | Passenger Air Bag On Indicator Control
2 | 0.35 L-GN | 353 | Passenger Air Bag Off Indicator Control
3 | -- | -- | Not Used
4 | 0.35 D-BU | 913 | Passenger Seat Belt Tension Sensor Signal
5 | 0.35 BK/WH | 1251 | Ground
6 | 0.35 PK/WH | 916 | Passenger Presence Sensor Signal
7 | 0.35 D-BU/WH | 918 | 5-Volt Reference
8 | -- | -- | Not Used
9 | 0.35 PK | 1339 | Ignition 1 Voltage
10-13 | -- | -- | Not Used
14 | 0.35 YE | 914 | Low Reference
15 | 0.35 YE/WH | 917 | Low Reference
16 | 0.35 PK/BK | 915 | 5-Volt Reference
17 | -- | -- | Not Used
18 | 0.35 PU | 5018 | Occupant Sensor Serial Data

### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

#### Connector Part Information

- OEM: 15422250
- Service: 88987995
- Description: 3-Way F GT 150 Series Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-BU/WH | 918 | 5-Volt Reference
B | 0.35 PK/WH | 916 | Passenger Presence Sensor Signal
C | 0.35 YE/WH | 917 | Low Reference

### Inflatable Restraint Instrument Panel (I/P) Module X1

#### Connector Part Information

- OEM: 699467-7
- Service: See Catalog
- Description: 2-Way F 90 Degree Lockable (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Instrument Panel (I/P) Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 3025 | I/P Module Stage 1 High Control
B | 0.5 OG | 3024 | I/P Module Stage 1 Low Control

### Inflatable Restraint Instrument Panel (I/P) Module X2

#### Connector Part Information

- OEM: 699467-7
- Service: See Catalog
- Description: 2-Way F 90 Degree Lockable (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Instrument Panel (I/P) Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 PU | 3026 | I/P Module Stage 2 Low Control
B | 0.5 GY | 3027 | I/P Module Stage 2 High Control

### Inflatable Restraint Passenger Air Bag On/Off Indicator

#### Connector Part Information

- OEM: 15398877
- Service: 88953369
- Description: 5-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Air Bag On/Off Indicator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/BK | 723 | Passenger Air Bag On Indicator Control
2 | 0.5 BK | 550 | Ground
3 | 0.35 PK | 353 | Passenger Air Bag Off Indicator Control
4 | 0.5 PK | 339 | Ignition 1 Voltage
5 | 0.35 PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Passenger Seat Belt Tension Sensor

#### Connector Part Information

- OEM: 15326808
- Service: See Note
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Seat Belt Tension Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 915 | 5-Volt Reference
B | 0.35 YE | 914 | Low Reference
C | 0.35 D-BU | 913 | Passenger Seat Belt Tension Sensor Signal

### Inflatable Restraint Roof Rail Module - Left (ASF)

#### Connector Part Information

- OEM: CA-252-92-5-Q
- Service: See Catalog
- Description: 2-Way F (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 5019 | Roof Rail Module - Left - High Control
2 | 0.5 WH | 5020 | Roof Rail Module - Left - Low Control

### Inflatable Restraint Roof Rail Module - Right (ASF)

#### Connector Part Information

- OEM: CA-252-92-5-Q
- Service: See Catalog
- Description: 2-Way F (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 D-GN | 5021 | Roof Rail Module - Right - High Control
2 | 0.5 WH | 5022 | Roof Rail Module - Right - Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (ASF)

#### Connector Part Information

- OEM: 15488865
- Service: 88988302
- Description: 60-Way F Micro-Pack 64 Series (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1340 | Battery Positive Voltage
2 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 PK | 5057 | Low Reference
4 | 0.35 TN/WH | 238 | Seat Belt Switch Left
5 | -- | -- | Not Available
6 | 0.35 OG | 1362 | Passenger Seat Belt Switch Right
7 | -- | -- | Not Available
8 | 0.5 PK | 5020 | Roof Rail Module - Left - Low Control
9 | 0.5 PU/WH | 5019 | Roof Rail Module - Left - High Control
10 | 0.5 YE/BK | 5021 | Roof Rail Module - Right - High Control
11 | 0.5 WH/BK | 5022 | Roof Rail Module - Right - Low Control
12 | 0.5 PU | 3026 | I/P Module Stage 2 Low Control
13 | 0.5 GY | 3027 | I/P Module Stage 2 High Control
14 | 0.5 TN | 3021 | Steering Wheel Module Stage 1 High Control
15 | 0.5 BN | 3020 | Steering Wheel Module Stage 1 Low Control
16 | 0.5 PK | 3022 | Steering Wheel Module Stage 2 Low Control
17 | 0.5 WH | 3023 | Steering Wheel Module Stage 2 High Control
18 | 0.5 YE | 3025 | I/P Module Stage 1 High Control
19 | 0.5 OG | 3024 | I/P Module Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | 0.8 BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | 0.35 PK | 1339 | Ignition 1 Voltage
34-37 | -- | -- | Not Available
38 | 0.35 YE | 1834 | Forward Discriminating Sensor Signal
39 | 0.35 TN/OG | 5045 | Discriminating Sensor Low Reference
40-45 | -- | -- | Not Available
46 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal
47 | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage
48 | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage
49 | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal
50-51 | -- | -- | Not Available
52 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
53 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
54-55 | -- | -- | Not Available
56 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
57 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
58-59 | -- | -- | Not Available
60 | 0.35 PK | 5018 | Occupant Sensor - Serial Data

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (without ASF)

#### Connector Part Information

- OEM: 15456067
- Service: 88987858
- Description: 60-Way F Micro-Pack 64 Series (BU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (without ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1340 | Battery Positive Voltage
2 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
3 | 0.35 PK | 5057 | Seat Position Sensor - Low Reference
4 | 0.35 TN/WH | 238 | Seat Belt Switch - Left
5 | -- | -- | Not Available
6 | 0.35 OG | 1362 | Seat Belt Switch - Right
7-11 | -- | -- | Not Available
12 | 0.5 PU | 3026 | I/P Module Stage 2 Low Control
13 | 0.5 GY | 3027 | I/P Module Stage 2 High Control
14 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
15 | 0.5 BN | 3020 | Steering Wheel Module Stage 1 Low Control
16 | 0.5 PK | 3022 | Steering Wheel Module Stage 2 Low Control
17 | 0.5 WH | 3023 | Steering Wheel Module Stage 2 High Control
18 | 0.5 YE | 3025 | I/P Module Stage 1 High Control
19 | 0.5 OG | 3024 | I/P Module Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | 0.8 BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | 0.35 PK | 1339 | Ignition 1 Voltage
34-37 | -- | -- | Not Available
38 | 0.35 YE | 1834 | Forward Discriminating Sensor Signal
39 | 0.35 TN/OG | 5045 | Discriminating Sensor - Low Reference
40-51 | -- | -- | Not Available
52 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
53 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
54-55 | -- | -- | Not Available
56 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
57 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left- Low Control
58-59 | -- | -- | Not Available
60 | 0.35 PK | 5018 | Occupant Sensor Serial Data

### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

#### Connector Part Information

- OEM: 15356725
- Service: 15306362
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Side Impact Sensor (SIS) - Left (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage
B | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal

### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

#### Connector Part Information

- OEM: 15356725
- Service: 15306362
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Side Impact Sensor (SIS) - Right (ASF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage
B | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal

### Inflatable Restraint Steering Wheel Module X1

#### Connector Part Information

- OEM: 54560236
- Service: See Catalog
- Description: 2-Way F ABX-4 Code B (WH)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
2 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module X2

#### Connector Part Information

- OEM: 54560222
- Service: See Catalog
- Description: 2-Way F Type G (PK)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control
2 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control

### Inflatable Restraint Steering Wheel Module Coil X1

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 (BK)

#### Terminal Part Information

- Pins: C, F, K
- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: D, E, G, J
- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.5 PK | 339 | Ignition 1 Voltage
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Remote Radio Control Signal (UK3)
F | 0.35 WH/BK | 644 | 12-Volt Reference (UK3)
G | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 TN | 28 | Horn Relay Control
K | 0.35 BK/WH | 151 | Ground

### Inflatable Restraint Steering Wheel Module Coil X2

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PK | 1539 | Ignition 1 Voltage (K34)
D | 0.35 GY | 1884 | Cruise Control Switch Signal (K34)
E | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | 0.35 WH/BK | 644 | 12-Volt Reference (UK3)
G | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
H | 0.35 D-GN/WH | 1358 | Driver Information Center Switch Signal
J | 0.35 TN | 28 | Horn Relay Control
K | 0.5 BK/WH | 1051 | Ground

### Inflatable Restraint Steering Wheel Module Coil X3

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module Coil X3

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 3020 | Steering Wheel Module Stage 2 Low Control
2 | 0.5 TN | 3021 | Steering Wheel Module Stage 2 High Control
3 | 0.5 PK | 3022 | Steering Wheel Module Stage 1 Low Control
4 | 0.5 WH | 3023 | Steering Wheel Module Stage 1 High Control

### INLINE Fuse - 50 AMP

#### Connector Part Information

- OEM: 12110057
- Service: 12110057
- Description: 2-Way F Maxi (BK)

#### Terminal Part Information

- Terminal/Tray: 12110127/19
- Core/Insulation Crimp: F/G
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### INLINE Fuse - 50 AMP

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 5 RD/BK | 142 | Battery Positive Voltage
B | 5 RD | 1 | Unfused Battery Positive Voltage

### Inside Rearview Mirror (UE1)

#### Connector Part Information

- OEM: 15441350
- Service: 15306351
- Description: 16-Way F Micro HVT (BK)

#### Terminal Part Information

- Pins: 1, 6, 8, 9, 11-15
- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: Pins 1, 6, 8, 9, 11, 12, 14, 15: J/J
- Core/Insulation Crimp: Pins 13: K/K
- Release Tool/Test Probe: 12180559/J-35616-6 (BN)

#### Inside Rearview Mirror (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 157 | Courtesy Lamp Control (CF5)
2-5 | -- | -- | Not Used
6 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage (CF5)
7 | -- | -- | Not Used
8 | 0.5 BK | 750 | Ground
9-10 | -- | -- | Not Used
11 | 0.35 D-GN/WH | 2514 | Keypad Signal
12 | 0.35 L-GN/BK | 2515 | Keypad Supply Voltage
13 | -- | -- | Not Used
14 | 0.35 YE/BK | 2516 | Keypad Green LED Signal
15 | 0.35 BN/WH | 2517 | Keypad Red LED Signal
16 | -- | -- | Not Used

### Inside Rearview Mirror (without UE1)

#### Connector Part Information

- OEM: 12124782
- Service: 15306078
- Description: 7-Way F Misc (BK)

#### Terminal Part Information

- Terminal/Tray: SVH-21T-P1.1/20
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12094429/J-35616-18 (BK)

#### Inside Rearview Mirror (without UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 BK | 750 | Ground
3-5 | -- | -- | Not Used
6 | 0.5 GY | 157 | Courtesy Lamp Control
7 | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Instrument Panel Cluster (IPC)

#### Connector Part Information

- OEM: 15429805
- Service: 89047195
- Description: 16-Way F Micro 64 (GY)

#### Terminal Part Information

- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

#### Instrument Panel Cluster (IPC)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1-4 | -- | -- | Not Used
5 | 0.35 D-GN/WH | 1358 | DIC Switch Signal
6 | 0.35 BN/WH | 419 | MIL Control
7 | -- | -- | Not Used
8 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.5 PK | 339 | Ignition 1 Voltage
12 | -- | -- | Not Used
13 | 0.5 RD/WH | 1440 | Battery Positive Voltage
14 | 0.35 D-GN | 264 | Security Indicator Supply Voltage
15 | 0.5 BK/WH | 1051 | Ground
16 | 0.8 BK | 550 | Ground

### Intake Air Pressure and Temperature Sensor (LNF)

#### Connector Part Information

- OEM: 15336035
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Intake Air Pressure and Temperature Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 597 | 5-Volt Reference
2 | 0.35 L-BU | 7329 | Pre-Throttle Air Temp and Press (TMAP) Temperature Signal
3 | 0.35 TN | 407 | Low Reference
4 | 0.35 PU | 7330 | Pre-Throttle Air Temp and Press (TMAP) Air Pressure Signal

### I/P Dimmer Switch

#### Connector Part Information

- OEM: 15332135
- Service: 15306414
- Description: 4-Way F GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### I/P Dimmer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | 0.35 PU | 719 | Low Reference
D | 0.35 D-GN | 44 | Instrument Panel Lamp Dimmer Switch Signal

### Knock Sensor (KS)

#### Connector Part Information

- OEM: 12077900
- Service: 12116247
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Knock Sensor (KS)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-BU | 496 | Knock Sensor (1) Signal
B | 0.5 GY | 1716 | Knock Sensor Signal

### Knock Sensor (KS) 2 (LNF)

#### Connector Part Information

- OEM: 12077900
- Service: See Catalog
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Knock Sensor (KS) 2 (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU | 1876 | KS 2 Signal
B | 0.35 GY | 2303 | KS 2 Signal

### License Lamp

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### License Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Supply Voltage
B | 0.8 BK | 750 | Ground (Cobalt)
0.5 BK | 750 | Ground (G5)

### Manifold Absolute Pressure (MAP) Sensor (L61/LE5)

#### Connector Part Information

- OEM: 15365614
- Service: 88987997
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Manifold Absolute Pressure (MAP) Sensor (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 2704 | 5-Volt Reference - 2
2 | 0.5 OG/BK | 469 | Low Reference
3 | 0.5 L-GN | 432 | MAP Sensor Signal

### Manifold Absolute Pressure (MAP) Sensor (LNF)

#### Connector Part Information

- OEM: 15398808
- Service: 88987997
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Manifold Absolute Pressure (MAP) Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 2704 | 5-Volt Reference - 2
2 | 0.5 OG/BK | 469 | Low Reference
3 | 0.5 L-GN | 432 | MAP Sensor Signal

### Marker Lamp - Left Front

#### Connector Part Information

- OEM: 16530675
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Supply Voltage
B | 0.5 BK | 150 | Ground
0.5 BK | 150 | Ground

### Marker Lamp - Left Rear (Coupe)

#### Connector Part Information

- OEM: 15491912
- Service: 88988366
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Marker Lamp - Left Rear (Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.5 BK | 750 | Ground

### Marker Lamp - Left Rear (Sedan)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Marker Lamp - Left Rear (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Supply Voltage
B | 0.5 BK | 750 | Ground

### Marker Lamp - Right Front

#### Connector Part Information

- OEM: 16530675
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Supply Voltage
B | 0.5 BK | 250 | Ground
0.5 BK | 250 | Ground

### Marker Lamp - Right Rear (Coupe)

#### Connector Part Information

- OEM: 15491912
- Service: 88988366
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Marker Lamp - Right Rear (Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BN | 9 | Park Lamp Supply Voltage
2 | 0.5 BK | 850 | Ground

### Marker Lamp - Right Rear (Sedan)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

- Pins: B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Marker Lamp - Right Rear (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 9 | Park Lamp Supply Voltage
B | 0.5 BK | 850 | Ground

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 YE | 492 | MAF Sensor Signal
B | 0.5 BK/WH | 451 | Ground
C | 0.5 PK/BK | 5291 | Ignition 1 Voltage
D | 0.35 TN | 2760 | Low Reference
E | 0.35 L-BU | 6289 | IAT Sensor Signal

### Mode Actuator

#### Connector Part Information

- OEM: 12064993
- Service: 12102485
- Description: 6-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Mode Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
5 | 0.35 PK | 339 | Ignition 1 Voltage
6 | 0.35 TN | 2273 | Mode Door Control
7 | 0.35 BK/WH | 550 | Ground
8 | -- | -- | Not Available
9 | 0.35 L-GN | 2275 | Mode Position Signal
10 | 0.35 L-BU/BK | 1688 | 5-Volt Reference - 2

### Outside Rearview Mirror - Driver (DG7)

#### Connector Part Information

- OEM: 15419810
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: See Terminal Repair Kit
- Terminal/Tray: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Driver (DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 WH/BK | 81 | Left Mirror Motor Right Control (Coupe)
0.35 WH | 81 | Left Mirror Motor Right Control (Sedan)
B | 0.35 L-GN | 89 | Left Mirror Motor Down Control
C | 0.35 YE | 329 | Left Mirror Motor Supply Voltage
D | -- | -- | Not Used

### Outside Rearview Mirror - Passenger (DG7)

#### Connector Part Information

- OEM: 15419810
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: See Terminal Repair Kit
- Terminal/Tray: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror - Passenger (DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU/WH | 889 | Right Mirror Motor Down Control
B | 0.35 OG/WH | 881 | Right Mirror Motor Right Control
C | 0.35 WH | 330 | Right Mirror Motor Supply Voltage
D | -- | -- | Not Used

### Outside Rearview Mirror Switch (DG7)

#### Connector Part Information

- OEM: 12064769
- Service: See Catalog
- Description: 10-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: See Terminal Repair Kit
- Terminal/Tray: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Outside Rearview Mirror Switch (DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.5 BK | 1250 | Ground
C | 0.35 WH | 330 | Right Mirror Motor Supply Voltage (Coupe)
0.35 WH/BK | 330 | Right Mirror Motor Supply Voltage (Sedan)
D | 0.35 WH/BK | 81 | Left Mirror Motor Right Control (Coupe)
0.35 WH | 81 | Left Mirror Motor Right Control (Sedan)
E | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage (1)
F | 0.35 L-GN | 89 | Left Mirror Motor Down Control
G | 0.35 RD/WH | 440 | Battery Positive Voltage
H | 0.35 YE | 329 | Left Mirror Motor Supply Voltage
J | 0.35 OG/WH | 881 | Right Mirror Motor Right Control
K | 0.35 PU/WH | 889 | Right Mirror Motor Down Control

### Park Brake Switch

#### Connector Part Information

- OEM: 12047682
- Service: 12101850
- Description: 1-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Park Brake Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-BU | 1134 | Park Brake Switch Signal

### Park/Neutral Position (PNP) Switch (MN5/MXO)

#### Connector Part Information

- OEM: 15416724
- Service: 89046696
- Description: 12-Way F GT 150, 280 Series Solid (L-GY)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Neutral Position (PNP) Switch (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 451 | Ground
2 | 0.35 WH | 776 | Transmission Range Signal P
3 | -- | -- | Not Used
4 | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
5 | 0.5 PK/BK | 539 | Ignition 1 Voltage
6-7 | -- | -- | Not Used
8 | 0.35 YE | 772 | Transmission Range Signal B
9 | 0.35 TN/WH | 771 | Transmission Range Signal A
10 | 0.35 GY | 773 | Transmission Range Signal C
11 | 0.5 BK/WH | 451 | Ground
12 | 0.5 D-GN | 6307 | Park/Neutral Signal

### Park/Turn Signal Lamp - Left Front

#### Connector Part Information

- OEM: 0001340
- Service: See Catalog
- Description: 3-Way F CE-F22.2 Series Bulbsocket, Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Left Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 14 | Left Turn Signal Lamp Supply Voltage
B | 0.35 BN | 9 | Park Lamp Supply Voltage
0.35 BN | 9 | Park Lamp Supply Voltage
G | 0.8 BK | 150 | Ground
0.8 BK | 150 | Ground

### Park/Turn Signal Lamp - Right Front

#### Connector Part Information

- OEM: 0001340
- Service: See Catalog
- Description: 3-Way F CE-F22.2 Series Bulbsocket, Sealed (BG)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Park/Turn Signal Lamp - Right Front

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU | 15 | Right Turn Signal Lamp Supply Voltage
B | 0.35 BN | 9 | Park Lamp Supply Voltage
0.35 BN | 9 | Park Lamp Supply Voltage
G | 0.8 BK | 250 | Ground
0.5 BK | 250 | Ground

### Pressure Control (PC) Solenoid Valve (MN5/MXO)

#### Connector Part Information

- OEM: 15466861
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series P2S (GY)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Pressure Control Solenoid Valve (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 1228 | Pressure Control (PC) Solenoid Valve High Control
B | 0.35 L-BU | 1229 | PC Solenoid Valve Low Control

### PRNDL Lamp

#### Connector Part Information

- OEM: 12162083
- Service: See Catalog
- Description: 2-Way F Lamp Socket Bulb Base Type W-2 Axial (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### PRNDL Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK | 1250 | Ground
B | 0.35 WH | 8 | Instrument Panel Lamp Supply Voltage

### Radio X1

#### Connector Part Information

- OEM: 15488568
- Service: 12110206
- Description: 14-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Pins: 1, 8
- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

- Pins: 2, 4-7 , 9, 11
- Terminal/Tray: 12146448/19
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 RD/WH | 1140 | Battery Positive Voltage
2-3 | -- | -- | Not Used
4 | 0.35 D-GN | 117 | Right Front Speaker Output (-) (UQ4)
0.35 L-GN | 1948 | Right Front Low Level Audio Signal (-) (UQ3)
5 | 0.35 L-GN | 200 | Right Front Speaker Output (+) (UQ4)
0.35 L-GN/WH | 512 | Right Front Low Level Audio Signal (+) (UQ3)
6 | 0.35 GY | 118 | Left Front Speaker Output (-) (UQ4)
0.35 D-GN | 1947 | Left Front Low Level Audio (-) (UQ3)
7 | 0.35 TN | 201 | Left Front Speaker Output (+) (UQ4)
0.35 TN | 511 | Left Front Low Level Audio Signal (UQ3)
8 | 1 BK/WH | 1051 | Ground
9 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
10 | -- | -- | Not Used
11 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal (UK3)
12-14 | -- | -- | Not Used

### Radio X2

#### Connector Part Information

- OEM: 15491285
- Service: 15305996
- Description: 16-Way F Micro-Pack 100 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Radio X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BN/WH | 367 | Left Audio Signal (+) (U2K)
2 | 0.35 D-GN/WH | 368 | Right Audio Signal (+) (U2K)
3 | 0.35 PK | 314 | Radio On Signal (UQ3)
4 | 0.35 D-BU | 46 | Right Rear Speaker Output (+) (UQ4)
0.35 D-BU | 546 | Right Rear Low Level Audio Signal (+) (UQ3)
5 | 0.35 L-BU | 115 | Right Rear Speaker Output (-) (UQ4)
0.35 TN | 1946 | Right Rear Low Level Audio Signal (-) (UQ3)
6 | 0.35 BN | 199 | Left Rear Speaker Output (+) (UQ4)
0.35 BN/WH | 599 | Left Rear Low Level Audio Signal (+) (UQ3)
7 | 0.35 YE | 116 | Left Rear Speaker Output (-) (UQ4)
0.35 BN | 1999 | Left Rear Low Level Audio Signal (-) (UQ3)
8 | 0.35 PK/BK | 2062 | Cellular Telephone Voice Signal (UE1)
9 | 0.35 TN/WH | 372 | Audio Common (U2K)
10-13 | -- | -- | Not Used
14 | 0.35 WH/BK | 644 | 10-Volt Reference (UK3)
15 | 0.35 L-GN | 1011 | Remote Radio Control Signal (UQ3)
16 | 0.35 OG/BK | 2061 | Cellular Telephone Voice Low Reference (UE1)

### Rear Compartment Courtesy Lamp

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Rear Compartment Courtesy Lamp

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG/BK | 737 | Rear Compartment Lamp Control
B | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage

### Rear Compartment Lid Release Actuator

#### Connector Part Information

- OEM: 15489043
- Service: 88988309
- Description: 4-Way F Timer Micro III Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Rear Compartment Lid Release Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.5 OG/BK | 744 | Rear Compartment Lid Ajar Switch Signal
3 | 0.5 BK | 750 | Ground
4 | 0.8 TN/WH | 56 | Rear Compartment Lid Release Switch

### Rear Compartment Lid Release Switch

#### Connector Part Information

- OEM: 12089248
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Rear Compartment Lid Release Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | -- | -- | Not Used
C | 0.35 TN | 1576 | Rear Compartment Lid Release Switch Signal
D | -- | -- | Not Used

### Rear Window Defogger Grid X1

#### Connector Part Information

- OEM: 12092133
- Service: 12167133
- Description: 1-Way F Metri-Pack 630 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12103325/3
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3 BK | 293 | Rear Defog Element Supply Voltage

### Rear Window Defogger Grid X2

#### Connector Part Information

- OEM: 12092133
- Service: 12167133
- Description: 1-Way F Metri-Pack 630 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12103325/3
- Core/Insulation Crimp: A/B
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Rear Window Defogger Grid X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3 BK | 850 | Ground

### Recirculation Actuator

#### Connector Part Information

- OEM: 12059110
- Service: 88953271
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Recirculation Actuator

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 L-GN/BK | 1647 | Open Recirculation Door Control - B
B | 0.35 PK/WH | 1648 | Close Recirculation Door Control - A

### Remote Control Door Lock Receiver (RCDLR) (AU0)

#### Connector Part Information

- OEM: 13514032
- Service: 12102635
- Description: 4-Way F Micro-Pack 100 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12146447/3
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12031876-1/J-35616-6 (BN)

#### Remote Control Door Lock Receiver (RCDLR) (AU0)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 BK/WH | 1051 | Ground
2 | 0.35 D-GN | 5060 | Keyless Entry Program Enable Signal
3 | -- | -- | Not Used
4 | 0.5 RD/WH | 1140 | Battery Positive Voltage

### Seat Belt Retractor Pretensioner - Driver

#### Connector Part Information

- OEM: 15380395
- Service: 88988308
- Description: 2-Way F MISC (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
2 | 0.5 TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control

### Seat Belt Retractor Pretensioner - Passenger

#### Connector Part Information

- OEM: 15380395
- Service: 88988308
- Description: 2-Way F MISC (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 OG | 2117 | Seat Belt Pretensioner - Right - Low Control
2 | 0.5 L-GN | 2116 | Seat Belt Pretensioner - Right - High Control

### Seat Belt Switch - Driver

#### Connector Part Information

- OEM: 15332132
- Service: 88986266
- Description: 3-Way F MISC (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Switch - Driver

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 TN/WH | 238 | Seat Belt Switch - Left
B | -- | -- | Not Used
C | 0.35 PK | 5057 | Low Reference

### Seat Belt Switch - Passenger

#### Connector Part Information

- OEM: 15332133
- Service: 88986266
- Description: 3-Way M GT150 (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Switch - Passenger

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch - Right
B | -- | -- | Not Used
C | 0.35 BN | 5057 | Low Reference

### Secondary Air Injection (AIR) Pump (NU6)

#### Connector Part Information

- OEM: 12124819
- Service: 12085498
- Description: 2-Way F Metri-Pack 280 Series (NA)

#### Terminal Part Information

- Terminal/Tray: 12077413/4
- Core/Insulation Crimp: B/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Secondary Air Injection (AIR) Pump (NU6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 5 OG | 78 | AIR Pump Supply Voltage
B | 5 BK | 1050 | Ground

### Secondary Air Injection (AIR) Solenoid (NU6)

#### Connector Part Information

- OEM: 13539171
- Service: 88988601
- Description: 6-Way F Metri-Pack 150 Sealed Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Secondary Air Injection (AIR) Solenoid (NU6)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN | 407 | Low Reference
2 | 0.35 BN/WH | 6331 | AIR Solenoid Position Sensor
3 | 0.35 WH | 6452 | 5-Volt Reference
4 | 0.5 BK/WH | 451 | Ground
5 | -- | -- | Not Used
6 | 0.5 PK/BK | 415 | AIR Solenoid Supply Voltage

### Speaker - Left Front Door (UQ3)

#### Connector Part Information

- OEM: 15485606
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Front Door (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY/BK | 118 | Left Front Speaker Output (-)
B | 0.35 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front Door (UQ4)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Front Door (UQ4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 118 | Left Front Speaker Output (-)
B | 0.35 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Front Door Tweeter (UQ3)

#### Connector Part Information

- OEM: 12064870
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Left Front Door Tweeter (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 GY | 118 | Left Front Speaker Output (-)
B | 0.35 TN | 201 | Left Front Speaker Output (+)

### Speaker - Left Rear (UQ3)

#### Connector Part Information

- OEM: 12064869
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Rear (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1.0 YE/BK | 116 | Left Rear Speaker Output (-)
B | 0.8 BN/WH | 199 | Left Rear Speaker Output (+)

### Speaker - Left Rear (UQ4)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Left Rear (UQ4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 116 | Left Rear Speaker Output (-)
B | 0.5 BN | 199 | Left Rear Speaker Output (+)

### Speaker - Right Front Door (UQ3)

#### Connector Part Information

- OEM: 15485606
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Front Door (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 117 | Right Front Speaker Output (-)
B | 0.35 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front Door (UQ4)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Front Door (UQ4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 117 | Right Front Speaker Output (-)
B | 0.35 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Front Door Tweeter (UQ3)

#### Connector Part Information

- OEM: 12064870
- Service: See Catalog
- Description: 2-Way M Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Speaker - Right Front Door Tweeter (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 D-GN | 117 | Right Front Speaker Output (-) (Coupe)
0.35 D-GN/WH | 117 | Right Front Speaker Output (-) (Sedan)
B | 0.35 L-GN | 200 | Right Front Speaker Output (+)

### Speaker - Right Rear (UQ3)

#### Connector Part Information

- OEM: 12064869
- Service: 12117323
- Description: 2-Way F Metri-Pack 150 Series (BU)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Rear (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 1 L-BU/BK | 115 | Right Rear Speaker Output (-)
B | 1 D-BU/BK | 46 | Right Rear Speaker Output (+)

### Speaker - Right Rear (UQ4)

#### Connector Part Information

- OEM: 12052832
- Service: 12101825
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Right Rear (UQ4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 L-BU | 115 | Right Rear Speaker Output (-)
B | 0.5 D-BU | 46 | Right Rear Speaker Output (+)

### Speaker - Subwoofer (UQ3)

#### Connector Part Information

- OEM: 12064760
- Service: 12085208
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Speaker - Subwoofer (UQ3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 L-BU/BK | 315 | Right Rear Subwoofer Speaker Output (+)
B | 0.8 D-GN | 1795 | Right Rear Subwoofer Speaker Output (+)
C | 0.8 D-BU/WH | 346 | Rear Subwoofer Speaker Output (-)
D | 0.8 L-GN/BK | 1794 | Rear Subwoofer Speaker Output (+)

### Starter X1

#### Connector Part Information

- OEM: 12089916
- Service: See Catalog
- Description: 1-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Starter X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 PU | 6 | Starter Solenoid Crank Voltage

### Starter X2 (To Battery)

#### Terminal Part Information

- Terminal: 12161134
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter X2 (To Battery)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 32 RD | 1 | Battery Positive Voltage

### Starter X2 (To Generator)

#### Terminal Part Information

- Terminal: 12103501
- Core/Insulation Crimp: N/A
- Description: Ring Terminal

#### Starter X2 (To Generator)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
+ | 8 BK | 2 | Battery Positive Voltage

### Steering Angle Sensor (JL4/JL9)

#### Connector Part Information

- OEM: 13547374
- Service: See Catalog
- Description: 6-Way F 064 GET Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Angle Sensor (JL4/JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 GY | 1056 | 5-Volt Reference
2 | -- | -- | Not Used
3 | 0.35 PK/BK | 6434 | CAN Bus High Serial Data
4 | 0.35 GY/BK | 6435 | CAN Bus Low Serial Data
5 | -- | -- | Not Used
6 | 0.35 OG/BK | 556 | Low Reference

### Steering Wheel Controls - Left (K34)

#### Connector Part Information

- OEM: 50-57-9407
- Service: See Catalog
- Description: 7-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Controls - Left (K34)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN/WH | 1358 | DIC Switch Signal
2 | -- | -- | Not Used
3 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
4 | 0.5 PK | 339 | Ignition 1 Voltage
5 | 0.35 GY | 1884 | Cruise Control Switch Signal
6 | -- | -- | Not Used
7 | 0.35 BK/WH | 151 | Ground

### Steering Wheel Controls Right (K34 with UK3)

#### Connector Part Information

- OEM: 12103499
- Service: 88987918
- Description: 4-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Steering Wheel Controls Right (K34 with UK3)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 151 | Ground
2 | 0.35 WH/BK | 644 | 12-Volt Reference
3 | 0.35 GY | 8 | Instrument Panel Lamps Supply Voltage
4 | 0.35 D-BU | 1796 | Steering Wheel Controls Signal

### Sunroof Motor (CF5)

#### Connector Part Information

- OEM: 12186775
- Service: 15306098
- Description: 3-Way F (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Sunroof Motor (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 131 | Sunroof Limit Switch Low Reference
2 | 0.5 WH | 750 | Ground
3 | 0.5 D-GN | 127 | Sunroof Motor Open Control

### Sunroof Switch (CF5)

#### Connector Part Information

- OEM: 12059800
- Service: 15306169
- Description: 5-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-E
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A-D: E/C
- Core/Insulation Crimp: Pins E: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Sunroof Switch (CF5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BK | 750 | Ground
B | 0.5 L-BU | 131 | Sunroof Limit Switch Range Signal
C | 0.5 L-GN | 129 | Sunroof Motor Close Control
D | 0.5 D-GN | 127 | Sunroof Motor Open Control
E | 1 D-GN | 1301 | RAP Fuse Supply Voltage

### Tail/Stop and Turn Signal Lamp - Left (Coupe)

#### Connector Part Information

- OEM: 12040977
- Service: 12085492
- Description: 3-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Left (Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
C | 0.5 BK | 750 | Ground

### Tail/Stop and Turn Signal Lamp - Left (Sedan)

#### Connector Part Information

- OEM: 16530671
- Service: See Catalog
- Description: 3-Way F (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Left (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
0.5 BN | 9 | Park Lamp Supply Voltage
G | 0.5 BK | 750 | Ground
0.5 BK | 750 | Ground

### Tail/Stop and Turn Signal Lamp - Right (Coupe)

#### Connector Part Information

- OEM: 12040977
- Service: 12085492
- Description: 3-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Pins: A, B
- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

- Pins: C
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Right (Coupe)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
C | 0.5 BK | 850 | Ground

### Tail/Stop and Turn Signal Lamp - Right (Sedan)

#### Connector Part Information

- OEM: 16530671
- Service: See Catalog
- Description: 3-Way F (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Tail/Stop and Turn Signal Lamp - Right (Sedan)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 YE | 19 | Left Rear Stop/Turn Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage
0.5 BN | 9 | Park Lamp Supply Voltage
G | 0.5 BK | 850 | Ground
0.5 BK | 850 | Ground

### Theft Deterrent Control Module

#### Connector Part Information

- OEM: 15383337
- Service: 88988353
- Description: 5-Way F (BK)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Theft Deterrent Control Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 RD/WH | 1540 | Battery Positive Voltage
2 | 0.35 BN | 4 | Accessory Voltage Signal
3 | 0.35 BK/WH | 1051 | Ground
4 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
5 | -- | -- | Not Used

### Throttle Actuator Control (TAC) Module

#### Connector Part Information

- OEM: 15355297
- Service: 88988106
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Actuator Control (TAC) Module

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 BN | 582 | Throttle Actuator Motor Control (2)
B | 0.5 YE | 581 | Throttle Actuator Motor Control (1)
C | 0.5 TN | 2752 | Low Reference
D | 0.5 D-GN | 485 | Throttle Position Sensor (1) Signal
E | 0.5 GY | 2701 | 5-Volt Reference
F | 0.5 PU | 486 | Throttle Position Sensor (2) Signal

### Torque Converter Clutch Pulse Width Modulation (TCC PWM) Solenoid Valve (MN5/MXO)

#### Connector Part Information

- OEM: 15473845
- Service: Non-Serviceable
- Description: 2-Way F Metri-Pack 150.2 Series P2S (BU)

#### Terminal Part Information

- Terminal: Non-Serviceable
- Core/Insulation Crimp: Non-Serviceable
- Release Tool/Test Probe: Non-Serviceable

#### Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 RD | 839 | Ignition 1 Voltage
B | 0.35 TN | 418 | TCC PWM Solenoid Valve Control

### Traction Control Switch (JL4/JL9)

#### Connector Part Information

- OEM: 12047785
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Traction Control Switch (JL4/JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BK/WH | 651 | Ground
B | -- | -- | Not Used
C | 0.35 L-BU | 1788 | Traction Control Switch Signal
D | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Transmission Control Module (TCM) (MN5/MXO)

#### Connector Part Information

- OEM: 15480141
- Service: 89046898
- Description: 49-Way F Micro-64 GT 280 Series Sealed (BK with BU center)

#### Terminal Part Information

- Pins: 1-46
- Terminal/Tray: 15359541/4
- Core/Insulation Crimp: M/M
- Release Tool/Test Probe: 15381651-2/J-35616-64B (L-BU)

- Pins: 49
- Terminal/Tray: 15491972/24
- Core/Insulation Crimp: E/5
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Transmission Control Module (TCM) (MN5/MXO)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 TN/BK | 422 | Torque Converter Clutch Pulse Width Modulated (TCC PWM) Solenoid Valve Control
2 | 0.35 L-GN | 1222 | 1-2 Shift Solenoid (SS) Valve Control
3 | 0.35 OG/BK | 1230 | Input Speed Sensor (ISS) High Signal
4-5 | -- | -- | Not Used
6 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus - (CAN)
7 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus + (CAN)
8 | -- | -- | Not Used
9 | 0.35 YE | 657 | TCC Release Switch Signal
10 | -- | -- | Not Used
11 | 0.35 BN | 4 | Accessory Voltage
12-15 | -- | -- | Not Used
16 | 0.35 PU | 401 | Output Speed Sensor (OSS) Low Signal
17 | 0.35 L-BU/WH | 1229 | Pressure Control (PC) Solenoid Valve Low Control
18-19 | -- | -- | Not Used
20 | 0.35 YE/BK | 1223 | 2-3 SS Valve Control
21-22 | -- | -- | Not Used
23 | 0.35 GY | 773 | Transmission Range Switch Signal C
24-25 | -- | -- | Not Used
26 | 0.35 D-BU/WH | 1231 | ISS Low Signal
27-28 | -- | -- | Not Used
29 | 0.35 TN/WH | 771 | Transmission Range Switch Signal A
30 | 0.5 TN | 2762 | Transmission Fluid Temperature (TFT) Sensor Low Reference
31 | 0.5 PK | 1039 | Ignition 1 Voltage
32 | 0.5 RD/WH | 840 | Battery Positive Voltage
33 | 0.35 OG | 1226 | Transmission Fluid Pressure (TFP) Switch Signal C
34 | -- | -- | Not Used
35 | 0.35 YE/BK | 1227 | TFT Sensor Signal
36 | -- | -- | Not Used
37 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus - (CAN)
38 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus + (CAN)
39 | 0.35 WH | 776 | Transmission Range Switch Signal P
40 | 0.35 OG/BK | 1228 | PC Solenoid Valve High Control
41 | 0.35 YE | 400 | OSS High Signal
42 | 0.35 L-BU | 20 | Stop Lamp Switch Signal
43 | -- | -- | Not Used
44 | 0.35 D-BU | 1225 | TFP Switch Signal B
45 | -- | -- | Not Used
46 | 0.35 YE | 772 | Transmission Range Switch Signal B
47-48 | -- | -- | Not Used
49 | 0.5 BK/WH | 451 | Ground

### Turbo Bypass Valve Solenoid (LNF)

#### Connector Part Information

- OEM: 10756754
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbo Bypass Valve Solenoid (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | D-GN | 6391 | Turbo Bypass Valve Control
2 | PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turbocharger Boost Gauge (LNF)

#### Connector Part Information

- OEM: 12089248
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbocharger Boost Gauge (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PK | 439 | Ignition 1 Voltage
B | 0.35 GY | 8 | Instrument Panel Lamps Dimming Signal
C | 0.35 TN | 891 | Boost Gauge Signal
D | 0.35 BK/WH | 651 | Ground

### Turbocharger Boost Pressure Sensor (LNF)

#### Connector Part Information

- OEM: 15336035
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (NA)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbocharger Boost Pressure Sensor (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY | 597 | 5-Volt Reference
2 | 0.35 PU/WH | 7329 | PreThrottle Air Temp and Press (TMAP) Temperature Signal
3 | 0.5 TN | 407 | Low Reference
4 | 0.35 PU | 7330 | PreThrottle Air Temp and Press (TMAP) Air Pressure Signal

### Turbocharger Wastegate Solenoid (LNF)

#### Connector Part Information

- OEM: 10756754
- Service: See Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Turbocharger Wastegate Solenoid (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 YE | 258 | Wastegate Solenoid Control
2 | 0.5 PK/BK | 5293 | Powertrain Main Relay Fused Supply (4)

### Turn Signal/Multifunction Switch X1

#### Connector Part Information

- OEM: 15450317
- Service: 88987843
- Description: 8-Way F Misc (WH)

#### Terminal Part Information

- Terminal/Tray: SNAC-A03T-M040/20
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12094429/J-35616-12 (BU)

#### Turn Signal/Multifunction Switch X1

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 BK/WH | 651 | Ground
2 | 0.35 WH | 103 | Headlamp Switch Headlamps On Signal
3 | 0.35 BN/WH | 301 | Park Lamp Switch Signal
4 | 0.35 PU/WH | 549 | Headlamp Switch Headlamps Off Signal
5-8 | -- | -- | Not Used

### Turn Signal/Multifunction Switch X2

#### Connector Part Information

- OEM: 15393435
- Service: 88986438
- Description: 10-Way F Micro-Pack 064 Series (GY)

#### Terminal Part Information

- Terminal/Tray: 12177007/19
- Core/Insulation Crimp: E/2
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Turn Signal/Multifunction Switch X2

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 BK/WH | 651 | Ground
C | 0.35 BN | 1356 | Flash To Pass Switch Signal
D | 0.35 PU | 524 | Headlamp Dimmer Switch High Beam Signal
E | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
F | 0.35 YE | 10 | Headlamp Switch Signal
G | 0.35 YE/BK | 1418 | Left Turn Signal Switch Signal
H | 0.35 D-GN/WH | 1419 | Right Turn Signal Switch Signal
J-K | -- | -- | Not Used

### Vehicle Communication Interface Module (VCIM) X1 (UE1)

#### Connector Part Information

- OEM: 15431362
- Service: 15306351
- Description: 16-Way F Micro HVT (WH)

#### Terminal Part Information

- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12181559/J-35616-16 (L-GN)

#### Vehicle Communication Interface Module (VCIM) X1 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | 0.35 BN/WH | 2517 | Keypad Red LED Signal
3 | 0.35 YE/BK | 2516 | Keypad Green LED Signal
4-5 | -- | -- | Not Used
6 | 0.35 L-GN/BK | 2515 | Keypad Supply Voltage
7 | -- | -- | Not Used
8 | 0.5 BK/WH | 751 | Ground
9-10 | -- | -- | Not Used
11 | 0.35 D-GN/WH | 2514 | Keypad Signal
12-14 | -- | -- | Not Used
15 | 0.5 RD/WH | 1240 | Battery Positive Voltage
16 | -- | -- | Not Used

### Vehicle Communication Interface Module (VCIM) X2 (UE1)

#### Connector Part Information

- OEM: 15431365
- Service: 88952886
- Description: 12-Way F Micro 100A (WH)

#### Terminal Part Information

- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12181559/J-35616-16 (L-GN)

#### Vehicle Communication Interface Module (VCIM) X2 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 PK/BK | 2062 | Cellular Telephone Voice Signal
2 | 0.35 OG/BK | 2061 | Cellular Telephone Voice Low Reference
3-7 | -- | -- | Not Used
8 | BARE | 813 | Drain Wire
9 | 0.35 GY | 655 | Cellular Microphone Signal
10 | BARE | 1489 | Drain Wire
11-12 | -- | -- | Not Used

### Vehicle Communication Interface Module (VCIM) X3 (UE1)

#### Connector Part Information

- OEM: 15431368
- Service: 88988545
- Description: 12-Way F Micro 100A (BK)

#### Terminal Part Information

- Terminal/Tray: 15445905/23
- Core/Insulation Crimp: J/J
- Release Tool/Test Probe: 12181559/J-35616-16 (L-GN)

#### Vehicle Communication Interface Module (VCIM) X3 (UE1)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
2 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
3 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
4-7 | -- | -- | Not Used
8 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus (+)
9 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus (-)
10-12 | -- | -- | Not Used

### Vehicle Speed Sensor (VSS) (L61/LE5)

#### Connector Part Information

- OEM: 15449028
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: N/A
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Vehicle Speed Sensor (VSS) (L61/LE5)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 401 | VSS Low Signal (MN5/MX0)
0.35 PU/WH | 6356 | VSS Low Signal (M86)
B | 0.35 YE | 400 | VSS High Signal (MN5/MX0)
0.35 BN/WH | 6354 | VSS High Signal (M86)

### Vehicle Speed Sensor (VSS) (LNF)

#### Connector Part Information

- OEM: 15336004
- Service: N/A
- Description: 2-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: N/A
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: N/A

#### Vehicle Speed Sensor (VSS) (LNF)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 PU | 401 | VSS Low Signal
B | 0.35 YE | 400 | VSS High Signal

### Wheel Speed Sensor (WSS) - Left Front (JM4/JL9/JL4)

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Left Front (JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 830 | Left Front Wheel Speed Sensor Signal
B | 0.5 TN | 873 | Left Front Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Left Rear (L61/LE5 with JM4/JL9/JL4)

#### Connector Part Information

- OEM: 15305168
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Left Rear (L61/LE5 with JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 884 | Left Rear Wheel Speed Sensor Signal
B | 0.8 RD | 885 | Left Rear Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Left Rear (LNF with JM4/JL9/JL4)

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Left Rear (LNF with JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BK | 884 | Left Rear Wheel Speed Sensor Signal
B | 0.8 RD | 885 | Left Rear Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Right Front (JM4/JL9/JL4)

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Right Front (JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
B | 0.5 TN | 833 | Right Front Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Right Rear (L61/LE5 with JM4/JL9/JL4)

#### Connector Part Information

- OEM: 15305168
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Right Rear (L61/LE5 with JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal
B | 0.8 WH | 883 | Right Rear Wheel Speed Sensor Low Reference

### Wheel Speed Sensor (WSS) - Right Rear (LNF with JM4/JL9/JL4)

#### Connector Part Information

- OEM: 12052644
- Service: See Catalog
- Description: 2-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Wheel Speed Sensor (WSS) - Right Rear (LNF with JM4/JL9/JL4)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal
B | 0.8 WH | 883 | Right Rear Wheel Speed Sensor Low Reference

### Window Motor - Driver (AU3/DG7)

#### Connector Part Information

- OEM: 12129487
- Service: 12167133
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Motor - Driver (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 164 | Power Window Motor Left Front Up Control (Coupe)
A | 2 BN | 165 | Power Window Motor Left Front Down Control (Sedan)
B | 2 BN | 165 | Power Window Motor Left Front Down Control (Coupe)
B | 2 D-BU | 164 | Power Window Motor Left Front Up Control (Sedan)

### Window Motor - Front Passenger (AU3/DG7)

#### Connector Part Information

- OEM: 12129487
- Service: 12167133
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Motor - Front Passenger (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 666 | Power Window Motor Right Front Up Control (Coupe)
A | 2 BN | 667 | Power Window Motor Right Front Down Control (Sedan)
B | 2 BN | 667 | Power Window Motor Right Front Down Control (Coupe)
B | 2 D-BU | 666 | Power Window Motor Right Front Up Control (Sedan)

### Window Motor - Left Rear (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 12129487
- Service: 12167133
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Motor - Left Rear (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 668 | Power Window Motor Left Rear Up Control
B | 2 BN | 669 | Power Window Motor Left Rear Down Control

### Window Motor - Right Rear (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 12129487
- Service: 12167133
- Description: 2-Way F Metri-Pack 280 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12110845/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Motor - Right Rear (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 670 | Power Window Motor Right Rear Up Control
B | 2 BN | 671 | Power Window Motor Right Rear Down Control

### Window Switch - Driver (Coupe) (AU3/DG7)

#### Connector Part Information

- OEM: 15326924
- Service: 12167133
- Description: 8-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Driver (Coupe) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 L-BU | 166 | Power Window Master Switch Right Front Up Signal
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D | 2 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 2 BK | 650 | Ground
G | 2 D-BU | 164 | Power Window Motor Left Front Up Control
H | 2 BN | 165 | Power Window Motor Left Front Down Control

### Window Switch - Driver X1 (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 15326900
- Service: See Catalog
- Description: 6-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Driver X1 (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.35 BN | 165 | Power Window Motor Left Front Down Control
B | 2 L-BU | 166 | Power Window Master Switch Right Front Up Signal
C | 0.35 TN | 167 | Power Window Master Switch Right Front Down Signal
D | -- | -- | Not Used
E | 0.35 D-BU | 164 | Power Window Motor Left Front Up Control
F | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage

### Window Switch - Driver X2 (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 15326924
- Service: See Catalog
- Description: 8-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Driver X2 (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.5 BK | 650 | Ground
C | 2 PU | 169 | Power Window Master Switch Left Rear Down Signal
D | 2 D-GN | 168 | Power Window Master Switch Left Rear Up Signal
E | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
F | 2 D-BU | 1307 | Power Window Master Switch Lockout Signal
G | 2 L-GN | 170 | Power Window Master Switch Right Rear Up Signal
H | 2 PU | 171 | Power Window Master Switch Right Rear Down Signal

### Window Switch - Front Passenger (AU3/DG7)

#### Connector Part Information

- OEM: 12191825
- Service: See Catalog
- Description: 8-Way F GT 280 Series Sealed (BN)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Front Passenger (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
B | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
C | 0.5 BK | 650 | Ground
D | 3 TN | 167 | Power Window Master Switch Right Front Down Signal
E | -- | -- | Not Used
F | 3 BN | 667 | Power Window Motor Right Front Down Control
G | 3 D-BU | 666 | Power Window Motor Right Front Up Control
H | 3 L-BU | 166 | Power Window Master Switch Right Front Up Signal

### Window Switch - Left Rear (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 12191825
- Service: See Catalog
- Description: 8-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Left Rear (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 1307 | Power Window Master Switch Lockout Signal
B-C | -- | -- | Not Used
D | 2 PU | 169 | Power Window Master Switch Left Rear Down Signal
E | -- | -- | Not Used
F | 2 BN | 669 | Power Window Motor Left Rear Down Control
G | 2 D-BU | 668 | Power Window Motor Left Rear Up Control
H | 2 D-GN | 168 | Power Window Master Switch Left Rear Up Signal

### Window Switch - Right Rear (Sedan) (AU3/DG7)

#### Connector Part Information

- OEM: 12191825
- Service: See Catalog
- Description: 8-Way F GT 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15304712/2
- Core/Insulation Crimp: C
- Release Tool/Test Probe: 12094430/J-35616-42 (RD)

#### Window Switch - Right Rear (Sedan) (AU3/DG7)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 2 D-BU | 1307 | Power Window Master Switch Lockout Signal
B-C | -- | -- | Not Used
D | 2 PU | 171 | Power Window Master Switch Right Rear Down Signal
E | -- | -- | Not Used
F | 2 D-BU | 670 | Power Window Motor Right Rear Up Control
G | 2 BN | 671 | Power Window Motor Right Rear Down Control
H | 2 L-GN | 170 | Power Window Master Switch Right Rear Up Signal

### Windshield Washer Fluid Pump

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Washer Fluid Pump

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | 0.5 OG | 228 | Windshield Washer Pump Control
B | 0.5 BK | 150 | Ground

### Windshield Wiper Motor

#### Connector Part Information

- OEM: 10811710
- Service: 88987987
- Description: 4-Way F Timer JR-Power Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Windshield Wiper Motor

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 1 PU | 92 | Windshield Wiper Motor High Speed Control
2 | 1 D-GN | 95 | Windshield Wiper Motor Low Speed Control
3 | 0.5 YE | 196 | Windshield Wiper Motor Park Switch Signal
4 | 1 BK | 150 | Ground

### Windshield Wiper/Washer Switch

#### Connector Part Information

- OEM: 12059800
- Service: 15306169
- Description: 5-Way F Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12064971/5
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Windshield Wiper/Washer Switch

Pin | Wire | Circuit | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | 0.35 OG | 228 | Windshield Washer Pump Control
C | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
D | 0.35 PK | 439 | Ignition 1 Voltage
E | 0.35 GY | 112 | Windshield Wiper Switch Signal 1

### Yaw and Lateral Acceleration Sensor (JL4/JL9)

#### Connector Part Information

- OEM: 10750569
- Service: See Catalog
- Description: 6-Way F MQS Socket Housing, Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Yaw and Lateral Acceleration Sensor (JL4/JL9)

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | 0.5 GY/BK | 6435 | CAN Bus Low Serial Data
2 | 0.5 PK/BK | 6434 | CAN Bus High Serial Data
3 | 0.5 D-GN | 2087 | 12-Volt Reference
4 | -- | -- | Not Used
5 | 0.5 L-BU | 2088 | Low Reference
6 | -- | -- | Not Used