For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pipe Fitting | 19 N·m | 14 lb ft
Brake Pressure Modulator Valve (BPMV) to Mounting Bracket Bolt | 11 N·m | 97 lb in
BPMV Mounting Bracket Bolt | 25 N·m | 18 lb ft
BPMV Mounting Pin | 10 N·m | 89 lb in
Electronic Brake Control Module (EBCM) Bolt (With JL4) | 3 N·m | 27 lb in
EBCM Bolt (Without JL4) | 2.3 N·m | 20 lb in
Engine Control Module (ECM) Bracket and BPMV Bracket Mounting Bolt | 12 N·m | 106 lb in
Yaw Rate Sensor Nut | 10 N·m | 89 lb in