For 1990-2009 cars

## Rear Turn Signal Lamp Bulb Replacement Chevrolet Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Wire Harness Connector Tip Rotate counter-clockwise and remove from the tail lamp housing.
2 | Tail Stop / Turn Signal Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Remove the bulb from the wire harness connector.

## Rear Turn Signal Lamp Bulb Replacement Chevrolet / Pontiac Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear tail lamp assembly. Refer to Tail Lamp Replacement.

1 | Rear Stop Tail Turn Signal Lamp Socket Tip Twist and remove the bulb socket from the tail lamp assembly.
2 | Stop Tail Turn Signal Lamp Bulb Warning: Refer to Halogen Bulb Warning in the Preface section. Tip Remove the stop tail turn signal lamp bulb.