For 1990-2009 cars

Connector 1: | Battery Current Sensor
Connector 2: | Clutch Pedal Postion (CPP) Switch (M86)
Connector 3: | Clutch Start Switch (M86)
Connector 4: | Generator (LSJ)
Connector 5: | Generator (L61/LE5)

### Battery Current Sensor

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Battery Current Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GY | 596 | 5-Volt Reference-1
B | TN/WH | 1704 | Sensor Low Reference
C | WH | 5075 | Current Sensor Signal

### Clutch Pedal Postion (CPP) Switch (M86)

#### Connector Part Information

- OEM: 15479480
- Service: 88988317
- Description: 2-Way F Micro-Pack 280 Series (L-GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Clutch Pedal Postion (CPP) Switch (M86)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BN/WH | 379 | CPP Switch Signal
B | PK/BK | 5291 | Ignition 1 Voltage

### Clutch Start Switch (M86)

#### Connector Part Information

- OEM: 12041433
- Service: 12126463
- Description: 2-Way F Metri-Pack 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12034046/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Clutch Start Switch (M86)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK | 339 | Ignition 1 Voltage
B | YE | 575 | Starter Control

### Generator (LSJ)

#### Connector Part Information

- OEM: 15355066
- Service: 15306329
- Description: 2-Way F Metri-Pack 150 Series Sealed (BG)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Generator (LSJ)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Available
B | RD | 225 | Generator Turn On Signal
C | GY | 23 | Generator Field Duty Cycle Signal
D | -- | -- | Not Available

### Generator (L61/LE5)

#### Connector Part Information

- OEM: 12186308
- Service: 89046837
- Description: 2-Way F Timer JR-Power Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 4-964286-1/16
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12093647/J-35616-4A (PU)

#### Generator (L61/LE5)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 225 | Generator Turn On Signal
2 | GY | 23 | Generator Field Duty Cycle Signal