For 1990-2009 cars

Table 1: | Engine Specifications

The following approximate capacities are given in English and metric conversions. Please refer to Recommended Fluids and Lubricantsfor more information.

Application | Capacities
--- | ---
English | Metric
Air Conditioning Refrigerant R134a | For the air conditioning system refrigerant charge amount, see the refrigerant caution label located under the hood. See your dealer/retailer for more information.
Cooling System

- 2.2L L4 Engine

7.4 qt

7.0 L

Engine Oil with Filter

- 2.2L L4 Engine

5.0 qt

4.7 L

Fuel Tank

- 2.2L L4 Engine (with NU6 emissions)

13.5 gal

51.1 L

- 2.2L L4 Engine (without NU6 emissions)

13.0 gal

49.2 L

Transmission Fluid (Drain and Refill)

- Transmission, Automatic

7.0 qt

6.6 L

- Transmission, Manual

1.7 qt

1.6 L

Wheel Nut Torque | 100 lb ft | 140 N·m
All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual.

#### Engine Specifications

Engine | VIN Code | Transmission | Spark Plug Gap
--- | --- | --- | ---
2.2L L4 Engine | H | Automatic Manual | 0.040 in (1.01 mm)