For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Check Link Bolts | 20 N·m | 15 lb ft
Door Check Link Nuts | 10 N·m | 89 lb in
Door Lock Screws | 10 N·m | 89 lb in
Door Striker Screws | 25 N·m | 18 lb ft
Front Side Door Lock Screws | 10 N·m | 89 lb in
Front Side Door Outside Handle Screws | 10 N·m | 89 lb in
Hinge to Body Bolts | 35 N·m | 26 lb ft
Hinge to Door Bolts | 25 N·m | 18 lb ft
Rear Compartment Lid Latch Bolts | 10 N·m | 89 lb in
Rear Compartment Lid Latch Striker Bolts | 10 N·m | 89 lb in
Rear Side Door Outside Handle Screws | 10 N·m | 89 lb in
Rear Side Door Lock Screws | 10 N·m | 89 lb in
Side Door Inside Cover Screw | 2 N·m | 18 lb in