For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Arm Rest Mounting Bolts | 9 N·m | 80 lb in
Console Mounting Screws | 2 N·m | 18 lb in
I/P Compartment Door Screws | 2 N·m | 18 lb in
I/P Pad Screws | 2.2 N·m | 19 lb in
I/P Retainer Bolts | 9 N·m | 80 lb in
I/P Retainer Nuts | 9 N·m | 80 lb in
I/P Retainer Screws | 9 N·m | 80 lb in
Knee Bolster Trim Screws | 2 N·m | 18 lb in
Radio to I/P | 9 N·m | 80 lb in