For 1990-2009 cars

## Lock Pillar Upper Garnish Molding Replacement Coupe

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.
1 | Panel Assembly, C Pillar Trim Upper
2 | Clip, Retainer (Qty: 9)

## Lock Pillar Upper Garnish Molding Replacement Sedan

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .
1 | Cover, Screw Upper Quarter Trim
2 | Screw, Upper Quarter Trim Tighten 2 N·m (18 lb in)
3 | Panel Assembly, Upper Quarter Trim
4 | Clip, Upper Quarter Trim