For 1990-2009 cars

Table 1: | Body Control Module (BCM)
Table 2: | Electronic Brake Control Module (EBCM)
Table 3: | Powertrain Control Module (PCM)

#### Body Control Module (BCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
Brake Fluid Level Sensor | BCM Data | Yes/No | OK/Low
ETS Switch | BCM Data | On/Off | Off

#### Electronic Brake Control Module (EBCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
ABS Active | EBCM Data | Yes/No | No
ABS Warning Lamp | EBCM Data | On/Off | Off
Ignition Voltage | EBCM Data | Volts | B+
LF Inlet Solenoid Command | EBCM Data | On/Off | Off
LF Outlet Solenoid Command | EBCM Data | On/Off | Off
LF Wheel Speed Sensor | EBCM Data | mph/km/h | 0
LR Inlet Solenoid Command | EBCM Data | On/Off | Off
LR Outlet Solenoid Command | EBCM Data | On/Off | Off
LR Wheel Speed Sensor | EBCM Data | mph/km/h | 0
Pump Motor Command | EBCM Data | On/Off | Off
Pump Motor Feedback Signal | EBCM Data | On/Off | Off
RF Inlet Solenoid Command | EBCM Data | On/Off | Off
RF Outlet Solenoid Command | EBCM Data | On/Off | Off
RF Wheel Speed Sensor | EBCM Data | mph/km/h | 0
RR Inlet Solenoid Command | EBCM Data | On/Off | Off
RR Outlet Solenoid Command | EBCM Data | On/Off | Off
RR Wheel Speed Sensor | EBCM Data | mph/km/h | 0
Rough Road Parameter | EBCM Data | g | Varies
Solenoid Relay Feedback Signal | EBCM Data | On/Off | On
Solenoid Relay Command | EBCM Data | On/Off | On
Traction Active Lamp | EBCM Data | On/Off | Off
Traction Disabled | EBCM Data | Yes/No | No
Traction Off Lamp | EBCM Data | On/Off | Off
Vehicle Speed | EBCM Data | mph/km/h | 0

#### Powertrain Control Module (PCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
Torque Request Signal | PCM Data | % | 90
Traction Control Status | PCM Data | Active/Inactive | Inactive
Vehicle Speed | PCM Data | mph/km/h | 0