For 1990-2009 cars

Connector 1: | Inflatable Restraint Front End Sensor
Connector 2: | Inflatable Restraint Front Passenger Presence System (PPS) Module
Connector 3: | Inflatable Restraint Front Passenger Presence System (PPS) Sensor
Connector 4: | Inflatable Restraint I/P Module C1
Connector 5: | Inflatable Restraint I/P Module C2
Connector 6: | Inflatable Restraint Passenger Air Bag On/Off Indicator
Connector 7: | Inflatable Restraint Passenger Seat Belt Tension Sensor
Connector 8: | Inflatable Restraint Roof Rail Module - Left (ASF)
Connector 9: | Inflatable Restraint Roof Rail Module - Right (ASF)
Connector 10: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/ASF)
Connector 11: | Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/o ASF)
Connector 12: | Inflatable Restraint Side Impact Sensor - Left (ASF)
Connector 13: | Inflatable Restraint Side Impact Sensor - Right (ASF)
Connector 14: | Inflatable Restraint Steering Wheel Module C1
Connector 15: | Inflatable Restraint Steering Wheel Module C2
Connector 16: | Inflatable Restraint Steering Wheel Module Coil C1
Connector 17: | Inflatable Restraint Steering Wheel Module Coil C2
Connector 18: | Inflatable Restraint Steering Wheel Module Coil C3
Connector 19: | Seat Belt Retractor Pretensioner - Driver
Connector 20: | Seat Belt Retractor Pretensioner - Passenger

### Inflatable Restraint Front End Sensor

#### Connector Part Information

- OEM: 15356722
- Service: 15306405
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front End Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN/OG | 5045 | Discriminating Sensor - Low Reference
B | YE | 1834 | Forward Discriminating Sensor Signal

### Inflatable Restraint Front Passenger Presence System (PPS) Module

#### Connector Part Information

- OEM: 15431682
- Service: Service by Harness - See Part Catalog
- Description: 18-Way F Micro-Pack 100W Series Sealed (BK)

#### Terminal Part Information

- Pins: 1, 2, 4, 6, 7, 9, 14-16, 18
- Terminal/Tray: Service With Terminated Lead
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12122523/J-35616-6 (BN)

- Pins: 5
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Front Passenger Presence System (PPS) Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN/BK | 723 | Passenger Air Bag On Indicator Control
2 | L-GN | 353 | Passenger Air Bag Off Indicator Control
3 | -- | -- | Not Used
4 | D-BU | 913 | Passenger Seat Belt Tension Sensor Signal
5 | BK/WH | 1251 | Ground
6 | PK/WH | 916 | Passenger Presence Sensor Signal
7 | D-BU/WH | 918 | 5-Volt Reference
8 | -- | -- | Not Used
9 | PK | 1339 | Ignition 1 Voltage
10-13 | -- | -- | Not Used
14 | YE | 914 | Low Reference
15 | YE/WH | 917 | Low Reference
16 | PK/BK | 915 | 5-Volt Reference
17 | -- | -- | Not Used
18 | PU | 5018 | Occupant Sensor Serial Data

### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

#### Connector Part Information

- OEM: 15422250
- Service: 88987995
- Description: 3-Way F GT 150 Series Sealed (D-GY)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Inflatable Restraint Front Passenger Presence System (PPS) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-BU/WH | 918 | 5-Volt Reference
B | PK/WH | 916 | Passenger Presence Sensor Signal
C | YE/WH | 917 | Low Reference

### Inflatable Restraint I/P Module C1

#### Connector Part Information

- OEM: 699467-7
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 90 Degree Lockable (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD/WH | 3025 | I/P Module Stage 1 High Control
B | L-GN/OG | 3024 | I/P Module Stage 1 Low Control

### Inflatable Restraint I/P Module C2

#### Connector Part Information

- OEM: 699467-7
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F 90 Degree Lockable (GY) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint I/P Module C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK/BK | 3026 | I/P Module Stage 2 Low Control
B | L-BU/OG | 3027 | I/P Module Stage 2 High Control

### Inflatable Restraint Passenger Air Bag On/Off Indicator

#### Connector Part Information

- OEM: 15398877
- Service: 88953374
- Description: 5-Way F (WH)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Air Bag On/Off Indicator

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN/BK | 723 | Passenger Air Bag On Indicator Control
2 | BK | 550 | Ground
3 | PK | 353 | Passenger Air Bag Off Indicator Control
4 | PK | 339 | Ignition 1 Voltage
5 | PU | 5234 | Passenger Seat Belt Indicator

### Inflatable Restraint Passenger Seat Belt Tension Sensor

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Passenger Seat Belt Tension Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK/BK | 915 | 5-Volt Reference
B | YE | 914 | Low Reference
C | D-BU | 913 | Passenger Seat Belt Tension Sensor Signal

### Inflatable Restraint Roof Rail Module - Left (ASF)

#### Connector Part Information

- OEM: CA-252-92-5-Q
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Left (ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 5019 | Roof Rail Module - Left - High Control
2 | WH | 5020 | Roof Rail Module - Left - Low Control

### Inflatable Restraint Roof Rail Module - Right (ASF)

#### Connector Part Information

- OEM: CA-252-92-5-Q
- Service: 15306044
- Description: 2-Way F (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Roof Rail Module - Right (ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 5021 | Roof Rail Module - Right - High Control
2 | WH | 5022 | Roof Rail Module - Right - Low Control

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/ASF)

#### Connector Part Information

- OEM: 15488865
- Service: 88988832
- Description: 60-Way F Micro-Pack 64 Series (RD) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | 1240 | Battery Positive Voltage
2 | D-GN | 5060 | Low Speed GMLAN Serial Data
3 | PK | 5057 | Low Reference
4 | TN/WH | 238 | Seat Belt Switch Left
5 | -- | -- | Not Available
6 | OG | 1362 | Passenger Seat Belt Switch Right
7 | -- | -- | Not Available
8 | PK | 5020 | Roof Rail Module - Left - Low Control
9 | PU/WH | 5019 | Roof Rail Module - Left - High Control
10 | YE/BK | 5021 | Roof Rail Module - Right - High Control
11 | WH/BK | 5022 | Roof Rail Module - Right - Low Control
12 | PU | 3026 | I/P Module Stage 2 Low Control
13 | GY | 3027 | I/P Module Stage 2 High Control
14 | TN | 3021 | Steering Wheel Module Stage 1 High Control
15 | BN | 3020 | Steering Wheel Module Stage 1 Low Control
16 | PK | 3022 | Steering Wheel Module Stage 2 Low Control
17 | WH | 3023 | Steering Wheel Module Stage 2 High Control
18 | YE | 3025 | I/P Module Stage 1 High Control
19 | OG | 3024 | I/P Module Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | PK | 1339 | Ignition 1 Voltage
34-37 | -- | -- | Not Available
38 | YE | 1834 | Forward Discriminating Sensor Signal
39 | TN/OG | 5045 | Discriminating Sensor Low Reference
40-45 | -- | -- | Not Available
46 | WH | 2132 | Side Impact Sensing Module - Left - Signal
47 | YE | 2131 | Side Impact Sensing Module - Left - Voltage
48 | TN | 2133 | Side Impact Sensing Module - Right - Voltage
49 | D-GN | 2134 | Side Impact Sensing Module - Right - Signal
50-51 | -- | -- | Not Available
52 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
53 | OG | 2117 | Seat Belt Pretensioner - Right - Low Control
54-55 | -- | -- | Not Available
56 | TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
57 | OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
58-59 | -- | -- | Not Available
60 | PK | 5018 | Occupant Sensor - Serial Data

### Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/o ASF)

#### Connector Part Information

- OEM: 15456067
- Service: 88988825
- Description: 60-Way F Micro-Pack 64 Series (BU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Sensing and Diagnostic Module (SDM) (w/o ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | RD/WH | 1240 | Battery Positive Voltage
2 | D-GN | 5060 | Low Speed GMLAN Serial Data
3 | PK | 5057 | Seat Position Sensor - Low Reference
4 | TN/WH | 238 | Seat Belt Switch - Left
5 | -- | -- | Not Available
6 | OG | 1362 | Seat Belt Switch - Right
7-11 | -- | -- | Not Available
12 | PU | 3026 | I/P Module Stage 2 Low Control
13 | GY | 3027 | I/P Module Stage 2 High Control
14 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control
15 | BN | 3020 | Steering Wheel Module Stage 1 Low Control
16 | PK | 3022 | Steering Wheel Module Stage 2 Low Control
17 | WH | 3023 | Steering Wheel Module Stage 2 High Control
18 | YE | 3025 | I/P Module Stage 1 High Control
19 | OG | 3024 | I/P Module Stage 1 Low Control
20-30 | -- | -- | Not Available
31 | BK/WH | 351 | Ground
32 | -- | -- | Not Available
33 | PK | 1339 | Ignition 1 Voltage
34-37 | -- | -- | Not Available
38 | YE | 1834 | Forward Discriminating Sensor Signal
39 | TN/OG | 5045 | Discriminating Sensor - Low Reference
40-51 | -- | -- | Not Available
52 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control
53 | OG | 2117 | Seat Belt Pretensioner - Right - Low Control
54-55 | -- | -- | Not Available
56 | TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control
57 | OG/BK | 2119 | Seat Belt Pretensioner - Lef t- Low Control
58-59 | -- | -- | Not Available
60 | PK | 5018 | Occupant sensor serial Data

### Inflatable Restraint Side Impact Sensor - Left (ASF)

#### Connector Part Information

- OEM: 15356724
- Service: 15306418
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Side Impact Sensor - Left (ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 2131 | Side Impact Sensing Module - Left - Voltage
B | WH | 2132 | Side Impact Sensing Module - Left - Signal

### Inflatable Restraint Side Impact Sensor - Right (ASF)

#### Connector Part Information

- OEM: 15356724
- Service: 15306418
- Description: 2-Way F GT 150 Series Sealed (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Side Impact Sensor - Right (ASF)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN | 2133 | Side Impact Sensing Module - Right - Voltage
B | D-GN | 2134 | Side Impact Sensing Module - Right - Signal

### Inflatable Restraint Steering Wheel Module C1

#### Connector Part Information

- OEM: CA-252-92-5-R
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F AMP (WH) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | TN | 3021 | Steering Wheel Module - Stage 1 - High Control
2 | BN | 3020 | Steering Wheel Module - Stage 1 - Low Control

### Inflatable Restraint Steering Wheel Module C2

#### Connector Part Information

- OEM: CA-252-92-5-R
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F AMP (PU) With (YE) Case

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH | 3023 | Steering Wheel Module - Stage 2 - High Control
2 | PK | 3022 | Steering Wheel Module-Stage 2 - Low Control

### Inflatable Restraint Steering Wheel Module Coil C1

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 (BK)

#### Terminal Part Information

- Pins: C, F, K
- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

- Pins: D, E, G, J
- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | PK | 339 | Ignition 1 Voltage
D | GY | 1884 | Cruise Control Switch Signal (K34)
E | D-BU | 1796 | Remote Radio Control Signal (UK3)
F | WH/BK | 1673 | 12-Volt Reference (UK3)
G | GY | 8 | Instrument Panel Lamp Supply Voltage
H | D-GN/WH | 1358 | Driver Information Center Switch Signal
J | TN | 28 | Horn Relay Control
K | BK | 151 | Ground

### Inflatable Restraint Steering Wheel Module Coil C2

#### Connector Part Information

- OEM: 15393433
- Service: 22710638
- Description: 10-Way F Micro-Pack 064 (BK)

#### Terminal Part Information

- Terminal/Tray: Service with Terminated Lead
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: 12180559-1/J-35616-64B (L-BU)

#### Inflatable Restraint Steering Wheel Module Coil C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | PK | 1539 | Ignition 1 Voltage (K34)
D | GY/BK | 1884 | Cruise Control Switch Signal (K34)
E | D-BU | 1796 | Steering Wheel Controls Signal (UK3)
F | WH/BK | 644 | 12-Volt Reference (UK3)
G | GY | 8 | Instrument Panel Lamp Supply Voltage
H | D-GN/WH | 1358 | Driver Information Center Switch Signal
J | TN | 28 | Horn Relay Control
K | BK/WH | 1051 | Ground

### Inflatable Restraint Steering Wheel Module Coil C3

#### Connector Part Information

- OEM: 15393421
- Service: 88987853
- Description: 4-Way F Micro-Pack 064 (YE)

#### Terminal Part Information

- Terminal/Tray: Service with Pigtail
- Core/Insulation Crimp: N/A
- Release Tool/Test Probe: See Terminal Repair Kit

#### Inflatable Restraint Steering Wheel Module Coil C3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 3020 | Steering Wheel Module Stage 2 Low Control
2 | TN | 3021 | Steering Wheel Module Stage 2 High Control
3 | PK | 3022 | Steering Wheel Module Stage 1 Low Control
4 | WH | 3023 | Steering Wheel Module Stage 1 High Control

### Seat Belt Retractor Pretensioner - Driver

#### Connector Part Information

- OEM: 15380395
- Service: 88988308
- Description: 2-Way F MISC (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG/BK | 2119 | Seat Belt Pretensioner - Left - Low Control
2 | TN/WH | 2118 | Seat Belt Pretensioner - Left - High Control

### Seat Belt Retractor Pretensioner - Passenger

#### Connector Part Information

- OEM: 15380395
- Service: 88988308
- Description: 2-Way F MISC (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Retractor Pretensioner - Passenger

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | OG | 2117 | Seat Belt Pretensioner - Right - Low Control
2 | L-GN | 2116 | Seat Belt Pretensioner - Right - High Control