For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Front Stabilizer Shaft Link Nut (Qty: 2) Tighten 65 N·m (48 lb ft)
2 | Front Stabilizer Shaft Link