For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Operating Conditions: Ignition ON, Engine OFF, All doors and trunk closed
Door Ajar Sw | Data Display | Door Closed/Door Ajar | Door Closed
Door Lock Switch | Data Display | Volts | 10.9
Door Lock Switch | Data Display | Idle/Unlock/Lock | Idle
Driver Door Lock Actuator Command | Data Display | Idle/Unlock/Lock/Invalid | Idle
Passenger Doors Lock Actuator Command | Data Display | Idle/Unlock/Lock/Invalid | Idle
Driver Door Ajar Sw | Data Display | Door Closed/Door Ajar | Door Closed
Trunk Ajar Switch | Data Display | Trunk Closed/Trunk Ajar | Trunk Closed
Trunk Motor | Data Display | On/Off | Off
Trunk Release Solenoid Command | Data Display | On/Off | Off
Trunk Release Switch | Data Display | Active/Inactive | Inactive