For 1990-2009 cars

Connector 1: | Accelerator Pedal Position (APP) Sensor
Connector 2: | Camshaft Position (CMP) Actuator Solenoid - Exhaust
Connector 3: | Camshaft Position (CMP) Actuator Solenoid - Intake
Connector 4: | Camshaft Position (CMP) Sensor - Exhaust
Connector 5: | Camshaft Position (CMP) Sensor - Intake
Connector 6: | Crankshaft Position (CKP) Sensor
Connector 7: | Engine Coolant Temperature (ECT) Sensor
Connector 8: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Connector 9: | Evaporative Emission (EVAP) Canister Vent Solenoid Valve
Connector 10: | Fuel Injector 1
Connector 11: | Fuel Injector 2
Connector 12: | Fuel Injector 3
Connector 13: | Fuel Injector 4
Connector 14: | Fuel Pump and Sender Assembly
Connector 15: | Fuel Tank Pressure (FTP) Sensor
Connector 16: | Heated Oxygen Sensor (HO2S) 1
Connector 17: | Heated Oxygen Sensor (HO2S) 2
Connector 18: | Ignition Coil/Module 1
Connector 19: | Ignition Coil/Module 2
Connector 20: | Ignition Coil/Module 3
Connector 21: | Ignition Coil/Module 4
Connector 22: | Knock Sensor (KS)
Connector 23: | Manifold Absolute Pressure (MAP) Sensor
Connector 24: | Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor
Connector 25: | Throttle Actuator Control (TAC) Module

### Accelerator Pedal Position (APP) Sensor

#### Connector Part Information

- OEM: 15326830
- Service: 88953153
- Description: 6-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Accelerator Pedal Position (APP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PU | 1272 | 5-Volt Reference - 1
B | L-BU | 1162 | APP Sensor 2 Signal
C | TN | 1274 | Low Reference
D | BN | 1271 | Low Reference
E | D-BU | 1161 | APP Sensor 1 Signal
F | WH/BK | 1164 | 5-Volt Reference - 2

### Camshaft Position (CMP) Actuator Solenoid - Exhaust

#### Connector Part Information

- OEM: 15336004
- Service: 15306187
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Actuator Solenoid - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH/BK | 6396 | CMP Actuator Solenoid Control Exhaust
B | L-GN | 5282 | Low Reference

### Camshaft Position (CMP) Actuator Solenoid - Intake

#### Connector Part Information

- OEM: 15335987
- Service: 15306430
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A
- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: B
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Camshaft Position (CMP) Actuator Solenoid - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK/BK | 6395 | CMP Actuator Solenoid Control Intake
B | PU | 5284 | Low Reference

### Camshaft Position (CMP) Sensor - Exhaust

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Exhaust

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE/BK | 5297 | 5-Volt Reference - 1
B | GY | 5296 | Low Reference
C | D-GN | 5273 | CMP Sensor Signal

### Camshaft Position (CMP) Sensor - Intake

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Camshaft Position (CMP) Sensor - Intake

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-BU | 5300 | 5-Volt Reference - 1
B | TN | 5301 | Low Reference
C | OG | 5275 | CMP Sensor Signal

### Crankshaft Position (CKP) Sensor

#### Connector Part Information

- OEM: 15326808
- Service: 15306388
- Description: 3-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Crankshaft Position (CKP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-GN | 2867 | 5-Volt Reference - 2
B | PU | 574 | Low Reference
C | YE | 573 | CKP Sensor Signal

### Engine Coolant Temperature (ECT) Sensor

#### Connector Part Information

- OEM: 15449028
- Service: 88987993
- Description: 2-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 15326267/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Engine Coolant Temperature (ECT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN | 2761 | Low Reference
B | YE | 410 | ECT Sensor Signal

### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PK/WH | 5291 | Ignition 1 Voltage
B | D-GN/WH | 428 | EVAP Canister Purge Solenoid Control

### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

#### Connector Part Information

- OEM: 12052643
- Service: 12101858
- Description: 2-Way F Metri-Pack 150 Series Sealed (RD)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Evaporative Emission (EVAP) Canister Vent Solenoid Valve

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RD/WH | 1840 | Battery Positive Voltage
B | WH | 1310 | EVAP Canister Vent Solenoid Control

### Fuel Injector 1

#### Connector Part Information

- OEM: 7283-8596-30
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | TN/BK | 1744 | Fuel Injector 1 Control

### Fuel Injector 2

#### Connector Part Information

- OEM: 7283-8596-30
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | L-GN/BK | 1745 | Fuel Injector 2 Control

### Fuel Injector 3

#### Connector Part Information

- OEM: 7283-8596-30
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | PK/BK | 1746 | Fuel Injector 3 Control

### Fuel Injector 4

#### Connector Part Information

- OEM: 7283-8596-30
- Service: Service by Harness - See Part Catalog
- Description: 2-Way F Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Injector 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PK | 139 | Ignition 1 Voltage
2 | L-BU/BK | 844 | Fuel Injector 4 Control

### Fuel Pump and Sender Assembly

#### Connector Part Information

- OEM: 15324787
- Service: 15306349
- Description: 4-Way F Apex (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Pump and Sender Assembly

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 120 | Fuel Pump Supply Voltage
2 | PU | 1589 | Fuel Level Sensor Signal
3 | BK/WH | 850 | Ground
4 | BK | 1250 | Ground

### Fuel Tank Pressure (FTP) Sensor

#### Connector Part Information

- OEM: 12059595
- Service: 88986451
- Description: 3-Way F Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Fuel Tank Pressure (FTP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK/WH | 2759 | Low Reference
B | D-GN | 890 | Fuel Tank Pressure Sensor Signal
C | GY/BK | 2709 | 5-Volt Reference 1

### Heated Oxygen Sensor (HO2S) 1

#### Connector Part Information

- OEM: 12176897
- Service: 15305960
- Description: 4-Way F Metri-Pack 150 Series Sealed (L-GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Heated Oxygen Sensor (HO2S) 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN/WH | 3111 | HO2S Low Signal Sensor 1
B | PU/WH | 3110 | HO2S High Signal Sensor 1
C | GY/WH | 3113 | HO2S Heater Low Control Sensor 1
D | PK/BK | 5291 | Ignition 1 Voltage

### Heated Oxygen Sensor (HO2S) 2

#### Connector Part Information

- OEM: 12160825
- Service: 15305801
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12045773/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

#### Heated Oxygen Sensor (HO2S) 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TN/WH | 1669 | HO2S Low Signal Sensor 2
B | PU/OG | 1668 | HO2S High Signal Sensor 2
C | GY/BK | 3122 | HO2S Heater Low Control Sensor 2
D | PK/BK | 5291 | Ignition 1 Voltage

### Ignition Coil/Module 1

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B-D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil/Module 1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1350 | Ground
B | BN | 2129 | Low Reference
C | PU | 2121 | IC 1 Control
D | PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 2

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B-D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil/Module 2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1350 | Ground
B | BN | 2129 | Low Reference
C | OG/WH | 2122 | IC 2 Control
D | PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 3

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B-D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil/Module 3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1350 | Ground
B | BN | 2129 | Low Reference
C | L-BU | 2123 | IC 3 Control
D | PK/BK | 5292 | Ignition 1 Voltage

### Ignition Coil/Module 4

#### Connector Part Information

- OEM: 15466325
- Service: 88988737
- Description: 4-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B-D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Ignition Coil/Module 4

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK | 1350 | Ground
B | BN | 2129 | Low Reference
C | D-GN/WH | 2124 | IC 4 Control
D | PK/BK | 5292 | Ignition 1 Voltage

### Knock Sensor (KS)

#### Connector Part Information

- OEM: 12077900
- Service: 12116247
- Description: 2-Way F Metri-Pack 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12077411/2
- Core/Insulation Crimp: 2/5
- Release Tool/Test Probe: 12094430/J-35616-4A (PU)

#### Knock Sensor (KS)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-BU | 496 | Knock Sensor Signal
B | GY | 1716 | Knock Sensor Signal

### Manifold Absolute Pressure (MAP) Sensor

#### Connector Part Information

- OEM: 12129946
- Service: 88987997
- Description: 3-Way F Metri-Pack 150 Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Manifold Absolute Pressure (MAP) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG/BK | 469 | Low Reference
B | L-GN | 432 | MAP Sensor Signal
C | GY | 2704 | 5-Volt Reference 1

### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

#### Connector Part Information

- OEM: 15326822
- Service: 88987186
- Description: 5-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YE | 492 | MAF Sensor Signal
B | BK/WH | 451 | Ground
C | PK/BK | 5291 | Ignition 1 Voltage
D | TN/BK | 2760 | Low Reference
E | TN | 472 | IAT Sensor Signal

### Throttle Actuator Control (TAC) Module

#### Connector Part Information

- OEM: 15326836
- Service: 88986255
- Description: 8-Way F Global Terminal 150 Series Sealed (BK)

#### Terminal Part Information

- Pins: A-H
- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A-D, G, H: E/A
- Core/Insulation Crimp: Pins E, F: 2/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Throttle Actuator Control (TAC) Module

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | D-GN | 485 | TP Sensor 1 Signal
B | TN/WH | 1704 | Low Reference
C | GY | 2701 | 5-Volt Reference - 2
D | PU | 486 | TP Sensor 2 Signal
E | BN | 582 | TAC Motor Control - 2
F | YE | 581 | TAC Motor Control - 1
G | TN | 2752 | Low Reference
H | L-BU/BK | 1688 | 5-Volt Reference - 2