For 1990-2009 cars

## High Mount Stop Lamp Bulb Replacement Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement.

1 | High Mount Stop Lamp Bulb Connector Tip Disengage the two outer tabs on the high mount stop lamp assembly from the bulb connector and remove the connector.
2 | High Mount Stop Lamp Bulb (Qty: 3)

## High Mount Stop Lamp Bulb Replacement Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear compartment lid inner panel trim. Refer to Rear Compartment Lid Inner Panel Trim Replacement .

1 | High Mount Stop Lamp Bulb Connector Tip Pinch the four tabs on the high mount stop lamp bulb connector and remove the connector from the high mount stop lamp.
2 | High Mount Stop Lamp Bulb (Qty: 3)