For 1990-2009 cars

## Headlamp Bulb Replacement w/DRL

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove either the LF or RF headlamp assembly. Refer to Headlamp Replacement .

1 | Headlamp Bulb Locking Ring Tip Turn the ring counterclockwise and remove.
2 | Headlamp Bulb Caution: Refer to Halogen Bulb Caution in the Preface section.
3 | Park and Turn Signal Lamp Socket DRL
4 | Park and Turn Signal Bulb DRL Tip Pull the bulb straight from the socket in order to remove.