For 1990-2009 cars

Callout | Component Name
--- | ---
Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

Remove the head restraint. Refer to Front Seat Head Restraint Replacement .

1 | Guide, Seat Shoulder Belt Tip Cut the retainers that secure the should belt guide to the head restraint to remove and install new retainers to reinstall.