For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Backup Lamp Nut | 4.5 N·m | 40 lb in
Backup Lamp Screw | 1.5 N·m | 13 lb in
Brake Pedal Position Sensor Bolt | 2 N·m | 18 lb in
Front Fog Lamp Screw | 2 N·m | 18 lb in
Front Headlamp Assembly Bolt | 10 N·m | 89 lb in
Front Headlamp Bracket Bolt | 9 N·m | 80 lb in
High Mounted Stop Lamp Nut | 4.5 N·m | 40 lb in
Instrument Panel Cluster Trim Plate Bolt | 10 N·m | 89 lb in
Instrument Panel Cluster Trim Plate Screw | 2.2 N·m | 19 lb in
License Plate Lamp Screw | 2.5 N·m | 22 lb in
Rear Side Marker Lamp Screw | 2.5 N·m | 22 lb in
Tail Lamp Nut-Chevrolet Export | 4.5 N·m | 40 lb in
Tail Lamp Screw-Chevrolet Export, G5 | 1.5 N·m | 13 lb in
Tail Lamp Nut-Chevrolet Coupe | 10 N·m | 89 lb in
Tail/Turn Signal Lamp Nut | 5 N·m | 44 lb in