For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the armrest if equipped. Refer to Front Floor Console Armrest Replacement.
2. Remove the console rear trim plate. Refer to Console Rear Trim Plate Replacement.
3. Remove the console front trim plate. Refer to Console Front Trim Plate Replacement.
4. Remove the rear cup holder. Refer to Front Floor Console Rear Cup Holder Replacement.
5. Remove the console extensions. Refer to Front Floor Console Extension Replacement - Side.

1 | Console Mounting Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 2 N·m (18 lb in)
2 | Center Floor Console Assembly Tip Disconnect the electrical connector.