For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the right console extension panel. Refer to Front Floor Console Extension Replacement - Side .

1 | Body Control Module Assembly Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Body Control Module Assembly Tip Reprogram the body control module (BCM) after replacement. Refer to Control Module References for programming and setup information.