For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

Remove the rear window shelf trim panel. Refer to Rear Window Shelf Trim Panel Replacement .

1 | Bolt, Child Tether Anchor (Qty: 3) Tighten 25 N·m (18 lb ft)
2 | Anchor Assembly, Child Tether