For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .
1 | Filler, Instrument Panel Steering Column Opening Refer to Steering Column Opening Filler Replacement .
2 | Plate, Instrument Panel Trim
3 | Plate, Instrument Panel Trim
4 | Retainer, Instrument Panel Cluster Trim Plate
5 | Bolt, Instrument Panel Cluster Trim Plate Tighten 10 N·m (89 lb in)
6 | Screw, Instrument Panel Cluster Trim Plate Tighten 2.2 N·m (19 lb in)
7 | Plate, Instrument Panel Cluster Trim
8 | Switch, Hazard Warning Tip Disconnect the electrical connector.