For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the armrest if equipped. Refer to Front Floor Console Armrest Replacement .
2. Remove the console rear trim plate. Refer to Console Rear Trim Plate Replacement .
3. Remove the console front trim plate. Refer to Console Front Trim Plate Replacement .
4. Remove the rear cup holder. Refer to Front Floor Console Rear Cup Holder Replacement .
5. Remove the console extensions. Refer to Front Floor Console Extension Replacement - Side .

1 | Console Mounting Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Center Floor Console Assembly Tip Disconnect the electrical connector.