For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Fender Bolts | 10 N·m | 89 lb in
Front Side Door Check Link Bolts | 20 N·m | 15 lb ft
Front Side Door Lower Hinge Bolts | 35 N·m | 26 lb ft
Front Side Door Upper Hinge Bolts | 35 N·m | 26 lb ft
Fuel Filler Pocket Screws | 2 N·m | 18 lb in
Hood Hinge Bolts | 10 N·m | 89 lb in
Hood Latch Bolts | 10 N·m | 89 lb in
Rear Compartment Lid Latch Bolts | 10 N·m | 89 lb in
Rear Compartment Lid Hinge Bolts | 10 N·m | 89 lb in
Rear Compartment Lid Hinge Nuts | 10 N·m | 89 lb in
Rear Side Door Check Link Bolts | 20 N·m | 15 lb ft
Rear Side Door Lower Hinge Bolts | 35 N·m | 26 lb ft
Rear Side Door Upper Hinge Bolts | 35 N·m | 26 lb ft