For 1990-2009 cars

Figure 1: |

#### I/P Components

(1) | Instrument Panel Cluster (IPC)
(2) | Ambient Light Sensor
(3) | Hazard Switch
(4) | Radio
(5) | Remote Control Door Lock Receiver (RCDLR) (AUO)
(6) | Heated Seat Switch - Passenger (KA1)
(7) | HVAC Control Module
(8) | Body Control Module (BCM)
(9) | Heated Seat Switch - Driver (KA1)
(10) | I/P Dimmer Switch
(11) | Fog Lamp Switch (T37)
(12) | Data Link Connector (DLC)
(13) | Rear Compartment Lid Release Switch
(14) | I/P Trim

Figure 2: |

#### Front of the Engine (L61)

(1) | Throttle Actuator Control (TAC) Module
(2) | Ignition Control Module (ICM)
(3) | Evaporative Emission (EVAP) Canister Purge Solenoid
(4) | Engine Oil Pressure (EOP) Switch
(5) | Crankshaft Position (CKP) Sensor
(6) | Knock Sensor (KS)
(7) | Starter
(8) | Starter Solenoid

Figure 3: |

#### Front of the Engine (LE5)

(1) | Fuel Injector 1
(2) | Fuel Injector 2
(3) | Fuel Injector 3
(4) | Manifold Absolute Pressure (MAP) Sensor
(5) | Fuel Injector 4
(6) | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
(7) | Camshaft Position (CMP) Sensor - Intake
(8) | Knock Sensor (KS)
(9) | Engine Oil Pressure (EOP) Switch
(10) | Crankshaft Position (CKP) Sensor
(11) | Starter Solenoid
(12) | Starter
(13) | Intake Manifold

Figure 4: |

#### Lower Front of the Engine (LSJ)

(1) | Starter Solenoid
(2) | Oil Pressure Switch
(3) | C102
(4) | Crankshaft Position (CKP) Sensor
(5) | Starter

Figure 5: |

#### Fuel Tank Components

(1) | Evaporative Emission (EVAP) Canister Vent Solenoid
(2) | Evaporative Emission (EVAP) Canister
(3) | Fuel Tank
(4) | Fuel Pump and Sender Assembly
(5) | C305
(6) | Fuel Filter
(7) | Fuel Tank Pressure (FTP) Sensor

Figure 6: |

#### Ambient Air Temperature Sensor

(1) | Headlamp - Left
(2) | Ambient Air Temperature Sensor
(3) | Headlamp Bracket

Figure 7: |

#### Supercharger Boost Gage (LSJ)

(1) | A-Pillar Trim
(2) | Supercharger Boost Gage (LSJ)