ISC ADJUSTMENTS REVISION INFORMATION. Pontiac J2000 1982

For 1990-2009 cars

# ISC ADJUSTMENTS REVISION INFORMATION

THIS INFORMATION IS BEING RELEASED TO CORRECT THE ISC ADJUSTMENT IN THE 1982 SKYHAWK CHASSIS AND BODY SERVICE MANUAL. STEP 12 ON PAGE 6C1-6, SECOND PARAGRAPH SHOULD READ LIKE THE FOLLOWING: THIS ADJUSTMENT MUST BE MADE WITHIN 50 SECONDS. AFTER 50 SECONDS, THE RPM WILL INCREASE AND CORRECT ADJUSTMENT CANNOT BE MADE. PLEASE MAKE THIS CORRECTION TO YOUR 1982 SKYHAWK CHASSIS AND BODY SERVICE MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.