IDLE SPEED CONTROL ADJUST CORRECTION-ROUGH IDLE. Pontiac J2000 1982

For 1990-2009 cars

# IDLE SPEED CONTROL ADJUST CORRECTION-ROUGH IDLE

THE IDLE SPEED CONTROL ADJUSTMENT PROCEDURES SHOWN ON PAGE 6C1-11 HAVE BEEN REVISED. WHEN ADJUSTING THE IDLE SPEED CONTROL PLUNGER, DO NOT PLACE THE AUTOMATIC TRANSMISSION IN "DRIVE" AS INDICATED IN STEP 12. PLEASE MAKE NOTE OF THIS IN YOUR SHOP MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.