REAR CONTROL ARM BUSHING TOOL NUMBER REVISION. Pontiac LeMans 1980

For 1990-2009 cars

# REAR CONTROL ARM BUSHING TOOL NUMBER REVISION

1980-84 PHOENIX & 6000

When removing or installing a control arm bushing on a 1980-84 Phoenix or 6000 use tool no. J-9519-23 in place of J-9519-10.

Please update page 3D-5 of your 1984 6000/Phoenix service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.