SERVICE MANUAL UPDATE SEC 8A REAR DEFOGGER GROUND LOCATION. Pontiac LeMans 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE SEC 8A REAR DEFOGGER GROUND LOCATION

#### SUBJECT: SERVICE MANUAL UPDATE, SECTION 8A REAR DEFOGGER GROUND (G402) LOCATION (RPO C49)

#### VEHICLES AFFECTED: 1992-93 "T" MODELS

APPLICATION: 1992 Pontiac LeMANS Sedan and Hatchback Models 1993 Asuna Sunfire

This service bulletin amends the rear defogger ground location for G402 on page 8A-200-2 in the 1992 Pontiac LeMANS Service Manual (ST-9210-T) and page 8A-200-3 in the 1993 Pontiac LeMANS and 1993 Asuna Sunfire Service Manual (ST-9310-T). This service bulletin should be used when checking the integrity of the ground.

G402 is located in the following places for all model years:

Hatchback Models: RH side of hatchback door behind trim panel.

Sedan Models: RH side of luggage compartment behind carpet on inner quarter panel.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.