THM 2004R CONVERT. CLUTCH STOP VALVE- NEW DESIGN CLUTCH. Pontiac LeMans 1981

For 1990-2009 cars

# THM 2004R CONVERT. CLUTCH STOP VALVE- NEW DESIGN CLUTCH

SOME FIELD REPORTS HAVE INDICATED IT IS POSSIBLE FOR THE PAST DESIGN CONVERTER CLUTCH STOP VALVE TO MOVE OFF LOCATION. IF THE CONVERTER CLUTCH STOP VALVE BECOMES MISLOCATED, THE CONVERTER CLUTCH WILL EITHER REMAIN APPLIED AT ALL TIMES OR FAIL TO APPLY. TO CORRECT EITHER CONDITION, INSTALL THE NEW DESIGN CONVERTER CLUTCH STOP VALVE. SEE FIGURE 1. THE NEW DESIGN CONVERTER CLUTCH STOP VALVE CAN BE ORDERED USING PART NUMBER 8634705, AND SHOULD BE USED AS A REPLACEMENT PART FOR ALL THM 200-4R TRANSMISSIONS. ANY THM 200-4R TRANSMISSION BUILT AFTER JANUARY 8, 1981, WILL CONTAIN THE NEW DESIGN CONVERTER CLUTCH STOP VALVE.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.