SLIP OR LOSS OF DRIVE AND/OR BURNT FORWARD & OVERUN CLUTCH. Pontiac Safari Wagon 1987

For 1990-2009 cars

# SLIP OR LOSS OF DRIVE AND/OR BURNT FORWARD & OVERUN CLUTCH

VEHICLE APPLICATIONS: F,Y AND B CARS, G AND M VANS C,K,R,V,S AND T TRUCKS

BULLETIN COVERS: (Figure 2)

A new auxiliary accumulator valve body (377) and a new cover (371) went into production to prevent the accumulator piston pin from working its way out of the auxiliary valve body. If the accumulator piston pin comes out of either end of the auxiliary valve body the following conditions could occur:

1. Loss of DRIVE 2. Slipping in DRIVE 3. Burned forward and overrun clutches

DATE OF PRODUCTION CHANGE: (Figure 1)

Beginning January 27, 1987 (Julian Date 027) all THM 700-R4 transmissions were produced with an auxiliary, accumulator valve body assembly (Figure 2) that has a stepped bore at bne end of the piston pin and a new cover with an oval instead of a round exhaust hole at the"Other end of the pin to retain the accumulator piston pin in place.

#### SERVICE ACTION:

The new auxiliary accumulator valve body (377) and cover (371) can be used on any 1987 THM 700-R4 transmission that has an auxiliary valve body (377).

#### NOTICE: If the accumulator piston pin has come out of the auxiliary valve body, check for burnt forward and overrun clutches.

SERVICE PARTS INFORMATION:

PART NUMBER DESCRIPTION MODELS AFFECTED ----------- ----------- --------------- 8663597 Auxiliary Accumulator MRM, MXM Valve Body Assembly FAM, MAM, MFM, MMM

8667036 Auxiliary Accumulator MCM, MTM, PRM, TAM, TBM, Valve Body Assembly YXM, PCM, TJM, TKM, TNM TRM, TUM, TXM 8667037 Auxiliary Accumulator MDM, MHM, MLM, MKM, MPM, Valve Body Assembly MUM, MWM, MZM 8667038 Auxiliary Accumulator TSM, YAM, YDM, YFM, YKM, Valve Body Assembly YLM, YMM, YNM, YPM, YSM, TYM, YZM

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.