REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION. Pontiac Sunbird 1985

For 1990-2009 cars

# REVISED FRONT WHEEL TOE SPECIFICATION MANUAL REVISION

1985 SUNBIRD AND GRAND AM

The front wheel toe Service Setting has been revised to -.06 degrees per wheel on 1985 Sunbird and Grand Am models. Please make this correction on page 3A-3 of the 1985 Sunbird and Grand Am Manuals.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.