FRONT BRAKE DISC LINING CHANGE NON-CHAMFERED PADS. Pontiac Sunbird 1984

For 1990-2009 cars

# FRONT BRAKE DISC LINING CHANGE NON-CHAMFERED PADS

1982-85 SUNBIRD

Front disc brake noise can be reduced on some 1982-84 and early 1985 "J" cars by the installation of non-chamfered front disc brake pads. These non-chamfered front disc pads are currently being used on 1985 production vehicles beginning with the following VIN's.

Without With Pontiac Aluminum Wheels Aluminum Wheels ------- --------------- ---------------- Lordstown 1G2JB6906F7510359 1G2JB3504F7512583

Use appropriate shop manual procedures for pad replacement.

Warranty Information

Use applicable labor operation number and labor time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.