REAR CAM COVER OIL LEAK IMPROVED SEAL AND COVER. Pontiac Sunbird 1984

For 1990-2009 cars

# REAR CAM COVER OIL LEAK IMPROVED SEAL AND COVER

1982-84 J 2000 AND SUNBIRD MODELS WITH 2.0L L4 ENGINES (L46 VIN CODE G, LQ5 VIN CODE P)

An improved seal for the rear cam cover, kit P/N 10054590, is available to replace the RTV sealant and cover plate. The surface should be thoroughly cleaned and checked for flush plugs in the sealing area before installing the new cover, P/N 14090972, and gasket, P/N 14090974.

Torque bolts to 8-14Nm (6-10 Lb. Ft. ).

Use existing labor operation number and labor time.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.